{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Parameter->PN","PN->Parameter","Disclaimer","All Data","Cross PN"],"not_rendered":{"charts":0,"images":23,"macros":1,"external_links":1,"defined_names":26,"comments":4,"pivot_tables":1},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Parameter->PN","index":0,"n_rows":4777,"n_cols":158,"rows_kept":1125,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
["Panasonic Polymer and Electrolytic Capacitor Quick Search",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"COUNTA(BF:BF)-1","v":4772}]
["Please select parameters below to find the capacitors to match your requirements."]
["Filters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Output"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Type","Voltage (V)","Cap. (uF)","ESR or Z (mOhm)","ESR or Z Freq.","Ripple Current (mArms)","Ripple Temp.","Ripple Freq.","ref \nESL \n(nH)","Size \n(mm)","Height (mm)","Max Height (mm)","Terminals","Temp Range (deg.C)","Endurance","MPQ (pcs)","Automotive Grade","Status","Product","Part Number","Remarks",null,null,"URL"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF6,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF6,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D181ER"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|","SMD",2,180,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D181ER"," ",{"$f":"IFERROR(_xlfn.IMAGE(H6,\"\"),\"\")","v":""},null,{"$f":"IFERROR(HYPERLINK(I6),\"\")","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D181ER"}]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF7,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF7,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLR0D221R4"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,220,4.5,"100kHz",8500,"45°C","100kHz",0.5,"7.3x4.3(D)",1,1,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLR0D221R4"," ",{"$f":"IFERROR(_xlfn.IMAGE(H7,\"\"),\"\")","v":""},null,{"$f":"IFERROR(HYPERLINK(I7),\"\")","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLR0D221R4"}]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF8,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF8,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSR0D221R4"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1,1,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSR0D221R4"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSR0D221R4"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF9,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF9,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLR0D221R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,6,"100kHz",7500,"45°C","100kHz",0.5,"7.3x4.3(D)",1,1,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLR0D221R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLR0D221R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF10,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF10,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLS0D221R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,null,null,null,null,null,null,1.1000000000000001,1.2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLS0D221R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLS0D221R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF11,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF11,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSR0D221R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1,1,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSR0D221R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSR0D221R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF12,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF12,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSS0D221R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,null,null,null,null,null,null,1.1000000000000001,1.2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSS0D221R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSS0D221R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF13,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF13,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D221ER"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D221ER"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D221ER"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF14,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF14,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D221R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,15,"100kHz",5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0D221R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D221R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF15,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF15,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D271E4"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,270,4.5,"100kHz",8500,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D271E4"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D271E4"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF16,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF16,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D271XE"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,6,"100kHz",7500,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D271XE"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D271XE"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF17,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF17,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2TPSF270M6E"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,"500kHz",3200,"45°C","100kHz",0.7,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","2TPSF270M6E"," ","",null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2TPSF270M6E"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF18,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF18,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D271ER"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D271ER"," ",{"$f":"IFERROR(_xlfn.IMAGE(H18,\"\"),\"\")","v":""},null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D271ER"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF19,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF19,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2TPSF270M9G"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,"300kHz",2400,"45°C","100kHz",0.7,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","2TPSF270M9G"," ","",null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2TPSF270M9G"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF20,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF20,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D271XR"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,12,"100kHz",5600,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0D271XR"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D271XR"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF21,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF21,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0D331R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,330,3,"100kHz",10200,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFGX0D331R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0D331R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF22,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF22,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0D331R4"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,4.5,"100kHz",8500,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLX0D331R4"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0D331R4"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF23,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF23,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D331E4"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D331E4"," ","",null,{"$f":"IFERROR(HYPERLINK(I23),\"\")","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D331E4"}]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF24,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF24,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLT0D331R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,6,"100kHz",7500,"45°C","100kHz",0.5,"7.3x4.3(D)",1.4,1.5,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLT0D331R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLT0D331R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF25,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF25,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0D331R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,null,null,null,null,null,null,1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLX0D331R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0D331R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF26,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF26,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFST0D331R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.4,1.5,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFST0D331R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFST0D331R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF27,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF27,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D331XE"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,null,null,null,null,null,null,1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D331XE"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D331XE"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF28,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF28,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D331ER"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D331ER"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D331ER"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF29,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF29,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0D331RE"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(1.6V)",3500,"No","Std","SP-Cap","EEFJX0D331RE","High Rel.","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0D331RE"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF30,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF30,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0D331RE"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(1.6V)",3500,"No","Std","SP-Cap","EEFKX0D331RE","High Rel.","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0D331RE"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF31,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF31,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0D331RE"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(1.6V)",3500,"No","Std","SP-Cap","EEFTX0D331RE","High Rel.","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0D331RE"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF32,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF32,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D331XR"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,12,"100kHz",5600,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0D331XR"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D331XR"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF33,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF33,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D331R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,15,"100kHz",5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0D331R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D331R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF34,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF34,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D391E4"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,390,4.5,"100kHz",8500,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D391E4"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D391E4"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF35,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF35,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D391XE"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,6,"100kHz",7500,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D391XE"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D391XE"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF36,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF36,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D391ER"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D391ER"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D391ER"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF37,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF37,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D391R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"|",null,null,null,15,"100kHz",5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0D391R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D391R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF38,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF38,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0D471L"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,470,3,"100kHz",10200,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFGX0D471L"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0D471L"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF39,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF39,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0D471R"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFGX0D471R"," ","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0D471R"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF40,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF40,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0D471RB"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(1.6V)",3500,"No","Std","SP-Cap","EEFJX0D471RB","High Rel.","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0D471RB"]
[null,null,null,null,null,null,null,{"$f":"INDEX('All Data'!AY:AY,MATCH('Parameter->PN'!BF41,'All Data'!R:R,))","v":"https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg"},{"$f":"INDEX('All Data'!AX:AX,MATCH('Parameter->PN'!BF41,'All Data'!R:R,0))","v":"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0D471RB"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(1.6V)",3500,"No","Std","SP-Cap","EEFKX0D471RB","High Rel.","",null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0D471RB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(1.6V)",3500,"No","Std","SP-Cap","EEFTX0D471RB","High Rel."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.5,"100kHz",8500,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLX0D471R4"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D471E4"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(1.6V)",3500,"No","Std","SP-Cap","EEFHX0D471R4"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 3000H(1.6V)",3500,"No","Std","SP-Cap","EEFJX0D471RC","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(1.6V)",3500,"No","Std","SP-Cap","EEFKX0D471RC","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(1.6V)",3500,"No","Std","SP-Cap","EEFTX0D471RC","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"100kHz",7500,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLX0D471R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D471XE"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(1.6V)",3500,"No","Std","SP-Cap","EEFHX0D471R6"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D471ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(1.6V)",3500,"No","Std","SP-Cap","EEFHX0D471R9"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 3000H(1.6V)",3500,"No","Std","SP-Cap","EEFJX0D471RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(1.6V)",3500,"No","Std","SP-Cap","EEFKX0D471RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(1.6V)",3500,"No","Std","SP-Cap","EEFTX0D471RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,"300kHz",2300,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","2TPE470MAJGB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",2300,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","2TPE470MAFB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0D471R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(1.6V)",3500,"No","Std","SP-Cap","EEFHX0D471R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,560,3,"100kHz",10200,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFGX0D561L"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFGX0D561R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2000000000000002,2.2999999999999998,2,"-55 to 125","125°C 3000H(1.6V)",3000,"No","Std","SP-Cap","EEFJZ0D561RB","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(1.6V)",3000,"No","Std","SP-Cap","EEFKZ0D561RB","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(1.6V)",3000,"No","Std","SP-Cap","EEFTZ0D561RB","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.5,"100kHz",8500,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLX0D561R4"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0D561E4"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2000000000000002,2.2999999999999998,2,"-55 to 125","125°C 3000H(1.6V)",3000,"No","Std","SP-Cap","EEFJZ0D561RC","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(1.6V)",3000,"No","Std","SP-Cap","EEFKZ0D561RC","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(1.6V)",3000,"No","Std","SP-Cap","EEFTZ0D561RC","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"100kHz",7500,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLX0D561R"," ",null,null,{"$f":"IFERROR(HYPERLINK(I71),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",2.2000000000000002,2.2999999999999998,2,"-55 to 125","125°C 3000H(1.6V)",3000,"No","Std","SP-Cap","EEFJZ0D561RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(1.6V)",3000,"No","Std","SP-Cap","EEFKZ0D561RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(1.6V)",3000,"No","Std","SP-Cap","EEFTZ0D561RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0D561R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,820,3,"100kHz",10200,"45°C","100kHz",1.2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2000,"No","Std","SP-Cap","EEFGY0D821R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1200,8,"100kHz",5230,"105°C","(空白)",2.6,"dia. 6.3",9.9,10,2,"-55 to 105","105°C 2000H",500,"No","Std","OS-CON","2SVPE1200M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.5,82,30,"100kHz",1970,"105°C","(空白)",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","NRND","OS-CON","2R5SVPA82MAA","→6SVP82M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,40,"100kHz",1670,"105°C","(空白)",2.4,"dia. 6.3",4.9000000000000004,5,2,"-55 to 105","105°C 1000H",1300,"No","NRND","OS-CON","2R5SVPB120M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E151ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,180,4.5,"100kHz",8500,"45°C","100kHz",0.5,"7.3x4.3(D)",1,1,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLR0E181R4"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1,1,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSR0E181R4"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"100kHz",7500,"45°C","100kHz",0.5,"7.3x4.3(D)",1,1,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLR0E181R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1000000000000001,1.2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLS0E181R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1,1,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSR0E181R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1000000000000001,1.2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSS0E181R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E181ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,"100kHz",2800,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","2R5SVPC180MV"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"100kHz",2690,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","NRND","OS-CON","2R5SVPA180MAA","→2R5SVPC390M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,"100kHz",2200,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","2R5SVPC180MY"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1970,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","2R5SVPC180M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,220,7,"100kHz",7000,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E221E7"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"100kHz",3900,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE220M9"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","2R5TAE220M9"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E221ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(2V)",3500,"No","Std","SP-Cap","EEFJX0E221RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFKX0E221RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFTX0E221RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",2000,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","2R5TPE220MAFB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3100,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE220MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","2R5TAE220MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0E221R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"300kHz",1800,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","2R5TPE220MFGB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2800,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE220MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,"100kHz",1700,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","2R5TPE220MLB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,"100kHz",2390,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","2R5SVP220M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",1600,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","2R5TPE220MAPB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2400,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","NRND","POSCAP","2R5TPE220M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","2R5TAE220M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1400,"45°C","100kHz",1.1000000000000001,"3.5x2.8(B)",1.1000000000000001,1.2,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","ETPS220MUD"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","2R5TPE220MUB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"100kHz",1400,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","2R5TPE220MAZB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 1000H",2000,"No","Std","POSCAP","2R5TPE220MZB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,45,"100kHz",1700,"45°C","100kHz",2,"7.3x4.3(D)",1.9,2,2,"-55 to 125","125°C 1000H(1.6V)",3000,"No","NRND","POSCAP","2R5THC220M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,270,6,"100kHz",7500,"45°C","100kHz",0.5,"7.3x4.3(D)",1.4,1.5,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLT0E271R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.4,1.5,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFST0E271R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"500kHz",3200,"45°C","100kHz",0.7,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","ETPSF270M6E"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"100kHz",7000,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E271E7"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"100kHz",3860,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","2R5SVPE270M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,330,3,"100kHz",10200,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFGX0E331R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.5,"100kHz",8500,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLX0E331R4"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E331E4"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",3500,"No","Std","SP-Cap","EEFHX0E331R4"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"100kHz",7500,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLX0E331R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E331XE"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",3500,"No","Std","SP-Cap","EEFHX0E331R6"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"100kHz",4400,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE330M7"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"100kHz",3200,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","ETPE330M9GB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3900,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE330M9"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E331ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",3500,"No","Std","SP-Cap","EEFHX0E331R9"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 3000H(2V)",3500,"No","Std","SP-Cap","EEFJX0E331RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFKX0E331RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFTX0E331RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"300kHz",3200,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","ETPE330MA9GB"," ",null,null,{"$f":"IFERROR(HYPERLINK(I135),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2999999999999998,"3.5x2.8(B)",1.9,2,2,"-55 to 125","125°C 1000H(2V)",2000,"No","Std","POSCAP","ETCE330M9GB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"100kHz",3860,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","2R5SVPE330MY"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"100kHz",3500,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE330MC"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",2700,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","ETPE330MFB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3100,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE330MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","2R5TAE330MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(1.6V)",3000,"No","NRND","POSCAP","2R5THE330MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3150,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","2R5SVPE330M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0E331R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",3500,"No","Std","SP-Cap","EEFHX0E331R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2450,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","ETPE330MIB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2800,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE330MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","2R5TAE330MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(1.6V)",3000,"No","NRND","POSCAP","2R5THE330MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"100kHz",3370,"105°C","100kHz",4.3,"dia. 8",6.9,7,2,"-55 to 105","105°C 2000H",1000,"No","NRND","OS-CON","2R5SVPA330MAA","→2R5SVPC390M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",2400,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","NRND","POSCAP","2R5TPE330M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","2R5TAE330M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(1.6V)",3000,"No","NRND","POSCAP","2R5THE330M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1400,"45°C","100kHz",1.1000000000000001,"3.5x2.8(B)",1.1000000000000001,1.2,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","ETPS330MUD"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"100kHz",1400,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","2R5TPE330MAZB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,390,3,"100kHz",10200,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 125","125°C 3000H(2V)",3500,"No","Std","SP-Cap","EEFJX0E391RB","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFKX0E391RB","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFTX0E391RB","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.5,"100kHz",8500,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E391E4"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(2V)",3500,"No","Std","SP-Cap","EEFJX0E391RC","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFKX0E391RC","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFTX0E391RC","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"100kHz",7500,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E391XE"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E391ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(2V)",3500,"No","Std","SP-Cap","EEFJX0E391RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFKX0E391RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFTX0E391RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"100kHz",3860,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","2R5SVPE390MX"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3900,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","2R5SVPE390M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3160,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","2R5SVPC390MV"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0E391R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",2410,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","2R5SVPC390M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,470,3,"100kHz",10200,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFGX0E471L"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFGX0E471R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(2V)",3500,"No","Std","SP-Cap","EEFJX0E471RB","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFKX0E471RB","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.5,"100kHz",8500,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLX0E471R4"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E471E4"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(2V)",3500,"No","Std","SP-Cap","EEFJX0E471RC","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFKX0E471RC","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"100kHz",4400,"45°C","100kHz",2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","2R5TPF470M6L"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7500,"45°C","100kHz",0.5,"7.3x4.3(D)",1.9,2,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLX0E471R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E471XE"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"100kHz",4400,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE470M7"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","2R5TPF470M7L"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"100kHz",3900,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE470M9"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0E471ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(2V)",3500,"No","Std","SP-Cap","EEFJX0E471RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(2V)",3500,"No","Std","SP-Cap","EEFKX0E471RE","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3850,"45°C","100kHz",2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","2R5TPF470M9L"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"100kHz",4400,"45°C","100kHz",2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","2R5TPF470ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"100kHz",3500,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE470MC"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3100,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE470MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","2R5TAE470MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0E471R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2800,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","2R5TPE470MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",2400,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"Yes","Std","POSCAP","2R5TAE470M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,560,16,"100kHz",3500,"105°C","100kHz",2.5,"dia. 6.3",6.4,6.5,2,"-55 to 105","105°C20000H",1000,"No","Std","OS-CON","2R5SVPT560M","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 2000H",1000,"No","Std","OS-CON","2R5SVT560M"," ",null,null,{"$f":"IFERROR(HYPERLINK(I199),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","2R5SVPC560M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,680,3,"100kHz",10200,"45°C","100kHz",1.2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2000,"No","Std","SP-Cap","EEFGY0E681R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"100kHz",6100,"45°C","100kHz",2.5,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","NRND","POSCAP","ETPF680M5H"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",2000,"No","NRND","POSCAP","ETCF680M5H"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"100kHz",4400,"45°C","100kHz",2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","2R5TPF680M6L"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",2500,"No","Std","POSCAP","ETCF680M6L"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"100kHz",4400,"45°C","100kHz",2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","2R5TPF680M7L"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",2500,"No","Std","POSCAP","ETCF680M7L"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"100kHz",4400,"45°C","100kHz",2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","2R5TPF680ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",2500,"No","Std","POSCAP","ETCF680ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"100kHz",3500,"45°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","2R5TPE680MCL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",2500,"No","Std","POSCAP","ETCE680MCL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,"100kHz",4520,"105°C","100kHz",4.4000000000000004,"dia. 8",11.9,12,2,"-55 to 105","105°C 2000H",400,"No","Std","OS-CON","2R5SVP680M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3100,"45°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","2R5TPE680MFL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","2R5TAE680MFL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",2500,"No","Std","POSCAP","ETCE680MFL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,"100kHz",3500,"105°C","100kHz",2.5,"dia. 6.3",6.4,6.5,2,"-55 to 105","105°C20000H",1000,"No","Std","OS-CON","2R5SVPT680MX","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 2000H",1000,"No","Std","OS-CON","2R5SVT680MX"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"100kHz",3370,"105°C","100kHz",4.3,"dia. 8",6.9,7,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","2R5SVPC680M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",1000,"No","Std","OS-CON","2R5SVPT680M","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 2000H",1000,"No","Std","OS-CON","2R5SVT680M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",2400,"45°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"Yes","Std","POSCAP","2R5TAE680ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2700,"45°C","100kHz",2.5,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","Std","POSCAP","ETPF680MPH"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"100kHz",1850,"45°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","2R5TPE680MWL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,820,9,"100kHz",5380,"105°C","100kHz",4.4000000000000004,"dia. 8",11.9,12,2,"-55 to 105","105°C 2000H",400,"No","Std","OS-CON","2R5SVPC820M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"100kHz",3900,"105°C","100kHz",2.5,"dia. 6.3",6.4,6.5,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","2R5SVPE820M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,"100kHz",3500,"105°C","100kHz",2.5,"dia. 6.3",6.4,6.5,2,"-55 to 105","105°C20000H",1000,"No","Std","OS-CON","2R5SVPT820M","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 2000H",1000,"No","Std","OS-CON","2R5SVT820M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,"100kHz",4240,"105°C","100kHz",5.2,"dia.10",7.9,8,2,"-55 to 105","105°C 2000H",500,"No","Std","OS-CON","2R5SVPA820M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,5,"100kHz",6100,"45°C","100kHz",2.5,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","Std","POSCAP","ETPF1000M5H"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",2000,"No","Std","POSCAP","ETCF1000M5H"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"100kHz",5600,"45°C","100kHz",2.5,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","Std","POSCAP","ETPF1000M6H"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",2000,"No","Std","POSCAP","ETCF1000M6H"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3900,"45°C","100kHz",2.6,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","Std","POSCAP","2R5TPE1000MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2V)",2000,"No","Std","POSCAP","ETCE1000MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,10,"100kHz",5150,"105°C","100kHz",4.4000000000000004,"dia. 8",11.9,12,2,"-55 to 105","105°C 2000H",400,"No","Std","OS-CON","2R5SVPC1500M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",400,"No","Std","OS-CON","2R5SVPT1500M","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 2000H",400,"No","Std","OS-CON","2R5SVT1500M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"100kHz",4400,"45°C","100kHz",2.6,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","Std","POSCAP","2R5TPE1500MC"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5440,"105°C","100kHz",5,"dia.10",12.6,12.7,2,"-55 to 105","105°C 2000H",400,"No","Std","OS-CON","2R5SVP1500M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3900,"45°C","100kHz",2.6,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","Std","POSCAP","2R5TPE1500MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2700,12,"100kHz",5070,"105°C","100kHz",5,"dia.10",12.6,12.7,2,"-55 to 105","105°C 2000H",400,"No","Std","OS-CON","2R5SVPC2700M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",400,"No","Std","OS-CON","2R5SVPT2700M","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 2000H",400,"No","Std","OS-CON","2R5SVT2700M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,33,200,"100kHz",740,"105°C","100kHz",2,"dia. 4",5.4,5.5,2,"-55 to 105","105°C 2000H",2000,"No","NRND","OS-CON","4SVP33M","→10SVP33M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",2000,"No","NRND","OS-CON","4SVPS33M","→10SVP33M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",26," 85°C","120Hz","(空白)","dia. 4",5.4,5.5,2,"-40 to  85"," 85°C 1000H",2000,"Yes","NRND","E-Cap","EEE0GA330SR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,39,70,"100kHz",1100,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","NRND","OS-CON","4SVP39M","→16SVP39M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47,"N/A","100kHz",34,"105°C","120Hz","(空白)","dia. 4",5.8,6.1,2,"-40 to 105","105°C 2000H",2000,"Yes","NRND","E-Cap","EEEHB0G470R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 4",5.4,5.5,2,"-40 to  85"," 85°C 1000H",2000,"Yes","NRND","E-Cap","EEE0GA470SR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,30,"100kHz",1970,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","NRND","OS-CON","4SVPA68MAA","→4SVP68M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",1500,"No","NRND","OS-CON","4SVPS68M","→4SVP68M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60,"100kHz",1400,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","4SVP68M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,"100kHz",1100,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","4TPB68M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,82,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0G820ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0G101ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"100kHz",1400,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","4TPE100MZB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"100kHz",1300,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","4TPE100MWB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1670,"105°C","100kHz",2.4,"dia. 6.3",4.9000000000000004,5,2,"-55 to 105","105°C 1000H",1300,"No","NRND","OS-CON","4SVPB100M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,"100kHz",1100,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"Yes","Std","POSCAP","4TAB100M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,950,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","4TPE100MBB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",61,"105°C","120Hz","(空白)","dia. 5",5.8,6.1,2,"-40 to 105","105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHB0G101R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 5",5.4,5.5,2,"-40 to  85"," 85°C 1000H",1000,"Yes","NRND","E-Cap","EEE0GA101SR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,9,"100kHz",6300,"45°C","100kHz",0.5,"7.3x4.3(D)",1,1,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLR0G121R"," ",null,null,{"$f":"IFERROR(HYPERLINK(I263),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1,1,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSR0G121R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.1000000000000001,1.2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCS0G121R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,7,"100kHz",7000,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0G151E7"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0G151ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0G151R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(3.2V)",3500,"No","Std","SP-Cap","EEFJX0G151RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(3.2V)",3500,"No","Std","SP-Cap","EEFKX0G151RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(3.2V)",3500,"No","Std","SP-Cap","EEFTX0G151RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2800,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","4TPE150MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(3.2V)",3000,"No","Std","POSCAP","4TCE150MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"100kHz",2730,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","4SVPC150MV"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"100kHz",2570,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","NRND","OS-CON","4SVPA150MAA","→16SVPC150M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",1000,"No","Std","OS-CON","4SVPS150M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,"100kHz",2240,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","4SVPC150MY"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1970,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","4SVPC150M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"100kHz",1400,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","4TPE150MAZB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"100kHz",1810,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","4SVP150MX"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",1000,"No","Std","OS-CON","4SVQP150M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",82,"105°C","120Hz","(空白)","dia. 6.3",5.8,6.1,2,"-40 to 105","105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHB0G151P"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,180,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0G181ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"100kHz",5600,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0G181XR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.4,1.5,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCT0G181R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0G181R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(3.2V)",3500,"No","Std","SP-Cap","EEFJX0G181RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(3.2V)",3500,"No","Std","SP-Cap","EEFKX0G181RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(3.2V)",3500,"No","Std","SP-Cap","EEFTX0G181RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,220,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0G221ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"100kHz",5600,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0G221XR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3100,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","4TPE220MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2.5V)",3000,"No","NRND","POSCAP","4THE220MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 1000H(3.2V)",3000,"No","Std","POSCAP","4TCE220MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0G221R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(3.2V)",3500,"No","Std","SP-Cap","EEFJX0G221RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(3.2V)",3500,"No","Std","SP-Cap","EEFKX0G221RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(3.2V)",3500,"No","Std","SP-Cap","EEFTX0G221RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2800,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","4TPE220MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","4TAE220MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2.5V)",3000,"No","NRND","POSCAP","4THE220MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 1000H(3.2V)",3000,"No","Std","POSCAP","4TCE220MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",2400,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","4TPE220M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","4TAE220M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(2.5V)",3000,"No","NRND","POSCAP","4THE220M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 1000H(3.2V)",3000,"No","Std","POSCAP","4TCE220M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1400,"45°C","100kHz",1.1000000000000001,"3.5x2.8(B)",1.1000000000000001,1.2,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","4TPS220MUD"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"100kHz",1400,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","4TPE220MAZB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1350,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","NRND","POSCAP","4TPE220MZB","→4TPE220MAZB",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,45,"100kHz",1750,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","4TPE220MV"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1150,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","NRND","POSCAP","4TPE220MVB","→4TPE220MAZB",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,"100kHz",950,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","NRND","POSCAP","4TPE220MBB","→4TPE220MAZB",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",82,"105°C","120Hz","(空白)","dia. 6.3",5.8,6.1,2,"-40 to 105","105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHB0G221P"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 6.3",5.4,5.5,2,"-40 to  85"," 85°C 1000H",1000,"Yes","NRND","E-Cap","EEE0GA221SP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,270,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0G271ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0G271R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"100kHz",3220,"105°C","100kHz",4.3,"dia. 8",6.9,7,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","4SVPA270MAA"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",1000,"No","NRND","OS-CON","4SVPS270M","→10SVPC270M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,330,6,"100kHz",7500,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0G331XE"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"100kHz",3900,"45°C","100kHz",2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","4TPF330M9L"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0G331ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"100kHz",4000,"45°C","100kHz",2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","4TPF330ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(3.2V)",2500,"No","Std","POSCAP","4TCF330ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3160,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","4SVPC330MV"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0G331R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3550,"45°C","100kHz",2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","4TPF330MFL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2800,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","4TPE330MI"," ",null,null,{"$f":"IFERROR(HYPERLINK(I327),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(3.2V)",3000,"No","Std","POSCAP","4TCE330MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,"100kHz",2630,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","4SVPC330MY"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",2400,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","4TPE330M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(3.2V)",3000,"No","Std","POSCAP","4TCE330M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,"100kHz",2320,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","4SVPC330M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"100kHz",2560,"105°C","100kHz",4.3,"dia. 8",6.9,7,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","4SVP330M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"100kHz",2000,"45°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 125","125°C 1000H(2.5V)",2500,"No","NRND","POSCAP","4THB330ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1850,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","4TPE330MW"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",80," 85°C","120Hz","(空白)","dia. 6.3",5.4,5.5,2,"-40 to  85"," 85°C 1000H",1000,"Yes","NRND","E-Cap","EEE0GA331WP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,470,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",2.8,3,2,"-55 to  85","_85°C 2000H",2000,"No","Std","SP-Cap","ECGSY0G471R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"100kHz",4400,"45°C","100kHz",2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","4TPF470ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(3.2V)",2500,"No","Std","POSCAP","4TCF470ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"100kHz",3500,"45°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","4TPE470MCL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(3.2V)",2500,"No","Std","POSCAP","4TCE470MCL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3100,"45°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","4TPE470MFL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(3.2V)",2500,"No","Std","POSCAP","4TCE470MFL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5100,"45°C","100kHz",1.2,"7.3x4.3(D)",2.8,3,2,"-55 to  85","_85°C 2000H",2000,"No","Std","SP-Cap","ECGCY0G471R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2800,"45°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","4TPE470MIL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","4TAE470MIL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(3.2V)",2500,"No","Std","POSCAP","4TCE470MIL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",2400,"45°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","4TPE470ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","4TAE470ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(3.2V)",2500,"No","Std","POSCAP","4TCE470ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"100kHz",1850,"45°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","4TPE470MWL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",200," 85°C","120Hz","(空白)","dia. 6.3",7.7,8,2,"-40 to  85"," 85°C 1000H",900,"Yes","NRND","E-Cap","EEE0GA471XP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,560,9,"100kHz",5380,"105°C","100kHz",4.4000000000000004,"dia. 8",11.9,12,2,"-55 to 105","105°C 2000H",400,"No","Std","OS-CON","4SVPC560MX"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,"100kHz",4520,"105°C","100kHz",4.4000000000000004,"dia. 8",11.9,12,2,"-55 to 105","105°C 2000H",400,"No","Std","OS-CON","4SVP560M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"100kHz",3220,"105°C","100kHz",4.3,"dia. 8",6.9,7,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","4SVPC560M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",1000,"No","Std","OS-CON","4SVPT560M","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 2000H",1000,"No","Std","OS-CON","4SVT560M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,680,10,"100kHz",4400,"45°C","100kHz",2.5,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","Std","POSCAP","4TPF680MAH"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(3.2V)",2000,"No","Std","POSCAP","4TCF680MAH"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3550,"45°C","100kHz",2.5,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","Std","POSCAP","4TPF680MFH"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"100kHz",4130,"105°C","100kHz",5.2,"dia.10",7.9,8,2,"-55 to 105","105°C 2000H",500,"No","Std","OS-CON","4SVPA680M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",500,"No","Std","OS-CON","4SVPS680M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",3700,"105°C","100kHz",5.2,"dia.10",7.9,8,2,"-55 to 105","105°C 2000H",500,"No","Std","OS-CON","4SVP680M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"100kHz",2350,"45°C","100kHz",2.5,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","Std","POSCAP","4TPF680MZH"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1200,12,"100kHz",4700,"105°C","100kHz",4.4000000000000004,"dia. 8",11.9,12,2,"-55 to 105","105°C 2000H",400,"No","Std","OS-CON","4SVPC1200M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5440,"105°C","100kHz",5,"dia.10",12.6,12.7,2,"-55 to 105","105°C 2000H",400,"No","Std","OS-CON","4SVP1200M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,12,"100kHz",4700,"105°C","100kHz",4.4000000000000004,"dia. 8",11.9,12,2,"-55 to 105","105°C 2000H",400,"No","Std","OS-CON","4SVPC1500M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",400,"No","Std","OS-CON","4SVPT1500M","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 2000H",400,"No","Std","OS-CON","4SVT1500M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.3,10,1350,"100kHz",90,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFN0J100R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,200,"100kHz",740,"105°C","100kHz",2,"dia. 4",5.4,5.5,2,"-55 to 105","105°C 2000H",2000,"No","NRND","OS-CON","6SVP22M","→6SVP47M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",2000,"No","NRND","OS-CON","6SVPS22M","→6SVP47M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,850,"100kHz",160,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFP0J220AR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1350,"100kHz",90,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFK0J220AR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK0J220R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFN0J220R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3000,"100kHz",60,"105°C","100kHz","(空白)","dia. 4",5.4,5.5,2,"-40 to 105","105°C 1000H",2000,"Yes","NRND","E-Cap","EEEFC0J220AR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFC0J220R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",26,"105°C","120Hz","(空白)","dia. 4",5.4,5.5,2,"-40 to 105","105°C 2000H",2000,"Yes","NRND","E-Cap","EEEHB0J220SR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.8,6.1,2,"-40 to 105","105°C 2000H",2000,"Yes","NRND","E-Cap","EEEHB0J220AR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHB0J220R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 3000H",2000,"Yes","NRND","E-Cap","EEEHC0J220R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,29,"105°C","120Hz","(空白)","dia. 4",5.4,5.5,2,"-40 to 105","105°C 1000H",2000,"Yes","NRND","E-Cap","EEEHA0J220AR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA0J220R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 5",5.4,5.5,2,"-40 to  85"," 85°C 2000H",1000,"Yes","NRND","E-Cap","EEE0JA220NR","Bipolar",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 4",5.4,5.5,2,"-40 to  85"," 85°C 2000H",2000,"Yes","NRND","E-Cap","EEE0JA220AR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE0JA220SR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,33,70,"100kHz",1100,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","6TPB33M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1350,"100kHz",90,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFN0J330R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",22," 85°C","120Hz","(空白)","dia. 4",5.4,5.5,2,"-40 to  85"," 85°C 1000H",2000,"Yes","NRND","E-Cap","EEE0JA330WAR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE0JA330WR"," ",null,null,{"$f":"IFERROR(HYPERLINK(I391),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,29,"105°C","120Hz","(空白)","dia. 4",5.4,5.5,2,"-40 to 105","105°C 1000H",2000,"Yes","NRND","E-Cap","EEEHAJ330WAR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA0J330WR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.8,6.1,2,"-40 to 105","105°C 2000H",2000,"Yes","NRND","E-Cap","EEEHB0J330AR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHB0J330R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47,30,"100kHz",1970,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","6SVPA47MAA"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",1500,"No","Std","OS-CON","6SVPS47M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,"100kHz",1100,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","6SVP47M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"Yes","Std","POSCAP","6TAB47M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,360,"100kHz",240,"105°C","100kHz","(空白)","dia. 5",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFP0J470AR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,700,"100kHz",160,"105°C","100kHz","(空白)","dia. 5",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFK0J470AR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK0J470R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,850,"100kHz",160,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFPJ470UAR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1350,"100kHz",90,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFKJ470UAR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK0J470UR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFN0J470R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1800,"100kHz",95,"105°C","100kHz","(空白)","dia. 5",5.4,5.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEFC0J470AR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFC0J470R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",26,"105°C","120Hz","(空白)","dia. 4",5.8,6.1,2,"-40 to 105","105°C 2000H",2000,"Yes","NRND","E-Cap","EEEHBJ470UAR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,46,"105°C","120Hz","(空白)","dia. 5",5.4,5.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEHA0J470AR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA0J470R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHB0J470SR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.8,6.1,2,"-40 to 105","105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHB0J470AR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHB0J470R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 3000H",1000,"Yes","NRND","E-Cap","EEEHC0J470R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 6.3",5.4,5.5,2,"-40 to  85"," 85°C 2000H",1000,"Yes","NRND","E-Cap","EEE0JA470NP","Bipolar",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 5",5.4,5.5,2,"-40 to  85"," 85°C 2000H",1000,"Yes","NRND","E-Cap","EEE0JA470AR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE0JA470SR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,36,"105°C","120Hz","(空白)","dia. 4",5.4,5.5,2,"-40 to 105","105°C 1000H",2000,"Yes","NRND","E-Cap","EEEHA0J470WR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 4",5.4,5.5,2,"-40 to  85"," 85°C 1000H",2000,"Yes","NRND","E-Cap","EEE0JA470WR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"105°C","120Hz","(空白)","dia. 6.3",5.8,6.1,2,"-40 to 105","105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHP0J470P","Bipolar",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,9,"100kHz",6300,"45°C","100kHz",0.5,"7.3x4.3(D)",1,1,3,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFLR0J680R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"7.3x4.3(D)",1,1,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSR0J680R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.1000000000000001,1.2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCS0J680R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,"100kHz",1100,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","6TPB68M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","POSCAP","6TAB68M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"100kHz",140,"105°C","100kHz","(空白)","dia. 6.3",5.4,5.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEFC0J680AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFC0J680P"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1350,"100kHz",90,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFN0J680UR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NRND","E-Cap","EEEFK0J680SR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,82,40,"100kHz",1670,"105°C","100kHz",2.4,"dia. 6.3",4.9000000000000004,5,2,"-55 to 105","105°C 1000H",1300,"No","NRND","OS-CON","6SVPB82M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,45,"100kHz",1700,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","6SVP82M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",1000,"No","NRND","OS-CON","6SVQP82M","→6SVP82M",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,15,"100kHz",5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.4,1.5,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCT0J101R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0J101R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2800,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","6TPE100MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(5V)",3000,"No","Std","POSCAP","6TCE100MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",1600,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","6TPE100MPB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2150,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","6SVPC100MY"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2400,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","6TPE100M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(5V)",3000,"No","Std","POSCAP","6TCE100M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1970,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","6SVPC100M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"100kHz",1400,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","6TPE100MAZB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 1000H",2000,"No","Std","POSCAP","6TPE100MZB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"100kHz",1300,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","6TPE100MWB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1810,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","6SVP100M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",1000,"No","Std","OS-CON","6SVQP100M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1850,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","6TPE100MW"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,45,"100kHz",1200,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","6TPE100MVB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,"100kHz",950,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","Std","POSCAP","6TPE100MBB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,260,"100kHz",300,"105°C","100kHz","(空白)","dia. 6.3",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFP0J101AP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFP0J101AL","Halogen-free",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,360,"100kHz",240,"105°C","100kHz","(空白)","dia. 6.3",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFK0J101AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK0J101P"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK0J101AL","Halogen-free, Lead-free Reflow",null,null,{"$f":"IFERROR(HYPERLINK(I455),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 5",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFPJ101UAR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450,"100kHz",300,"105°C","100kHz","(空白)","dia. 6.3",7.7,8,2,"-55 to 105","105°C 7000H",900,"Yes","Std","E-Cap","EEEFH0J101XL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,700,"100kHz",160,"105°C","100kHz","(空白)","dia. 5",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFKJ101UAR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK0J101UR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFN0J101R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,850,"100kHz",160,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFT0J101AR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"100kHz",140,"105°C","100kHz","(空白)","dia. 6.3",5.4,5.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEFC0J101AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFC0J101P"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",47,"105°C","120Hz","(空白)","dia. 5",5.4,5.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEHAJ101WAR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA0J101WR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 5",5.4,5.5,2,"-40 to  85"," 85°C 1000H",1000,"Yes","NRND","E-Cap","EEE0JA101WAR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE0JA101WR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,71,"105°C","120Hz","(空白)","dia. 6.3",5.4,5.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEHA0J101AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA0J101P"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHB0J101SP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.8,6.1,2,"-40 to 105","105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHB0J101AP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHB0J101P"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 3000H",1000,"Yes","NRND","E-Cap","EEEHC0J101P"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 6.3",5.4,5.5,2,"-40 to  85"," 85°C 2000H",1000,"Yes","NRND","E-Cap","EEE0JA101AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE0JA101SP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,42,"105°C","120Hz","(空白)","dia. 5",5.8,6.1,2,"-40 to 105","105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHBJ101UAR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,7,"100kHz",7000,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0J121E7"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0J121R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(5V)",3500,"No","Std","SP-Cap","EEFJX0J121RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(5V)",3500,"No","Std","SP-Cap","EEFKX0J121RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(5V)",3500,"No","Std","SP-Cap","EEFTX0J121RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,"100kHz",2780,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","6SVP120MV"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,"100kHz",2660,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","6SVPC120MV"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"100kHz",2570,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","6SVPA120MAA"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",1000,"No","Std","OS-CON","6SVPS120M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"100kHz",1400,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","6TPE120MAZB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0J151ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"100kHz",3520,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 105","105°C 2000H",1500,"No","Std","OS-CON","6SVPE150M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5600,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0J151XR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3100,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","6TPE150MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(5V)",3000,"No","Std","POSCAP","6TCE150MF"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5100,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFCX0J151R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 3000H(5V)",3500,"No","Std","SP-Cap","EEFJX0J151RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 5500H(5V)",3500,"No","Std","SP-Cap","EEFKX0J151RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 135","135°C 5500H(5V)",3500,"No","Std","SP-Cap","EEFTX0J151RF","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2800,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","6TPE150MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(4V)",3000,"No","NRND","POSCAP","6THE150MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 1000H(5V)",3000,"No","Std","POSCAP","6TCE150MI"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",1600,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","6TPE150MAPB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2400,"45°C","100kHz",1.8,"7.3x4.3(D)",1.8,1.9,2,"-55 to 105","105°C 2000H",3000,"No","Std","POSCAP","6TPE150M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","105°C 2000H",3000,"Yes","Std","POSCAP","6TVE150M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,180,9,"100kHz",6300,"45°C","100kHz",1.2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3500,"No","Std","SP-Cap","EEFSX0J181ER"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(5V)",2500,"No","Std","POSCAP","6TCF220ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",1000,"No","Std","OS-CON","6SVPS220M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"100kHz",1400,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","6TPE220MAZB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,260,"100kHz",300,"105°C","100kHz","(空白)","dia. 6.3",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFP0J221AP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,360,"100kHz",240,"105°C","100kHz","(空白)","dia. 6.3",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFK0J221AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74,"105°C","120Hz","(空白)","dia. 6.3",5.4,5.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEHA0J221WP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,330,9,"100kHz",3900,"45°C","100kHz",2,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","6TPF330M9L"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2800,"45°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","Std","POSCAP","6TPE330MIL"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 2000H",2500,"No","Std","POSCAP","6TPB330ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,260,"100kHz",300,"105°C","100kHz","(空白)","dia. 6.3",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFT0J331AP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFN0J331XP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE0JA331P"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",1000,"No","Std","OS-CON","6SVPT390M","High Rel.",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 2000H",1000,"No","Std","OS-CON","6SVT390M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",3000,"45°C","100kHz",2.6,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","Std","POSCAP","6TPE470M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFTJ471XAL","Halogen-free",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NRND","E-Cap","EEEFKJ471XSP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",3000,"45°C","100kHz",2.6,"7.3x4.3(D)",3.8,4,2,"-55 to 105","105°C 2000H",2000,"No","Std","POSCAP","6TPE680M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 2000H",400,"No","Std","OS-CON","6SVT820M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK0J102AL","Halogen-free, Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"105°C","120Hz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to 105","105°C 1000H",500,"Yes","NRND","E-Cap","EEEHA0J102AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFP0J152AL","Halogen-free",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK0J152GL","Halogen-free",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA0J152P"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",680,"105°C","120Hz","(空白)","dia.12.5",13.5,14,2,"-55 to 105","105°C 5000H",200,"Yes","Std","E-Cap","EEEHD0J332AQ","Medium Size",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",1540,"105°C","120Hz","(空白)","dia.18",16.5,17,2,"-55 to 105","105°C 5000H",125,"Yes","Std","E-Cap","EEEHD0J752AM","Medium Size",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",25," 85°C","120Hz","(空白)","dia. 4",5.4,5.5,2,"-40 to  85"," 85°C 2000H",2000,"Yes","NRND","E-Cap","EEE1AA100NR","Bipolar",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA1A220WR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1350,"100kHz",90,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFKA330UAR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1A330UR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,43,"105°C","120Hz","(空白)","dia. 5",5.4,5.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEHA1A330AR","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47,35,"100kHz",1400,"45°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","_85°C 1000H",2000,"No","Std","POSCAP","10TPE47MAZB"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56,40,"100kHz",1670,"105°C","100kHz",2.4,"dia. 6.3",4.9000000000000004,5,2,"-55 to 105","105°C 1000H",1300,"No","NRND","OS-CON","10SVPB56M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2200,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","10SVPA68MAA"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"100kHz",230,"105°C","100kHz","(空白)","dia. 8",6.2,6.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEFC1A101AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA1A101WP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE1AA101SP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",1000,"No","Std","OS-CON","10SVQP120M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","105°C 2000H",2500,"Yes","Std","POSCAP","10TVE150ML"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,260,"100kHz",300,"105°C","100kHz","(空白)","dia. 6.3",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFP1A151AP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"100kHz",230,"105°C","100kHz","(空白)","dia. 8",6.2,6.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEFC1A151AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(6.3V)",2000,"No","NRND","POSCAP","10THB220M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 8",6.2,6.5,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFK1A221AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,360,"100kHz",240,"105°C","100kHz","(空白)","dia. 6.3",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFN1A221UP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NRND","E-Cap","EEEFK1A221SP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 2000H",500,"Yes","NRND","E-Cap","EEEHB1A221AP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",3700,"105°C","100kHz",5.2,"dia.10",7.9,8,2,"-55 to 105","105°C 2000H",500,"No","Std","OS-CON","10SVP270M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,80,"100kHz",850,"105°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFP1A331AP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1A331AL","Halogen-free, Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,197,"125°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-40 to 125","125°C 3000H",500,"Yes","Std","E-Cap","EEETK1A331UP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFC1A471P","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1A471AL","Halogen-free, Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA1A471UP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C 2000H",500,"Yes","NRND","E-Cap","EEE1AA471UP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,"100kHz",600,"105°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C10000H",500,"Yes","Std","E-Cap","EEEFH1A561L"," ",null,null,{"$f":"IFERROR(HYPERLINK(I967),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1A681AL","Halogen-free, Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFP1A102AL","Halogen-free",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",500,"Yes","Std","E-Cap","EEEFT1A102GP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1200,80,"100kHz",850,"105°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFPA122UAP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,80,"100kHz",850,"105°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFN1A152UP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NRND","E-Cap","EEEFK1A152SP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2400,60,"100kHz",1100,"105°C","100kHz","(空白)","dia.12.5",13.5,14,2,"-55 to 105","105°C 5000H",200,"Yes","Std","E-Cap","EEEFK1A242SQ","Medium Size",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",1280,"105°C","120Hz","(空白)","dia.16",16.5,17,2,"-55 to 105","105°C 5000H",125,"Yes","Std","E-Cap","EEEHD1A472AM","Medium Size",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1C100R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.8,6.1,2,"-40 to 105","105°C 2000H",2000,"Yes","NRND","E-Cap","EEEHB1C100AR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,90,"100kHz",1000,"105°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 2000H",2000,"No","NRND","POSCAP","16TQC22MYFB","→16TQC33MB2",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFN1C220R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA1C220R"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,"100kHz",1400,"105°C","100kHz",2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3000,"No","NRND","POSCAP","16TQC33MYFD","→20TQC33MD2",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,90,"100kHz",1000,"105°C","100kHz",1.3,"3.5x2.8(B)",1.9,2,2,"-55 to 105","105°C 1000H",2000,"No","NRND","POSCAP","16TQC33MYFB","→16TQC33MB2",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65,"105°C","120Hz","(空白)","dia. 6.3",5.8,6.1,2,"-40 to 105","105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHB1C330AP"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"New","POSCAP","16TQC47MD2","Reflow upgrade",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,360,"100kHz",240,"105°C","100kHz","(空白)","dia. 6.3",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFK1C470AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1350,"100kHz",90,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFN1C470UR"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 6.3",5.4,5.5,2,"-40 to  85"," 85°C 2000H",1000,"Yes","NRND","E-Cap","EEE1CA470AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,25,"100kHz",2440,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","16SVPC68MV"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,"100kHz",1500,"105°C","100kHz",2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3000,"No","NRND","POSCAP","16TQC68MYF","→16TQC68MD2",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"100kHz",230,"105°C","100kHz","(空白)","dia. 8",6.2,6.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEFC1C680AP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 2000H",1000,"No","Std","OS-CON","16SVPD82M"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"New","POSCAP","16TQC100MD2","Reflow upgrade",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFP1C101AL","Halogen-free",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"100kHz",197,"125°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-40 to 125","125°C 2000H",500,"Yes","Std","E-Cap","EEETG1C101P"," ",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 6.3",5.4,5.5,2,"-40 to  85"," 85°C 1000H",1000,"Yes","NRND","E-Cap","EEE1CA101WAP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,"100kHz",1800,"105°C","100kHz",2.2999999999999998,"7.3x4.3(D)",2.8,3,2,"-55 to 105","105°C 2000H",2500,"No","NRND","POSCAP","16TQC150MYF","→16TQC150MD3",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,340,"100kHz",280,"105°C","100kHz","(空白)","dia. 6.3",7.7,8,2,"-55 to 105","105°C 2000H",900,"Yes","Std","E-Cap","EEEFKC151XAP","Lead-free Reflow",null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1C151XP"," ",null,null,{"$f":"IFERROR(HYPERLINK(I1223),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,29,"100kHz",3430,"105°C","100kHz",5.2,"dia.10",7.9,8,2,"-55 to 105","105°C 2000H",500,"No","Std","OS-CON","16SVPA180M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFPC221XAL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 8",6.2,6.5,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFK1C221AP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFN1C221XL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA1C221XP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,"100kHz",4070,"105°C","100kHz",4.4000000000000004,"dia. 8",11.9,12,2,"-55 to 105","105°C 2000H",400,"No","Std","OS-CON","16SVPC270M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,330,6.5,"100kHz",7500,"105°C","100kHz",2.6,"dia. 6.3",10.4,10.5,2,"-55 to 105","105°C 5000H",700,"No","Std","OS-CON","16SVPG330M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"100kHz",500,"125°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to 125","125°C 3000H",500,"Yes","Std","E-Cap","EEETP1C331AP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,750,"125°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to 125","125°C 3000H",500,"Yes","Std","E-Cap","EEETC1C331P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1C331GL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA1C331P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFP1C471AL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1C471P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA1C471P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,"100kHz",4950,"105°C","100kHz",4.4000000000000004,"dia. 8",11.9,12,2,"-55 to 105","105°C 5000H",400,"No","Std","OS-CON","16SVPF560M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",400,"No","Std","OS-CON","16SVPT560M","High Rel."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NRND","E-Cap","EEEFK1C561SP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"100kHz",670,"105°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to 105","105°C 1000H",500,"Yes","NRND","E-Cap","EEEFC1C681AP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,160,"100kHz",600,"105°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFN1C681UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFT1C821UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",500,"No","Std","OS-CON","16SVPT1000MX","High Rel."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEETKC102UAQ","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1800,60,"100kHz",1100,"105°C","100kHz","(空白)","dia.12.5",13.5,14,2,"-55 to 105","105°C 5000H",200,"Yes","Std","E-Cap","EEEFK1C182SQ","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEETK1C332AM","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4700,33,"100kHz",2060,"105°C","100kHz","(空白)","dia.18",16.5,17,2,"-55 to 105","105°C 5000H",125,"Yes","Std","E-Cap","EEEFK1C472AM","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2040,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","20SVPA22M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,60,"100kHz",1450,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 2000H",1000,"No","Std","OS-CON","20SVP27M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",1000,"No","Std","OS-CON","20SVQP47M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"100kHz",2400,"105°C","100kHz",5.2,"dia.10",7.9,8,2,"-55 to 105","105°C 2000H",500,"No","Std","OS-CON","20SVP68M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",1000,"No","Std","OS-CON","20SVF120M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",1000,"No","Std","OS-CON","20SVPT180M","High Rel."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,390,14,"100kHz",4950,"105°C","100kHz",4.4000000000000004,"dia. 8",11.9,12,2,"-55 to 105","105°C 5000H",400,"No","Std","OS-CON","20SVPF390M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 2000H",400,"No","Std","OS-CON","20SVT560M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.8,3000,"100kHz",60,"105°C","100kHz","(空白)","dia. 4",5.4,5.5,2,"-40 to 105","105°C 1000H",2000,"Yes","NRND","E-Cap","EEEFC1E6R8AR","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHB1E6R8R"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",22,"105°C","120Hz","(空白)","dia. 4",5.4,5.5,2,"-40 to 105","105°C 1000H",2000,"Yes","NRND","E-Cap","EEEHAE100WAR","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.8,6.1,2,"-40 to 105","105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHB1E100AR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,48,"100kHz",1835,"105°C","100kHz",4.3,"dia. 8",6.9,7,2,"-55 to 125","125°C 2000H",1000,"No","Std","OS-CON","25SVPD22M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1E220R"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,850,"100kHz",160,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFT1E220AR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,"105°C","120Hz","(空白)","dia. 6.3",5.4,5.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEHA1E220AP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,33,35,"100kHz",2600,"105°C","100kHz",2.1,"dia. 5",5.9,6,2,"-55 to 125","125°C 1000H",1500,"No","Std","OS-CON","25SVPK33M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1E330P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1E330UR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 3000H",1000,"Yes","NRND","E-Cap","EEEHC1E330P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,"100kHz",900,"125°C","100kHz",2.6,"dia. 6.3",5.8,6.1,2,"-55 to 125","125°C 4000H",1000,"Yes","Std","Hybrid","EEHZC1E470P","EEHZC1E470V (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1E470P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450,"100kHz",300,"105°C","100kHz","(空白)","dia. 6.3",7.7,8,2,"-55 to 105","105°C 7000H",900,"Yes","Std","E-Cap","EEEFH1E470XL"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.7,8,2,"-40 to 105","105°C 3000H",900,"Yes","NRND","E-Cap","EEEHC1E470XP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,80,"100kHz",850,"125°C","100kHz",2.2999999999999998,"dia. 5",5.8,6.1,2,"-55 to 125","125°C 4000H",1000,"Yes","Std","Hybrid","EEHZK1E560UR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H(20V)",2500,"No","NRND","POSCAP","25TDC68MYF","→25TDC68MD3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 5",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFT1E680AR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",1000,"No","Std","OS-CON","25SVPT100M","High Rel."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFPE101XAL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"100kHz",450,"105°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-40 to 105","105°C 1000H",500,"Yes","NRND","E-Cap","EEEFC1E101AP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFC1E101P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",180," 85°C","120Hz","(空白)","dia. 8",10.199999999999999,10.5,2,"-40 to  85"," 85°C 2000H",500,"Yes","NRND","E-Cap","EEE1EA101AP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHB1E101P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE1EA101XP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,38,"100kHz",1500,"125°C","100kHz",2.6,"dia. 6.3",5.8,6.1,2,"-55 to 135","125°C 4000H / 135°C 2000H",1000,"Yes","New","Hybrid","EEHZL1E151P","EEHZL1E151V (anti-vib)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1E151P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,340,"100kHz",280,"105°C","100kHz","(空白)","dia. 6.3",7.7,8,2,"-55 to 105","105°C 2000H",900,"Yes","Std","E-Cap","EEEFNE181XUP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2300,"105°C","100kHz",3.4,"dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C10000H",500,"Yes","Std","Hybrid","EEHZA1E221P","EEHZA1E221V (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFTE221XAL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFN1E221P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,197,"125°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-40 to 125","125°C 3000H",500,"Yes","Std","E-Cap","EEETK1E221UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE1EA221P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",400,"No","Std","OS-CON","25SVPT330M","High Rel."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,"100kHz",2000,"125°C","100kHz",3.4,"dia. 8",10.199999999999999,10.5,2,"-55 to 125","125°C 4000H",500,"Yes","Std","Hybrid","EEHZK1E331UP","EEHZK1E331UV (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,850,"105°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-55 to 105","105°C10000H",500,"Yes","Std","E-Cap","EEEFH1E331L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,270,"125°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to 125","125°C 3000H",500,"Yes","Std","E-Cap","EEETK1E331UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"100kHz",270,"125°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to 125","125°C 2000H",500,"Yes","Std","E-Cap","EEETG1E331UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to  85"," 85°C 2000H",500,"Yes","NRND","E-Cap","EEE1EA331AP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFP1E471AL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",500,"Yes","Std","E-Cap","EEEFK1E471GP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,750,"125°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to 125","125°C 3000H",500,"Yes","Std","E-Cap","EEETC1E471UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C 2000H",500,"Yes","NRND","E-Cap","EEE1EA471P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFT1E561UL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,"100kHz",800,"125°C","100kHz","(空白)","dia.12.5",13.5,14,2,"-40 to 125","125°C 2000H",200,"Yes","Std","E-Cap","EEVTG1E681UQ","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NRND","E-Cap","EEEFK1E821SP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,"100kHz",4000,"125°C","100kHz",5.2,"dia.10",16.5,16.8,2,"-55 to 125","125°C 4000H / 135°C 4000H",250,"Yes","Std","Hybrid","EEHZS1E102UP","EEHZS1E102UV (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",580,"105°C","120Hz","(空白)","dia.12.5",13.5,14,2,"-55 to 105","105°C 5000H",200,"Yes","Std","E-Cap","EEEHD1E102AQ","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",1200,"105°C","120Hz","(空白)","dia.16",16.5,17,2,"-55 to 105","105°C 5000H",125,"Yes","Std","E-Cap","EEEHD1E222AM","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEVFK1E332M","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3000,"100kHz",60,"105°C","100kHz","(空白)","dia. 4",5.4,5.5,2,"-40 to 105","105°C 1000H",2000,"Yes","NRND","E-Cap","EEEFC1V4R7AR","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"105°C","120Hz","(空白)","dia. 4",5.8,6.1,2,"-40 to 105","105°C 3000H",2000,"Yes","NRND","E-Cap","EEEHC1V4R7R"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,"100kHz",1000,"105°C","(空白)",2,"7.3x4.3(D)",1.9,2,2,"-55 to 105","105°C 2000H",3000,"No","NRND","POSCAP","35TQC10MYF","→35TQC10MD2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450,"100kHz",300,"105°C","100kHz","(空白)","dia. 6.3",7.7,8,2,"-55 to 105","105°C 7000H",900,"Yes","Std","E-Cap","EEEFH1V100XL"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7200,"100kHz",28,"105°C","120Hz","(空白)","dia. 5",5.8,6.1,2,"-40 to 105","105°C 5000H",1000,"Yes","NRND","E-Cap","EEEHD1V100AR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"New","POSCAP","35TQC15MD2","Reflow upgrade"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NRND","E-Cap","EEEFK1V180SR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,360,"100kHz",240,"105°C","100kHz","(空白)","dia. 5",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFP1V220AR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFC1V220P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHB1V220P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1V330P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1V330AL","Halogen-free, Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,130," 85°C","120Hz","(空白)","dia. 8",6.2,6.5,2,"-40 to  85"," 85°C 2000H",1000,"Yes","NRND","E-Cap","EEE1VA330AP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57,"105°C","120Hz","(空白)","dia. 6.3",7.7,8,2,"-40 to 105","105°C 3000H",900,"Yes","NRND","E-Cap","EEEHC1V330XP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",3650,"105°C","100kHz",5,"dia.10",12.6,12.7,2,"-55 to 125","125°C 2000H",400,"No","Std","OS-CON","35SVPD47M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"New","POSCAP","35TQS47MEX"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFC1V470P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE1VA470WP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA1V470P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56,60,"100kHz",1200,"125°C","100kHz",2.6,"dia. 6.3",5.8,6.1,2,"-55 to 125","125°C 4000H",1000,"Yes","Std","Hybrid","EEHZK1V560P","EEHZK1V560V (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFT1V680AL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C20000H",400,"No","Std","OS-CON","35SVPT82M","High Rel."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"100kHz",1700,"125°C","100kHz",2.8,"dia. 6.3",7.7,8,2,"-55 to 125","125°C 4000H",900,"Yes","Std","Hybrid","EEHZK1V101XP","EEHZK1V101XV (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFK1V101AP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,260,"100kHz",300,"105°C","100kHz","(空白)","dia. 6.3",5.8,6.1,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFT1V101AP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 8",10.199999999999999,10.5,2,"-40 to 125","125°C 3000H",500,"Yes","Std","E-Cap","EEETK1V101UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE1VA101P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,"105°C","120Hz","(空白)","dia. 8",10.199999999999999,10.5,2,"-40 to 105","105°C 1000H",500,"Yes","NRND","E-Cap","EEEHAV101UAP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFNV121XUL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,"100kHz",1900,"125°C","100kHz",2.8,"dia. 6.3",7.7,8,2,"-55 to 135","125°C 4000H / 135°C 2000H",900,"Yes","New","Hybrid","EEHZL1V151XP","EEHZL1V151XV (anti-vib)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1V151P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1V151GL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFC1V221P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1V221GL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,170,"105°C","120Hz","(空白)","dia. 8",10.199999999999999,10.5,2,"-40 to 105","105°C 1000H",500,"Yes","NRND","E-Cap","EEEHAV221UAP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA1V221P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,160,"100kHz",600,"105°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFN1V271UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFP1V331AL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFC1V331P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",250,"105°C","120Hz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to 105","105°C 1000H",500,"Yes","NRND","E-Cap","EEEHAV331UAP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFT1V391UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,470,9,"100kHz",5500,"125°C","100kHz",5.2,"dia.10",16.5,16.8,2,"-55 to 135","125°C 4000H / 135°C 4000H",250,"Yes","Std","Hybrid","EEHZU1V471P","EEHZU1V471V (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,560,60,"100kHz",1190,"105°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFT1V561AP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFT1V561AL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEVFK1V681Q","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEVFK1V152M","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",1450,"105°C","120Hz","(空白)","dia.18",16.5,17,2,"-55 to 105","105°C 5000H",125,"Yes","Std","E-Cap","EEEHD1V182AM","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.8,6.1,2,"-40 to 105","105°C 2000H",2000,"Yes","NRND","E-Cap","EEEHB1H1R0AR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 2000H",2000,"Yes","NRND","E-Cap","EEEHB1H2R2SR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12000,"100kHz",16,"105°C","120Hz","(空白)","dia. 4",5.8,6.1,2,"-40 to 105","105°C 5000H",2000,"Yes","NRND","E-Cap","EEEHD1H3R3R"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 4",5.4,5.5,2,"-40 to  85"," 85°C 2000H",2000,"Yes","NRND","E-Cap","EEE1HA3R3AR","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3000,"100kHz",50,"105°C","100kHz","(空白)","dia. 5",5.4,5.5,2,"-40 to 105","105°C 1000H",1000,"Yes","NRND","E-Cap","EEEFC1H4R7R"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 3000H",1000,"Yes","NRND","E-Cap","EEEHC1H4R7R"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,40,"100kHz",2500,"105°C","100kHz",2.7,"dia. 6.3",5.9,6,2,"-55 to 105","105°C 5000H",1000,"No","Std","OS-CON","50SVPF10M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3500,"100kHz",60,"105°C","100kHz","(空白)","dia. 4",5.8,6.1,2,"-55 to 105","105°C 2000H",2000,"Yes","Std","E-Cap","EEEFN1H100UR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHB1H100P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125°C 2000H",1000,"No","Std","OS-CON","50SVT18M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NRND","E-Cap","EEEFK1H220SR"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 2000H",1000,"Yes","NRND","E-Cap","EEEHB1H220AP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE1HA220WP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1H330L","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,91,"105°C","120Hz","(空白)","dia. 8",10.199999999999999,10.5,2,"-40 to 105","105°C 1000H",500,"Yes","NRND","E-Cap","EEEHA1H330AP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",500,"Yes","NRND","E-Cap","EEEHC1H330P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NRND","E-Cap","EEEFK1H390SP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 8",6.2,6.5,2,"-55 to 105","105°C 2000H",1000,"Yes","Std","E-Cap","EEEFK1H470P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEHA1H470UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,130," 85°C","120Hz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to  85"," 85°C 2000H",500,"Yes","NRND","E-Cap","EEE1HA470AP","Lead-free Reflow"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE1HA470P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"135°C","100kHz",3.4,"dia. 8",10.199999999999999,10.5,2,"-55 to 145","135°C 4000H / 145°C 2000H",500,"Yes","Std","Hybrid","EEHZE1H680P","EEHZE1H680V (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,680,"100kHz",195,"105°C","100kHz","(空白)","dia. 6.3",7.7,8,2,"-55 to 105","105°C 2000H",900,"Yes","Std","E-Cap","EEEFNH820XUP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,180,"100kHz",670,"105°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFP1H101AP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFK1H101P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEE1HA101P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,12,"100kHz",4600,"125°C","100kHz",4.88,"dia.10",12.5,12.8,2,"-55 to 135","125°C 4000H / 135°C 4000H",400,"Yes","Std","Hybrid","EEHZU1H151P","EEHZU1H151V (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1H151GL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,340,"100kHz",350,"105°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFN1H181UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,180,"100kHz",670,"105°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFK1H221P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"100kHz",500,"105°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to 105","105°C 1000H",500,"Yes","NRND","E-Cap","EEEFC1H221P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,180,"100kHz",670,"105°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFN1H271UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEETK1H331AQ","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,680,73,"100kHz",1610,"105°C","100kHz","(空白)","dia.16",16.5,17,2,"-55 to 105","105°C 5000H",125,"Yes","Std","E-Cap","EEEFK1H681AM","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"100kHz",900,"125°C","100kHz","(空白)","dia.16",16.5,17,2,"-40 to 125","125°C 2000H",125,"Yes","Std","E-Cap","EEVTG1H681UM","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFN1J100L","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2000,"100kHz",45,"105°C","120Hz","(空白)","dia. 8",6.2,6.5,2,"-40 to 105","105°C 5000H",1000,"Yes","NRND","E-Cap","EEEHD1J100P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1J220L","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,33,22,"100kHz",3300,"125°C","100kHz",3.4,"dia. 8",10.199999999999999,10.5,2,"-55 to 135","125°C 4000H / 135°C 4000H",500,"Yes","New","Hybrid","EEHZV1J330P","EEHZV1J330V (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1J330L","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"105°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C10000H",500,"Yes","New","E-Cap","EEEFH2A330L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"100kHz",100,"125°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-40 to 125","125°C 2000H",500,"Yes","Std","E-Cap","EEETG1J470UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1400,"125°C","100kHz",4,"dia.10",10.199999999999999,10.5,2,"-55 to 125","125°C 4000H",500,"Yes","Std","Hybrid","EEHZC1J560P","EEHZC1J560V (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1800,"105°C","100kHz",4,"dia.10",10.199999999999999,10.5,2,"-55 to 105","105°C10000H",500,"Yes","Std","Hybrid","EEHZA1J680P","EEHZA1J680V (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFK1J680UL","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,12,"100kHz",4600,"125°C","100kHz",4.88,"dia.10",12.5,12.8,2,"-55 to 135","125°C 4000H / 135°C 4000H",400,"Yes","Std","Hybrid","EEHZU1J101P","EEHZU1J101V (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFN1J101L","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",3280,"105°C","100kHz",5,"dia.10",12.6,12.7,2,"-55 to 125","125°C 1000H",400,"No","New","OS-CON","63SXV150M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,260,"100kHz",350,"125°C","100kHz","(空白)","dia.12.5",13.5,14,2,"-40 to 125","125°C 2000H",200,"Yes","Std","E-Cap","EEVTG1J221Q","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,680,80,"100kHz",1690,"105°C","100kHz","(空白)","dia.18",16.5,17,2,"-55 to 105","105°C 5000H",125,"Yes","Std","E-Cap","EEEFK1J681AM","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,470,100,"100kHz",1900,"125°C","100kHz","(空白)","dia.16",16.5,17,2,"-55 to 125","125°C 3000H",125,"Yes","Std","E-Cap","EEETP70471M","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,60,"100kHz",1100,"105°C","100kHz",4.3,"dia. 8",6.9,7,2,"-55 to 125","125°C 1000H",1000,"No","Std","OS-CON","80SXV12M"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,45,"100kHz",1550,"105°C","100kHz",3.4,"dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C10000H",500,"Yes","Std","Hybrid","EEHZA1K220P","EEHZA1K220V (anti-vib.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,"100kHz",2080,"105°C","100kHz",4.7,"dia.10",7.9,8,2,"-55 to 125","125°C 1000H",500,"No","Std","OS-CON","80SXV27MX"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFN1K330L","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"100kHz",90,"125°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to 125","125°C 2000H",500,"Yes","Std","E-Cap","EEETG1K470UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEVFK1K680Q","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,420,"100kHz",250,"125°C","100kHz","(空白)","dia.12.5",13.5,14,2,"-40 to 125","125°C 2000H",200,"Yes","Std","E-Cap","EEVTG1K101UQ","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,330,170,"100kHz",793,"105°C","100kHz","(空白)","dia.16",16.5,17,2,"-55 to 105","105°C 5000H",125,"Yes","Std","E-Cap","EEEFK1K331AM","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,280,"100kHz",400,"125°C","100kHz","(空白)","dia.18",16.5,17,2,"-40 to 125","125°C 2000H",125,"Yes","Std","E-Cap","EEVTG1K471M","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,680,68,"100kHz",2600,"125°C","100kHz","(空白)","dia.18",21.5,22,2,"-55 to 125","125°C 4000H",75,"Yes","Std","E-Cap","EEETP1K681M","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",50," 85°C","120Hz","(空白)","dia. 8",6.2,6.5,2,"-40 to  85"," 85°C 2000H",1000,"Yes","NRND","E-Cap","EEE2AA100UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"100kHz",90,"125°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-40 to 125","125°C 2000H",500,"Yes","Std","E-Cap","EEETG2A220P"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1300,"100kHz",130,"105°C","100kHz","(空白)","dia. 8",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFN2A270UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEEFN2A330L","Halogen-free"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,700,"100kHz",200,"105°C","100kHz","(空白)","dia.10",10.199999999999999,10.5,2,"-55 to 105","105°C 2000H",500,"Yes","Std","E-Cap","EEEFN2A470UP"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEVFK2A101M","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,330,153,"100kHz",917,"105°C","100kHz","(空白)","dia.18",16.5,17,2,"-55 to 105","105°C 5000H",125,"Yes","Std","E-Cap","EEEFK2A331AM","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EEVFK2A331M","Medium Size"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"100kHz",4700,"105°C","100kHz",2.7,"dia. 8",9,9,2,"-55 to 105","105°C 5000H",200,"No","NRND","OS-CON","2SEPC560MX","→4SVPC560M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2700,10,"100kHz",5560,"105°C","100kHz",5.8,"dia.10",13,13,2,"-55 to 105","105°C 5000H",200,"No","NRND","OS-CON","2SEPC2700M","→2R5SVPC2700M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",500,"No","NRND","OS-CON","4SEQP150M","→4SVQP150M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",140," 85°C","120Hz","(空白)","dia. 8",7,8,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA0GKA471"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1200,12,"100kHz",5440,"105°C","100kHz",5.8,"dia.10",13,13,2,"-55 to 105","105°C 3000H",200,"No","NRND","OS-CON","4SEP1200M","→4SVP1200M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,6,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA0JKS330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",71," 85°C","120Hz","(空白)","dia. 6.3",5,6,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA0JKS101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 5",7,8,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA0JKA101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,130,"100kHz",455,"105°C","100kHz","(空白)","dia. 6.3",11.2,12.7,2,"-40 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUFR0J221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350,"100kHz",290,"105°C","100kHz","(空白)","dia. 6.3",11.2,12.2,2,"-55 to 105","105°C 1000H",200,"Yes","Std","E-Cap","EEUFC0J331S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"100kHz",5700,"105°C","100kHz",2.7,"dia. 8",9,9,2,"-55 to 105","105°C 5000H",200,"No","NRND","OS-CON","6SEPC470MX","→6SVP470M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,560,7,"100kHz",5600,"105°C","100kHz",2,"dia. 6.3",9,9,2,"-55 to 105","105°C 5000H",500,"No","NRND","OS-CON","6SEPC560MW","→10SVP560M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85,"100kHz",730,"105°C","100kHz","(空白)","dia. 8",15,16.5,2,"-55 to 105","105°C 2000H",200,"Yes","Std","E-Cap","EEUFC0J821L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,580," 85°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA0JM102"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1560,"105°C","100kHz","(空白)","dia. 8",20,22,2,"-40 to 105","105°C 9000H",200,"No","Std","E-Cap","EEUFR0J152L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,"100kHz",1240,"105°C","100kHz","(空白)","dia. 8",15,16.5,2,"-40 to 105","105°C 8000H",200,"No","Std","E-Cap","EEUFS0J152L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2000,30,"100kHz",1560,"105°C","100kHz","(空白)","dia. 8",20,22,2,"-40 to 105","105°C 9000H",200,"No","Std","E-Cap","EEUFS0J202L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,890," 85°C","120Hz","(空白)","dia.10",16,17,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA0JM222"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",2140,"105°C","100kHz","(空白)","dia.10",30,32,2,"-55 to 105","105°C 4000H",100,"Yes","Std","E-Cap","EEUFK0J332L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2600,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUFR0J392"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,36,"100kHz",2060,"105°C","100kHz","(空白)","dia.18",15,16.5,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFK0J472S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,"100kHz",3300,"105°C","100kHz","(空白)","dia.16",20,22,2,"-40 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUFM0J562S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2655,"105°C","100kHz","(空白)","dia.12.5",40,42,2,"-55 to 105","105°C 5000H",100,"Yes","NRND","E-Cap","EEUFC0J682L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"100kHz",2555,"105°C","100kHz","(空白)","dia.16",25,27,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC0J682"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,"100kHz",3820,"105°C","100kHz","(空白)","dia.16",25,27,2,"-40 to 105","105°C10000H",100,"No","Std","E-Cap","EEUFR0J822"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1650,"105°C","120Hz","(空白)","dia.16",25,27,2,"-55 to 105","105°C 2000H",100,"Yes","Std","E-Cap","ECA0JHG103"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,10,"N/A","100kHz",25," 85°C","120Hz","(空白)","dia. 4",7,8,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA1AKN100","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,6,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA1ASN330","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",500,"No","NRND","OS-CON","10SEQP56M","→10SVQP56M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,110,"105°C","120Hz","(空白)","dia. 6.3",7,8,2,"-55 to 105","105°C 1000H",200,"No","Std","E-Cap","EEAGA1A101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,220,130,"100kHz",455,"105°C","100kHz","(空白)","dia. 6.3",11.2,12.7,2,"-40 to 105","105°C 2000H",200,"No","Std","E-Cap","EEUFM1A221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",200," 85°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECEA1AN221U","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",200,"No","NRND","OS-CON","10SEQP270M","→10SVP270M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,280," 85°C","120Hz","(空白)","dia.10",16,17,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECEA1AN331U","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,560,13,"100kHz",5230,"105°C","100kHz",5.8,"dia.10",13,13,2,"-55 to 105","105°C 3000H",200,"No","NRND","OS-CON","10SEP560M","→10SVP560M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85,"100kHz",730,"105°C","100kHz","(空白)","dia. 8",15,16.5,2,"-55 to 105","105°C 2000H",200,"Yes","Std","E-Cap","EEUFC1A681L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1560,"105°C","100kHz","(空白)","dia. 8",20,22,2,"-40 to 105","105°C 4000H",200,"No","Std","E-Cap","EEUFM1A102L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,630," 85°C","120Hz","(空白)","dia.10",12.5,13.5,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA1AM102"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1560,"105°C","100kHz","(空白)","dia. 8",20,22,2,"-40 to 105","105°C 9000H",200,"No","Std","E-Cap","EEUFR1A152L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,45,"100kHz",1440,"105°C","100kHz","(空白)","dia.10",25,27,2,"-55 to 105","105°C 3000H",200,"Yes","Std","E-Cap","EEUFC1A152"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2000,20,"100kHz",2180,"105°C","100kHz","(空白)","dia.10",20,22,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUFS1A202"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,540,"105°C","120Hz","(空白)","dia.12.5",20,22,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUEB1A222"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3300,15,"100kHz",3190,"105°C","100kHz","(空白)","dia.12.5",25,27,2,"-40 to 105","105°C 7000H",200,"No","Std","E-Cap","EEUFM1A332"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,802,"105°C","120Hz","(空白)","dia.12.5",25,27,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUEB1A332"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3190,"105°C","100kHz","(空白)","dia.12.5",25,27,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUFS1A472"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",1200," 85°C","120Hz","(空白)","dia.18",35.5,37.5,2,"-40 to  85"," 85°C 2000H",50,"No","Std","E-Cap","ECEA1AN472U","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,"100kHz",3300,"105°C","100kHz","(空白)","dia.16",20,22,2,"-40 to 105","105°C10000H",100,"No","Std","E-Cap","EEUFS1A562S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6800,12,"100kHz",3750,"105°C","100kHz","(空白)","dia.12.5",35,37,2,"-40 to 105","105°C10000H",100,"No","Std","E-Cap","EEUFR1A682L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1570,"105°C","120Hz","(空白)","dia.16",25,27,2,"-55 to 105","105°C 2000H",100,"Yes","Std","E-Cap","ECA1AHG682"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1890,"105°C","120Hz","(空白)","dia.16",31.5,33.5,2,"-55 to 105","105°C 2000H",100,"Yes","Std","E-Cap","ECA1AHG103"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,4.7,"N/A","100kHz",20," 85°C","120Hz","(空白)","dia. 4",7,8,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA1CKN4R7","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"N/A","100kHz",60,"105°C","120Hz","(空白)","dia. 5",11,12,2,"-40 to 105","105°C 1000H",200,"No","Std","E-Cap","ECA1CEN220","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,33,"N/A","100kHz",80,"105°C","120Hz","(空白)","dia. 5",11,12,2,"-40 to 105","105°C 1000H",200,"No","Std","E-Cap","ECA1CEN330","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47,800,"100kHz",175,"105°C","100kHz","(空白)","dia. 5",11,12,2,"-40 to 105","105°C 1000H",200,"Yes","Std","E-Cap","EEUFC1C470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",200,"No","Std","E-Cap","EEUFR1C680"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,800,"100kHz",175,"105°C","100kHz","(空白)","dia. 5",11,12,2,"-55 to 105","105°C 1000H",200,"Yes","Std","E-Cap","EEUFC1C680"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,2,"-55 to 105","105°C 1000H",200,"No","Std","E-Cap","EEUHD1C101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"100kHz",3220,"105°C","100kHz",2.8,"dia. 8",7,7,2,"-55 to 105","105°C 5000H",200,"No","NRND","OS-CON","16SEPC150MD","→16SVPC150M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",500,"No","NRND","OS-CON","16SEF180M","→16SVF180M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,270,8,"100kHz",5800,"105°C","100kHz",2.6,"dia. 6.3",10,10,2,"-55 to 105","105°C 5000H",500,"No","NRND","OS-CON","16SEPG270M","→16SVPG270M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,117,"100kHz",555,"105°C","100kHz","(空白)","dia. 8",11.5,12.5,2,"-55 to 105","105°C 2000H",200,"Yes","Std","E-Cap","EEUFC1C331"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,38,"100kHz",1290,"105°C","100kHz","(空白)","dia.10",12.5,14,2,"-40 to 105","105°C 4000H",200,"No","Std","E-Cap","EEUFM1C471"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,440," 85°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA1CM471"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1560,"105°C","100kHz","(空白)","dia. 8",20,22,2,"-40 to 105","105°C 4000H",200,"No","Std","E-Cap","EEUFM1C681L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63,"100kHz",900,"105°C","100kHz","(空白)","dia.10",12.5,14,2,"-55 to 105","105°C 4000H",200,"Yes","Std","E-Cap","EEUFK1C681"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,"100kHz",2180,"105°C","100kHz","(空白)","dia.10",20,22,2,"-40 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUFM1C102"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,560,"105°C","120Hz","(空白)","dia.10",16,17,2,"-55 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA1CHG102"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,18,"100kHz",2600,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-40 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUFM1C152"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,38,"100kHz",2000,"105°C","100kHz","(空白)","dia.18",15,16.5,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC1C182S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,"100kHz",2250,"125°C","100kHz","(空白)","dia.18",20,22,2,"-40 to 125","125°C 2000H",100,"Yes","Std","E-Cap","EEUTA1C222S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"100kHz",2280,"105°C","100kHz","(空白)","dia.12.5",25,27,2,"-55 to 105","105°C 5000H",200,"Yes","Std","E-Cap","EEUFK1C272"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",2310,"105°C","100kHz","(空白)","dia.12.5",30,32,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC1C272L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"100kHz",2510,"105°C","100kHz","(空白)","dia.12.5",35,37,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC1C332"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,"100kHz",3820,"105°C","100kHz","(空白)","dia.16",25,27,2,"-40 to 105","105°C 7000H",100,"No","Std","E-Cap","EEUFM1C392"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,"100kHz",3300,"105°C","100kHz","(空白)","dia.16",20,22,2,"-40 to 105","105°C10000H",100,"No","Std","E-Cap","EEUFS1C472S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5600,14,"100kHz",3820,"105°C","100kHz","(空白)","dia.16",25,27,2,"-40 to 105","105°C10000H",100,"No","Std","E-Cap","EEUFR1C562"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,27,2,"-55 to 105","105°C 2000H",100,"No","Std","E-Cap","EEUHD1C682"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",500,"No","NRND","OS-CON","20SEQP22M","→20SVQP22M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",500,"No","NRND","OS-CON","20SEF120M","→20SVF120M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,20,"100kHz",4320,"105°C","100kHz",5.8,"dia.10",13,13,2,"-55 to 105","105°C 3000H",200,"No","NRND","OS-CON","20SEP150M","→20SVP150M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,3.3,"N/A","100kHz",18," 85°C","120Hz","(空白)","dia. 5",5,6,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA1ESN3R3","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 85°C","120Hz","(空白)","dia. 5",11,12,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECEA1EN100U","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 5",7,8,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA1EKA220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",200,"No","Std","E-Cap","EEUFR1E470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,300,"100kHz",280,"105°C","100kHz","(空白)","dia. 5",11,12.5,2,"-40 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUFR1E680"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 5000H",200,"No","Std","E-Cap","EEUFR1E101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,27,"100kHz",800,"150°C","100kHz",3.4,"dia. 8",9.5,10.5,2,"-55 to 150","150°C 1000H",200,"Yes","Std","Hybrid","EEHAZF1E151B"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1600,"125°C","100kHz",3.4,"dia. 8",9.5,10.5,2,"-55 to 125","125°C 4000H",1000,"Yes","Std","Hybrid","EEHAZC1E151B"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2300,"105°C","100kHz",3.4,"dia. 8",9.5,10.5,2,"-55 to 105","105°C10000H",1000,"Yes","Std","Hybrid","EEHAZA1E221B"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,125,"105°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-40 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUEB1E221S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",200,"No","NRND","OS-CON","25SEF330M","→25SVF330M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,130,"100kHz",945,"135°C","100kHz","(空白)","dia.10",16,17.5,2,"-40 to 135","135°C 2000H",200,"Yes","Std","E-Cap","EEUTP1E331"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5000,"105°C","100kHz",5.8,"dia.10",13,13,2,"-55 to 125","125°C 1000H",200,"No","NRND","OS-CON","25SEK470M","→25SVPK470M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63,"100kHz",900,"105°C","100kHz","(空白)","dia.10",12.5,14,2,"-55 to 105","105°C 4000H",200,"Yes","Std","E-Cap","EEUFK1E471"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,510,130,"100kHz",945,"135°C","100kHz","(空白)","dia.10",16,17.5,2,"-40 to 135","135°C 2000H",200,"Yes","Std","E-Cap","EEUTP1E511"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,560,11,"100kHz",4000,"125°C","100kHz",5.2,"dia.10",15.7,16.7,2,"-55 to 125","125°C 4000H / 135°C 4000H",500,"Yes","Std","Hybrid","EEHAZS1E561B"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,"100kHz",2180,"105°C","100kHz","(空白)","dia.10",20,22,2,"-40 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUFM1E681"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,52,"100kHz",1100,"135°C","100kHz","(空白)","dia.10",20,22,2,"-40 to 135","135°C 2000H",200,"Yes","Std","E-Cap","EEUTP1E821"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,38,"100kHz",1655,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC1E102"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,498,"105°C","120Hz","(空白)","dia.12.5",20,22,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUEB1E102"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1490,"135°C","100kHz","(空白)","dia.12.5",20,22,2,"-40 to 135","135°C 2000H",200,"Yes","Std","E-Cap","EEUTP1E122"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"100kHz",2310,"105°C","100kHz","(空白)","dia.12.5",30,32,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC1E182L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"100kHz",3190,"105°C","100kHz","(空白)","dia.12.5",25,27,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUFS1E222"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,"100kHz",2330,"105°C","100kHz","(空白)","dia.16",20,22,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFK1E222S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1200," 85°C","120Hz","(空白)","dia.12.5",25,27,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA1EM222"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28,"100kHz",2250,"135°C","100kHz","(空白)","dia.18",20,22,2,"-40 to 135","135°C 2000H",100,"Yes","Std","E-Cap","EEUTP1E272S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,"100kHz",2760,"105°C","100kHz","(空白)","dia.16",25,27,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFK1E332"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4700,15,"100kHz",3680,"105°C","100kHz","(空白)","dia.18",35.5,37.5,2,"-55 to 105","105°C 5000H",50,"Yes","Std","E-Cap","EEUFC1E472"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6800,"N/A","100kHz",2040,"105°C","120Hz","(空白)","dia.18",35.5,37.5,2,"-55 to 105","105°C 2000H",50,"Yes","Std","E-Cap","ECA1EHG682"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",200,"No","NRND","OS-CON","32SEF68M","→35SVPK82M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7,"N/A","100kHz",22," 85°C","120Hz","(空白)","dia. 5",7,8,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA1VKN4R7","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30," 85°C","120Hz","(空白)","dia. 6.3",7,8,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA1VKN100","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60," 85°C","120Hz","(空白)","dia. 6.3",7,8,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA1VKA220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,39,30,"100kHz",2800,"105°C","100kHz",2.8,"dia. 8",7,7,2,"-55 to 105","105°C 5000H",200,"No","NRND","OS-CON","35SEPF39M","→35SVPF39M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,2,"-55 to 105","105°C 1000H",200,"No","Std","E-Cap","EEUHD1V470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,130,"100kHz",455,"105°C","100kHz","(空白)","dia. 6.3",11.2,12.7,2,"-40 to 105","105°C 2000H",200,"No","Std","E-Cap","EEUFM1V680"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,27,"100kHz",1600,"125°C","100kHz",3.4,"dia. 8",9.5,10.5,2,"-55 to 125","125°C 4000H",1000,"Yes","Std","Hybrid","EEHAZC1V101B"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125","125°C 1000H",200,"No","NRND","OS-CON","35SEF120M","→35SVPF120M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,117,"100kHz",555,"105°C","100kHz","(空白)","dia. 8",11.5,12.5,2,"-55 to 105","105°C 2000H",200,"Yes","Std","E-Cap","EEUFC1V151"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2500,"105°C","100kHz",4,"dia.10",9.5,10.5,2,"-55 to 105","105°C10000H",500,"Yes","Std","Hybrid","EEHAZA1V221B"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56,"100kHz",950,"105°C","100kHz","(空白)","dia. 8",11.5,13,2,"-40 to 105","105°C 6000H",200,"No","Std","E-Cap","EEUFR1V221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350," 85°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA1VM221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63,"100kHz",900,"105°C","100kHz","(空白)","dia.10",12.5,14,2,"-55 to 105","105°C 4000H",200,"Yes","Std","E-Cap","EEUFK1V271"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,"100kHz",1240,"105°C","100kHz","(空白)","dia. 8",15,16.5,2,"-40 to 105","105°C 8000H",200,"No","Std","E-Cap","EEUFS1V331L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,440," 85°C","120Hz","(空白)","dia.10",12.5,13.5,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA1VM331"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,"100kHz",3500,"125°C","100kHz",4.88,"dia.10",11.7,12.7,2,"-55 to 125","125°C 4000H / 135°C 4000H",500,"Yes","Std","Hybrid","EEHAZSV471UB"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,52,"100kHz",1220,"105°C","100kHz","(空白)","dia.10",20,22,2,"-55 to 105","105°C 3000H",200,"Yes","Std","E-Cap","EEUFC1V471"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,349,"105°C","120Hz","(空白)","dia.10",20,22,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUEB1V471"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,48,"100kHz",1400,"105°C","100kHz","(空白)","dia.12.5",15,16.5,2,"-55 to 105","105°C 5000H",200,"Yes","Std","E-Cap","EEUFK1V561S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,29,"100kHz",1890,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-55 to 105","105°C 5000H",200,"Yes","Std","E-Cap","EEUFK1V821"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2600,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUFR1V102"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,46,"100kHz",2180,"125°C","100kHz","(空白)","dia.18",20,22,2,"-40 to 125","125°C 2000H",100,"Yes","Std","E-Cap","EEUTA1V102S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,29,"100kHz",2205,"105°C","100kHz","(空白)","dia.16",20,22,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC1V122"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2720,"105°C","100kHz","(空白)","dia.12.5",30,32,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFK1V152L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,"100kHz",3300,"105°C","100kHz","(空白)","dia.16",20,22,2,"-40 to 105","105°C10000H",100,"No","Std","E-Cap","EEUFS1V182S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"100kHz",2655,"105°C","100kHz","(空白)","dia.12.5",40,42,2,"-55 to 105","105°C 5000H",100,"Yes","NRND","E-Cap","EEUFC1V182L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2200,12,"100kHz",3750,"105°C","100kHz","(空白)","dia.12.5",35,37,2,"-40 to 105","105°C10000H",100,"No","Std","E-Cap","EEUFR1V222L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.12.5",25,27,2,"-55 to 105","105°C 2000H",200,"No","Std","E-Cap","EEUHD1V222"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,27,2,"-55 to 105","105°C 2000H",100,"No","Std","E-Cap","EEUHD1V332"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia. 4",7,8,2,"-55 to 105","105°C 1000H",200,"No","Std","E-Cap","EEAGA1H2R2"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3,1300,"100kHz",65,"105°C","100kHz","(空白)","dia. 5",11,12,2,"-55 to 105","105°C 1000H",200,"Yes","Std","E-Cap","EEUFC1H3R3"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16," 85°C","120Hz","(空白)","dia. 5",7,8,2,"-40 to  85"," 85°C 1000H",200,"No","Std","E-Cap","ECEA1HKN3R3","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,2,"-55 to 105","105°C 1000H",200,"No","Std","E-Cap","EEUHD1H4R7"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"105°C","120Hz","(空白)","dia. 5",11,12,2,"-40 to 105","105°C 1000H",200,"No","Std","E-Cap","ECA1HEN4R7","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,"105°C","120Hz","(空白)","dia. 6.3",11.2,12.2,2,"-40 to 105","105°C 1000H",200,"No","Std","E-Cap","ECA1HEN100","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",55,"105°C","120Hz","(空白)","dia. 6.3",7,8,2,"-55 to 105","105°C 1000H",200,"No","Std","E-Cap","EEAGA1H150"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",90,"105°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-40 to 105","105°C 1000H",200,"No","Std","E-Cap","ECA1HEN220","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450,"100kHz",300,"125°C","100kHz","(空白)","dia. 8",11.5,12.5,2,"-40 to 125","125°C 2000H",200,"Yes","Std","E-Cap","EEUTA1H330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","No","Std","E-Cap","ECEA1HKA330Q"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,140,"105°C","120Hz","(空白)","dia.10",12.5,13.5,2,"-40 to 105","105°C 2000H",200,"No","Std","E-Cap","ECA1HEN470","Bipolar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"135°C","100kHz",3.4,"dia. 8",9.5,10.5,2,"-55 to 145","135°C 4000H / 145°C 2000H",1000,"Yes","Std","Hybrid","EEHAZE1H680B"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1800,"105°C","100kHz",3.4,"dia. 8",9.5,10.5,2,"-55 to 105","105°C10000H",1000,"Yes","Std","Hybrid","EEHAZA1H680B"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,180,"100kHz",555,"125°C","100kHz","(空白)","dia.10",12.5,13.5,2,"-40 to 125","125°C 2000H",200,"Yes","Std","E-Cap","EEUTA1H101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,20,"100kHz",4300,"105°C","100kHz",5.8,"dia.10",13,13,2,"-55 to 125","125°C 1000H",200,"No","NRND","OS-CON","50SEK120M","→50SVPK120M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 6000H",200,"No","Std","E-Cap","EEUFR1H151"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"100kHz",1650,"105°C","100kHz","(空白)","dia.10",16,17.5,2,"-40 to 105","105°C 4000H",200,"No","Std","E-Cap","EEUFM1H221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",400," 85°C","120Hz","(空白)","dia.10",12.5,13.5,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA1HM221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63,"100kHz",1480,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC1H331"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63,"100kHz",1480,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-55 to 105","105°C 5000H",200,"Yes","Std","E-Cap","EEUFC1H391"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60,"100kHz",1610,"105°C","100kHz","(空白)","dia.10",30,32,2,"-55 to 105","105°C 3000H",100,"Yes","Std","E-Cap","EEUFC1H471L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,370,"105°C","120Hz","(空白)","dia.12.5",20,22,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUEB1H471"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105°C 7000H",100,"No","Std","E-Cap","EEUFM1H681L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,"100kHz",3160,"105°C","100kHz","(空白)","dia.12.5",30,32,2,"-40 to 105","105°C10000H",100,"No","Std","E-Cap","EEUFS1H821L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A","100kHz",1050," 85°C","120Hz","(空白)","dia.12.5",25,27,2,"-40 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA1HM102"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2200,23,"100kHz",3100,"105°C","100kHz","(空白)","dia.18",35.5,37.5,2,"-55 to 105","105°C 5000H",50,"Yes","Std","E-Cap","EEUFC1H222"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Std","E-Cap","ECA1HHG222"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,510,"100kHz",175,"105°C","100kHz","(空白)","dia. 5",11,12.5,2,"-40 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUFS1J270"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,33,25,"100kHz",2950,"105°C","100kHz",4.0999999999999996,"dia. 8",12,12,2,"-55 to 125","125°C 1000H",200,"No","NRND","OS-CON","63SXE33M","→63SXV33M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,"105°C","120Hz","(空白)","dia. 6.3",11.2,12.2,2,"-40 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUEB1J330S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2950,"105°C","100kHz",4.0999999999999996,"dia. 8",12,12,2,"-55 to 125","125°C 1000H",200,"No","NRND","OS-CON","63SXE56M","→63SXV56M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,342,"100kHz",405,"105°C","100kHz","(空白)","dia. 8",11.5,12.5,2,"-55 to 105","105°C 2000H",200,"Yes","Std","E-Cap","EEUFC1J560"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"135°C","100kHz",4,"dia.10",9.5,10.5,2,"-55 to 145","135°C 4000H / 145°C 2000H",500,"Yes","Std","Hybrid","EEHAZE1J820B"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63,"100kHz",761,"105°C","100kHz","(空白)","dia.10",12.5,14,2,"-40 to 105","105°C 6000H",200,"No","Std","E-Cap","EEUFR1J101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,194,"100kHz",600,"105°C","100kHz","(空白)","dia.10",16,17,2,"-55 to 105","105°C 3000H",200,"Yes","Std","E-Cap","EEUFC1J121"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"100kHz",1020,"105°C","100kHz","(空白)","dia.12.5",15,16,2,"-55 to 105","105°C 5000H",200,"Yes","Std","E-Cap","EEUFC1J181S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,147,"100kHz",885,"105°C","100kHz","(空白)","dia.10",20,22,2,"-55 to 105","105°C 3000H",200,"Yes","Std","E-Cap","EEUFC1J221X"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,270,33,"100kHz",1500,"105°C","100kHz","(空白)","dia.10",25,27,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUFR1J271L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,90,"100kHz",1300,"105°C","100kHz","(空白)","dia.10",30,32,2,"-55 to 105","105°C 3000H",100,"Yes","Std","E-Cap","EEUFC1J331L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,"100kHz",2090,"105°C","100kHz","(空白)","dia.12.5",30,32,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC1J471L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47,"100kHz",2265,"105°C","100kHz","(空白)","dia.12.5",35,37,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC1J681L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,43,"100kHz",2670,"105°C","100kHz","(空白)","dia.16",31.5,33.5,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC1J821"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,30,"100kHz",3095,"105°C","100kHz","(空白)","dia.18",35.5,37.5,2,"-55 to 105","105°C 5000H",50,"Yes","Std","E-Cap","EEUFC1J152"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,28,"100kHz",3100,"105°C","100kHz",5.8,"dia.10",13,13,2,"-55 to 125","125°C 1000H",200,"No","NRND","OS-CON","72SXE100M","→72SXV100M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,36,"100kHz",1700,"105°C","100kHz",4,"dia.10",9.5,10.5,2,"-55 to 105","105°C10000H",500,"Yes","Std","Hybrid","EEHAZA1K330B"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,112,"100kHz",590,"105°C","100kHz","(空白)","dia. 8",15,16.5,2,"-40 to 105","105°C 8000H",200,"No","Std","E-Cap","EEUFS1K680"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,2.2000000000000002,"N/A","100kHz",21,"105°C","120Hz","(空白)","dia. 5",11,12,2,"-55 to 105","105°C 1000H",200,"Yes","Std","E-Cap","ECA2AHG2R2"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,38,"105°C","120Hz","(空白)","dia. 5",11,12,2,"-55 to 105","105°C 1000H",200,"Yes","Std","E-Cap","ECA2AHG4R7"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,30,"100kHz",3000,"105°C","100kHz",5.8,"dia.10",13,13,2,"-55 to 125","125°C 1000H",200,"No","NRND","OS-CON","100SXE22M","→100SXV22M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,160,"100kHz",490,"105°C","100kHz","(空白)","dia. 8",11.5,13,2,"-40 to 105","105°C 6000H",200,"No","Std","E-Cap","EEUFS2A270"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56,96,"100kHz",810,"105°C","100kHz","(空白)","dia. 8",20,22,2,"-40 to 105","105°C 9000H",200,"No","Std","E-Cap","EEUFS2A560L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,265,"105°C","120Hz","(空白)","dia.10",20,22,2,"-55 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2AHG101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,44,"100kHz",1200,"105°C","100kHz","(空白)","dia.10",25,27,2,"-40 to 105","105°C10000H",200,"No","Std","E-Cap","EEUFS2A121L"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,440,"105°C","120Hz","(空白)","dia.12.5",25,27,2,"-55 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2AHG221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,"100kHz",1420,"105°C","100kHz","(空白)","dia.18",25,27,2,"-55 to 105","105°C 5000H",100,"Yes","Std","E-Cap","EEUFC2A331S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,560,41,"100kHz",1770,"105°C","100kHz","(空白)","dia.18",35.5,37.5,2,"-55 to 105","105°C 5000H",50,"Yes","Std","E-Cap","EEUFC2A561"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,700,"105°C","100kHz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 8000H",200,"No","Std","E-Cap","EEUEE2C220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,470,"105°C","100kHz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUEB2C330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.12.5",25,27,2,"-25 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUEB2C680"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,"N/A","100kHz",1060,"105°C","100kHz","(空白)","dia.18",20,22,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2C101S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,335,"105°C","120Hz","(空白)","dia.16",25,27,2,"-25 to 105","105°C 2000H",100,"Yes","Std","E-Cap","ECA2CHG101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1700,"105°C","100kHz","(空白)","dia.16",31.5,33.5,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2C221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1690,"105°C","100kHz","(空白)","dia.18",31.5,33.5,2,"-25 to 105","105°C 5000H",50,"No","NRND","E-Cap","EEUEB2C331"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100," 85°C","120Hz","(空白)","dia.10",12.5,13.5,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2DM100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,220," 85°C","120Hz","(空白)","dia.10",20,22,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2DM330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.12.5",25,27,2,"-25 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUEB2D680"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1330,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2D680S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,220,"N/A","100kHz",2000,"105°C","100kHz","(空白)","dia.18",31.5,33.5,2,"-25 to 105","105°C10000H",50,"No","NRND","E-Cap","EEUED2D221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2600,"105°C","100kHz","(空白)","dia.18",31.5,33.5,2,"-25 to 105","105°C10000H",100,"No","NRND","E-Cap","EEUEE2D221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,86," 85°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2EM4R7"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,785,"105°C","100kHz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 8000H",200,"No","Std","E-Cap","EEUEE2E220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,710,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2E470S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,"N/A","100kHz",1200,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2E101S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",31.5,33.5,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2E101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2E101S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",31.5,33.5,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2E101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2100,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2E101S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",31.5,33.5,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2E101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,530," 85°C","120Hz","(空白)","dia.16",31.5,33.5,2,"-25 to  85"," 85°C 2000H",100,"No","Std","E-Cap","ECA2EM101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,365,"105°C","120Hz","(空白)","dia.16",31.5,33.5,2,"-25 to 105","105°C 2000H",100,"Yes","Std","E-Cap","ECA2EHG101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"N/A","100kHz",1800,"105°C","100kHz","(空白)","dia.18",31.5,33.5,2,"-25 to 105","105°C10000H",50,"No","NRND","E-Cap","EEUED2E151"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1470,"105°C","100kHz","(空白)","dia.18",31.5,33.5,2,"-25 to 105","105°C 5000H",50,"No","NRND","E-Cap","EEUEB2E151"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,220,"N/A","100kHz",2100,"105°C","100kHz","(空白)","dia.18",40,42,2,"-25 to 105","105°C10000H",50,"No","NRND","E-Cap","EEUED2E221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,930," 85°C","120Hz","(空白)","dia.18",40,42,2,"-25 to  85"," 85°C 2000H",50,"No","NRND","E-Cap","ECA2EM221"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350,2.2000000000000002,"N/A","100kHz",55," 85°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2VM2R2"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,"105°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2VHG2R2"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3,"N/A","100kHz",60," 85°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2VM3R3"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,38,"105°C","120Hz","(空白)","dia.10",12.5,13.5,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2VHG3R3"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7,"N/A","100kHz",50,"105°C","120Hz","(空白)","dia.10",16,17,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2VHG4R7"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65," 85°C","120Hz","(空白)","dia.10",12.5,13.5,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2VM4R7"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"N/A","100kHz",82,"105°C","120Hz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2VHG100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,270,"105°C","100kHz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUEB2V100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350,"105°C","100kHz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 8000H",200,"No","Std","E-Cap","EEUED2V100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115," 85°C","120Hz","(空白)","dia.10",20,22,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2VM100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"N/A","100kHz",480,"105°C","100kHz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 8000H",200,"No","Std","E-Cap","EEUEE2V150"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"N/A","100kHz",660,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-25 to 105","105°C10000H",200,"No","Std","E-Cap","EEUEE2V220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,480,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-25 to 105","105°C10000H",200,"No","Std","E-Cap","EEUED2V220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-25 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUEB2V220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,130,"105°C","120Hz","(空白)","dia.12.5",20,22,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2VHG220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,195," 85°C","120Hz","(空白)","dia.12.5",20,22,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2VM220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,33,"N/A","100kHz",900,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2V330S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,480,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2V330S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300," 85°C","120Hz","(空白)","dia.16",25,27,2,"-25 to  85"," 85°C 2000H",100,"No","Std","E-Cap","ECA2VM330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,195,"105°C","120Hz","(空白)","dia.16",25,27,2,"-25 to 105","105°C 2000H",100,"Yes","Std","E-Cap","ECA2VHG330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,640,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2V330S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,790,"105°C","100kHz","(空白)","dia.12.5",25,27,2,"-25 to 105","105°C10000H",200,"No","Std","E-Cap","EEUEE2V330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47,"N/A","100kHz",800,"105°C","100kHz","(空白)","dia.18",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2V470S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2V470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,230,"105°C","120Hz","(空白)","dia.16",25,27,2,"-25 to 105","105°C 2000H",100,"Yes","Std","E-Cap","ECA2VHG470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,640,"105°C","100kHz","(空白)","dia.18",20,22,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2V470S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",25,27,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2V470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1070,"105°C","100kHz","(空白)","dia.18",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2V470S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2V470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,325," 85°C","120Hz","(空白)","dia.16",25,27,2,"-25 to  85"," 85°C 2000H",100,"No","Std","E-Cap","ECA2VM470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,"N/A","100kHz",1000,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2V680S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1100,"105°C","100kHz","(空白)","dia.16",31.5,33.5,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2V680"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1330,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2V680S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1530,"105°C","100kHz","(空白)","dia.16",31.5,33.5,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2V680"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,780,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2V680S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",31.5,33.5,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2V680"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,82,"N/A","100kHz",1100,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2V820S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1530,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2V820S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,"N/A","100kHz",1200,"105°C","100kHz","(空白)","dia.18",31.5,33.5,2,"-25 to 105","105°C10000H",50,"No","NRND","E-Cap","EEUED2V101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,535," 85°C","120Hz","(空白)","dia.18",31.5,33.5,2,"-25 to  85"," 85°C 2000H",50,"No","NRND","E-Cap","ECA2VM101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,970,"105°C","100kHz","(空白)","dia.18",31.5,33.5,2,"-25 to 105","105°C 5000H",50,"No","NRND","E-Cap","EEUEB2V101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,375,"105°C","120Hz","(空白)","dia.18",31.5,33.5,2,"-25 to 105","105°C 2000H",50,"Yes","NRND","E-Cap","ECA2VHG101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,2.2000000000000002,"N/A","100kHz",50," 85°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2GM2R2"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"105°C","120Hz","(空白)","dia. 8",11.5,12.5,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2GHG2R2"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3,"N/A","100kHz",40,"105°C","120Hz","(空白)","dia.10",12.5,13.5,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2GHG3R3"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54," 85°C","120Hz","(空白)","dia.10",12.5,13.5,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2GM3R3"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7,"N/A","100kHz",50,"105°C","120Hz","(空白)","dia.10",16,17,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2GHG4R7"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,72," 85°C","120Hz","(空白)","dia.10",16,17,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2GM4R7"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"N/A","100kHz",80,"105°C","120Hz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2GHG100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"105°C","100kHz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 8000H",200,"No","Std","E-Cap","EEUED2G100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"105°C","100kHz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUEB2G100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,430,"105°C","100kHz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 8000H",200,"No","Std","E-Cap","EEUEE2G100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115," 85°C","120Hz","(空白)","dia.10",20,22,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2GM100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"N/A","100kHz",410,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-25 to 105","105°C10000H",200,"No","Std","E-Cap","EEUED2G150"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,590,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-25 to 105","105°C10000H",200,"No","Std","E-Cap","EEUEE2G150"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"N/A","100kHz",500,"105°C","100kHz","(空白)","dia.12.5",25,27,2,"-25 to 105","105°C10000H",200,"No","Std","E-Cap","EEUED2G220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2G220S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,410,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2G220S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.12.5",25,27,2,"-25 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUEB2G220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,760,"105°C","100kHz","(空白)","dia.12.5",25,27,2,"-25 to 105","105°C10000H",200,"No","Std","E-Cap","EEUEE2G220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,860,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2G220S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,145,"105°C","120Hz","(空白)","dia.12.5",25,27,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2GHG220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,215," 85°C","120Hz","(空白)","dia.12.5",25,27,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2GM220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,33,"N/A","100kHz",1020,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2G330S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600,"105°C","100kHz","(空白)","dia.18",20,22,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2G330S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",25,27,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2G330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,195,"105°C","120Hz","(空白)","dia.16",25,27,2,"-25 to 105","105°C 2000H",100,"Yes","Std","E-Cap","ECA2GHG330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,730,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2G330S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,275," 85°C","120Hz","(空白)","dia.16",25,27,2,"-25 to  85"," 85°C 2000H",100,"No","Std","E-Cap","ECA2GM330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47,"N/A","100kHz",840,"105°C","100kHz","(空白)","dia.18",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2G470S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2G470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"105°C","120Hz","(空白)","dia.16",31.5,33.5,2,"-25 to 105","105°C 2000H",100,"Yes","Std","E-Cap","ECA2GHG470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350," 85°C","120Hz","(空白)","dia.16",31.5,33.5,2,"-25 to  85"," 85°C 2000H",100,"No","Std","E-Cap","ECA2GM470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,730,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2G470S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",31.5,33.5,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2G470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1180,"105°C","100kHz","(空白)","dia.18",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2G470S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2G470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,"N/A","100kHz",1470,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2G680"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,82,"N/A","100kHz",1645,"105°C","100kHz","(空白)","dia.18",31.5,33.5,2,"-25 to 105","105°C10000H",50,"No","NRND","E-Cap","EEUEE2G820"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,"N/A","100kHz",2060,"105°C","100kHz","(空白)","dia.18",40,42,2,"-25 to 105","105°C10000H",50,"No","NRND","E-Cap","EEUEE2G101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600," 85°C","120Hz","(空白)","dia.18",40,42,2,"-25 to  85"," 85°C 2000H",50,"No","NRND","E-Cap","ECA2GM101"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450,2.2000000000000002,"N/A","100kHz",29,"105°C","120Hz","(空白)","dia.10",12.5,13.5,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2WHG2R2"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,44," 85°C","120Hz","(空白)","dia.10",12.5,13.5,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2WM2R2"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3,"N/A","100kHz",60," 85°C","120Hz","(空白)","dia.10",16,17,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2WM3R3"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,"105°C","120Hz","(空白)","dia.10",16,17,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2WHG3R3"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7,"N/A","100kHz",79," 85°C","120Hz","(空白)","dia.10",20,22,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2WM4R7"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,49,"105°C","120Hz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2WHG4R7"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"N/A","100kHz",350,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-25 to 105","105°C10000H",200,"No","Std","E-Cap","EEUED2W100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,130," 85°C","120Hz","(空白)","dia.12.5",20,22,2,"-25 to  85"," 85°C 2000H",200,"No","Std","E-Cap","ECA2WM100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,310,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-25 to 105","105°C 5000H",200,"No","Std","E-Cap","EEUEB2W100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,330,"105°C","100kHz","(空白)","dia.10",20,22,2,"-25 to 105","105°C 8000H",200,"No","Std","E-Cap","EEUEE2W100U"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,75,"105°C","120Hz","(空白)","dia.12.5",20,22,2,"-25 to 105","105°C 2000H",200,"Yes","Std","E-Cap","ECA2WHG100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,490,"105°C","100kHz","(空白)","dia.12.5",20,22,2,"-25 to 105","105°C10000H",200,"No","Std","E-Cap","EEUEE2W100"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"N/A","100kHz",560,"105°C","100kHz","(空白)","dia.12.5",25,27,2,"-25 to 105","105°C10000H",200,"No","Std","E-Cap","EEUED2W150"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,780,"105°C","100kHz","(空白)","dia.12.5",25,27,2,"-25 to 105","105°C10000H",200,"No","Std","E-Cap","EEUEE2W150"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"N/A","100kHz",680,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2W220S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,210," 85°C","120Hz","(空白)","dia.16",25,27,2,"-25 to  85"," 85°C 2000H",100,"No","Std","E-Cap","ECA2WM220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,560,"105°C","100kHz","(空白)","dia.18",20,22,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2W220S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",25,27,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2W220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,945,"105°C","100kHz","(空白)","dia.16",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2W220S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115,"105°C","120Hz","(空白)","dia.16",25,27,2,"-25 to 105","105°C 2000H",100,"Yes","Std","E-Cap","ECA2WHG220"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,33,"N/A","100kHz",1000,"105°C","100kHz","(空白)","dia.18",20,22,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2W330S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2W330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,850,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2W330S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",31.5,33.5,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUED2W330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,680,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2W330S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",31.5,33.5,2,"-25 to 105","105°C 5000H",100,"No","Std","E-Cap","EEUEB2W330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,155,"105°C","120Hz","(空白)","dia.16",31.5,33.5,2,"-25 to 105","105°C 2000H",100,"Yes","Std","E-Cap","ECA2WHG330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,285," 85°C","120Hz","(空白)","dia.16",31.5,33.5,2,"-25 to  85"," 85°C 2000H",100,"No","Std","E-Cap","ECA2WM330"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47,"N/A","100kHz",1200,"105°C","100kHz","(空白)","dia.18",25,27,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2W470S"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dia.16",31.5,33.5,2,"-25 to 105","105°C10000H",100,"No","Std","E-Cap","EEUEE2W470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,850,"105°C","100kHz","(空白)","dia.18",31.5,33.5,2,"-25 to 105","105°C 5000H",50,"No","NRND","E-Cap","EEUEB2W470"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56,"N/A","100kHz",1380,"105°C","100kHz","(空白)","dia.18",31.5,33.5,2,"-25 to 105","105°C10000H",50,"No","NRND","E-Cap","EEUEE2W560"," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,"N/A","100kHz",1800,"105°C","100kHz","(空白)","dia.18",40,42,2,"-25 to 105","105°C10000H",50,"No","NRND","E-Cap","EEUEE2W680"," "]

{"sheet":"PN->Parameter","index":1,"n_rows":106,"n_cols":30,"rows_kept":106,"cut":false,"hidden":false,"merged":[]}
["Panasonic Polymer & Electrolytic Capacitor Quick Search"]
[]
[null,null,null,null,null,null,null,null,null,null,""]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"特殊仕様処理 (ESR/Ripple非100kHz, Terminal非2-T)"]
["e0","e1","e2","Status","#","Part Number","Voltage Cap.","ESR, Ripple","Size (mm)","Mounting","Temp Range","Endurance","Product","Series","Automotive Grade","Remarks","V","uF","ESR (mOhm)","ESR Freq.","Ripple","Ripple Freq.","LxW (mm)","Number of Terminals","H max (mm)","URL",null,"ESR Freq. Pick","Ripple Freq. Pick","Terminal Pick"]
[null,null,null,{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F7<>\"\",COUNTIF($F$7:F7,\"*\"),\"\")","v":""},null,{"$f":"\nIF(F7=\"\",\"\",CONCATENATE(Q7,\"V \",R7,\"uF\"))","v":""},{"$f":"\nIF(F7=\"\",\"\",CONCATENATE(,S7,\"mOhm\",AB7,\", \",U7,\"Arms\",AC7))","v":""},{"$f":"\nIF(F7=\"\",\"\",CONCATENATE(W7,\" x \",Y7,\" \",AD7))","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F7,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F7,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F7,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F7=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F7,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F7,'All Data'!R:R,0))),\"\")","v":""},null,{"$f":"IF(T7<>\"100kHz\",\"@\"&T7,\"\")","v":"@"},{"$f":"IF(V7<>\"100kHz\",\"@\"&V7,\"\")","v":"@"},{"$f":"IF(X7<>2,\"(\"&X7&\"-T)\",\"\")","v":"(-T)"}]
[null,null,null,{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F8<>\"\",COUNTIF($F$7:F8,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F8,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F8,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F8,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F8=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F8,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F8,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F9<>\"\",COUNTIF($F$7:F9,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F9,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F9,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F9,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F9=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F9,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F9,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F10<>\"\",COUNTIF($F$7:F10,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F10,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F10,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F10,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F10=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F10,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F10,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F11<>\"\",COUNTIF($F$7:F11,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F11,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F11,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F11,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F11=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F11,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F11,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F12<>\"\",COUNTIF($F$7:F12,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F12,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F12,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F12,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F12=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F12,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F12,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F13<>\"\",COUNTIF($F$7:F13,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F13,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F13,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F13,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F13=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F13,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F13,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F14<>\"\",COUNTIF($F$7:F14,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F14,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F14,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F14,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F14=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F14,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F14,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F15<>\"\",COUNTIF($F$7:F15,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F15,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F15,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F15,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F15=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F15,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F15,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F16<>\"\",COUNTIF($F$7:F16,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F16,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F16,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F16,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F16=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F16,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F16,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F17<>\"\",COUNTIF($F$7:F17,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F17,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F17,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F17,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F17=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F17,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F17,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F18<>\"\",COUNTIF($F$7:F18,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F18,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F18,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F18,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F18=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F18,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F18,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F19<>\"\",COUNTIF($F$7:F19,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F19,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F19,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F19,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F19=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F19,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F19,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F20<>\"\",COUNTIF($F$7:F20,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F20,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F20,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F20,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F20=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F20,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F20,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F21<>\"\",COUNTIF($F$7:F21,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F21,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F21,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F21,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F21=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F21,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F21,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F22<>\"\",COUNTIF($F$7:F22,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F22,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F22,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F22,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F22=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F22,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F22,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F23<>\"\",COUNTIF($F$7:F23,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F23,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F23,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F23,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F23=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F23,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F23,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F24<>\"\",COUNTIF($F$7:F24,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F24,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F24,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F24,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F24=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F24,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F24,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F25<>\"\",COUNTIF($F$7:F25,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F25,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F25,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F25,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F25=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F25,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F25,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F26<>\"\",COUNTIF($F$7:F26,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F26,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F26,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F26,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F26=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F26,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F26,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F27<>\"\",COUNTIF($F$7:F27,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F27,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F27,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F27,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F27=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F27,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F27,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F28<>\"\",COUNTIF($F$7:F28,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F28,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F28,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F28,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F28=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F28,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F28,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F29<>\"\",COUNTIF($F$7:F29,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F29,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F29,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F29,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F29=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F29,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F29,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F30<>\"\",COUNTIF($F$7:F30,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F30,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F30,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F30,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F30=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F30,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F30,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F31<>\"\",COUNTIF($F$7:F31,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F31,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F31,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F31,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F31=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F31,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F31,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F32<>\"\",COUNTIF($F$7:F32,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F32,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F32,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F32,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F32=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F32,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F32,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F33<>\"\",COUNTIF($F$7:F33,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F33,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F33,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F33,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F33=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F33,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F33,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F34<>\"\",COUNTIF($F$7:F34,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F34,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F34,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F34,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F34=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F34,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F34,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F35<>\"\",COUNTIF($F$7:F35,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F35,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F35,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F35,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F35=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F35,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F35,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F36<>\"\",COUNTIF($F$7:F36,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F36,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F36,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F36,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F36=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F36,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F36,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F37<>\"\",COUNTIF($F$7:F37,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F37,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F37,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F37,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F37=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F37,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F37,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F38<>\"\",COUNTIF($F$7:F38,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F38,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F38,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F38,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F38=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F38,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F38,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F39<>\"\",COUNTIF($F$7:F39,\"*\"),\"\")","v":""},null,{"$f":"\nIF(F39=\"\",\"\",CONCATENATE(Q39,\"V \",R39,\"uF\"))","v":""},{"$f":"\nIF(F39=\"\",\"\",CONCATENATE(,S39,\"mOhm\",AB39,\", \",U39,\"Arms\",AC39))","v":""},{"$f":"\nIF(F39=\"\",\"\",CONCATENATE(W39,\" x \",Y39,\" \",AD39))","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F39,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F39,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F39,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F39=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F39,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F39,'All Data'!R:R,0))),\"\")","v":""},null,{"$f":"IF(T39<>\"100kHz\",\"@\"&T39,\"\")","v":"@"},{"$f":"IF(V39<>\"100kHz\",\"@\"&V39,\"\")","v":"@"},{"$f":"IF(X39<>2,\"(\"&X39&\"-T)\",\"\")","v":"(-T)"}]
[null,null,null,{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F40<>\"\",COUNTIF($F$7:F40,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F40,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F40,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F40,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F40=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F40,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F40,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F41<>\"\",COUNTIF($F$7:F41,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F41,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F41,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F41,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F41=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F41,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F41,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F42<>\"\",COUNTIF($F$7:F42,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F42,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F42,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F42,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F42=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F42,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F42,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F43<>\"\",COUNTIF($F$7:F43,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F43,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F43,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F43,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F43=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F43,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F43,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F44<>\"\",COUNTIF($F$7:F44,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F44,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F44,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F44,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F44=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F44,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F44,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F45<>\"\",COUNTIF($F$7:F45,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F45,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F45,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F45,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F45=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F45,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F45,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F46<>\"\",COUNTIF($F$7:F46,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F46,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F46,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F46,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F46=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F46,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F46,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F47<>\"\",COUNTIF($F$7:F47,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F47,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F47,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F47,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F47=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F47,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F47,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F48<>\"\",COUNTIF($F$7:F48,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F48,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F48,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F48,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F48=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F48,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F48,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F49<>\"\",COUNTIF($F$7:F49,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F49,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F49,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F49,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F49=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F49,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F49,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F50<>\"\",COUNTIF($F$7:F50,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F50,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F50,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F50,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F50=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F50,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F50,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F51<>\"\",COUNTIF($F$7:F51,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F51,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F51,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F51,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F51=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F51,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F51,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F52<>\"\",COUNTIF($F$7:F52,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F52,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F52,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F52,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F52=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F52,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F52,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F53<>\"\",COUNTIF($F$7:F53,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F53,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F53,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F53,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F53=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F53,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F53,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F54<>\"\",COUNTIF($F$7:F54,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F54,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F54,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F54,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F54=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F54,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F54,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F55<>\"\",COUNTIF($F$7:F55,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F55,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F55,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F55,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F55=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F55,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F55,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F56<>\"\",COUNTIF($F$7:F56,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F56,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F56,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F56,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F56=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F56,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F56,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F57<>\"\",COUNTIF($F$7:F57,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F57,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F57,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F57,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F57=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F57,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F57,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F58<>\"\",COUNTIF($F$7:F58,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F58,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F58,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F58,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F58=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F58,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F58,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F59<>\"\",COUNTIF($F$7:F59,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F59,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F59,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F59,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F59=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F59,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F59,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F60<>\"\",COUNTIF($F$7:F60,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F60,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F60,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F60,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F60=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F60,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F60,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F61<>\"\",COUNTIF($F$7:F61,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F61,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F61,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F61,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F61=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F61,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F61,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F62<>\"\",COUNTIF($F$7:F62,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F62,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F62,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F62,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F62=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F62,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F62,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F63<>\"\",COUNTIF($F$7:F63,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F63,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F63,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F63,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F63=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F63,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F63,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F64<>\"\",COUNTIF($F$7:F64,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F64,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F64,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F64,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F64=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F64,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F64,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F65<>\"\",COUNTIF($F$7:F65,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F65,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F65,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F65,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F65=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F65,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F65,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F66<>\"\",COUNTIF($F$7:F66,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F66,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F66,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F66,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F66=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F66,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F66,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F67<>\"\",COUNTIF($F$7:F67,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F67,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F67,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F67,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F67=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F67,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F67,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F68<>\"\",COUNTIF($F$7:F68,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F68,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F68,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F68,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F68=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F68,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F68,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F69<>\"\",COUNTIF($F$7:F69,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F69,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F69,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F69,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F69=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F69,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F69,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F70<>\"\",COUNTIF($F$7:F70,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F70,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F70,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F70,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F70=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F70,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F70,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F71<>\"\",COUNTIF($F$7:F71,\"*\"),\"\")","v":""},null,{"$f":"\nIF(F71=\"\",\"\",CONCATENATE(Q71,\"V \",R71,\"uF\"))","v":""},{"$f":"\nIF(F71=\"\",\"\",CONCATENATE(,S71,\"mOhm\",AB71,\", \",U71,\"Arms\",AC71))","v":""},{"$f":"\nIF(F71=\"\",\"\",CONCATENATE(W71,\" x \",Y71,\" \",AD71))","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F71,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F71,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F71,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F71=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F71,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F71,'All Data'!R:R,0))),\"\")","v":""},null,{"$f":"IF(T71<>\"100kHz\",\"@\"&T71,\"\")","v":"@"},{"$f":"IF(V71<>\"100kHz\",\"@\"&V71,\"\")","v":"@"},{"$f":"IF(X71<>2,\"(\"&X71&\"-T)\",\"\")","v":"(-T)"}]
[null,null,null,{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F72<>\"\",COUNTIF($F$7:F72,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F72,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F72,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F72,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F72=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F72,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F72,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F73<>\"\",COUNTIF($F$7:F73,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F73,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F73,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F73,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F73=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F73,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F73,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F74<>\"\",COUNTIF($F$7:F74,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F74,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F74,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F74,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F74=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F74,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F74,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F75<>\"\",COUNTIF($F$7:F75,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F75,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F75,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F75,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F75=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F75,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F75,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F76<>\"\",COUNTIF($F$7:F76,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F76,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F76,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F76,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F76=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F76,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F76,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F77<>\"\",COUNTIF($F$7:F77,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F77,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F77,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F77,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F77=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F77,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F77,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F78<>\"\",COUNTIF($F$7:F78,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F78,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F78,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F78,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F78=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F78,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F78,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F79<>\"\",COUNTIF($F$7:F79,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F79,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F79,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F79,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F79=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F79,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F79,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F80<>\"\",COUNTIF($F$7:F80,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F80,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F80,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F80,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F80=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F80,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F80,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F81<>\"\",COUNTIF($F$7:F81,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F81,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F81,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F81,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F81=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F81,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F81,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F82<>\"\",COUNTIF($F$7:F82,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F82,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F82,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F82,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F82=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F82,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F82,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F83<>\"\",COUNTIF($F$7:F83,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F83,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F83,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F83,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F83=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F83,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F83,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F84<>\"\",COUNTIF($F$7:F84,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F84,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F84,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F84,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F84=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F84,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F84,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F85<>\"\",COUNTIF($F$7:F85,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F85,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F85,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F85,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F85=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F85,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F85,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F86<>\"\",COUNTIF($F$7:F86,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F86,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F86,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F86,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F86=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F86,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F86,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F87<>\"\",COUNTIF($F$7:F87,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F87,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F87,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F87,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F87=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F87,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F87,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F88<>\"\",COUNTIF($F$7:F88,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F88,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F88,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F88,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F88=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F88,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F88,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F89<>\"\",COUNTIF($F$7:F89,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F89,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F89,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F89,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F89=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F89,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F89,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F90<>\"\",COUNTIF($F$7:F90,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F90,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F90,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F90,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F90=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F90,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F90,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F91<>\"\",COUNTIF($F$7:F91,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F91,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F91,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F91,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F91=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F91,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F91,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F92<>\"\",COUNTIF($F$7:F92,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F92,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F92,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F92,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F92=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F92,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F92,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F93<>\"\",COUNTIF($F$7:F93,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F93,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F93,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F93,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F93=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F93,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F93,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F94<>\"\",COUNTIF($F$7:F94,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F94,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F94,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F94,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F94=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F94,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F94,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F95<>\"\",COUNTIF($F$7:F95,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F95,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F95,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F95,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F95=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F95,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F95,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F96<>\"\",COUNTIF($F$7:F96,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F96,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F96,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F96,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F96=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F96,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F96,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F97<>\"\",COUNTIF($F$7:F97,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F97,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F97,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F97,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F97=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F97,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F97,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F98<>\"\",COUNTIF($F$7:F98,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F98,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F98,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F98,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F98=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F98,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F98,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F99<>\"\",COUNTIF($F$7:F99,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F99,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F99,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F99,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F99=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F99,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F99,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F100<>\"\",COUNTIF($F$7:F100,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F100,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F100,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F100,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F100=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F100,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F100,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F101<>\"\",COUNTIF($F$7:F101,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F101,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F101,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F101,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F101=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F101,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F101,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F102<>\"\",COUNTIF($F$7:F102,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F102,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F102,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F102,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F102=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F102,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F102,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F103<>\"\",COUNTIF($F$7:F103,\"*\"),\"\")","v":""},null,{"$f":"\nIF(F103=\"\",\"\",CONCATENATE(Q103,\"V \",R103,\"uF\"))","v":""},"","",{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F103,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F103,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F103,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F103=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F103,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F103,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F104<>\"\",COUNTIF($F$7:F104,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F104,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F104,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F104,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F104=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F104,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F104,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F105<>\"\",COUNTIF($F$7:F105,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F105,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F105,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F105,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F105=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F105,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F105,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]
[null,null,null,{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F106<>\"\",COUNTIF($F$7:F106,\"*\"),\"\")","v":""},null,"","","",{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$AC:$AC,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$L:$L,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$M:$M,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$AQ:$AQ,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AG:$AG,MATCH(F106,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AZ:$AZ,MATCH(F106,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(INDEX('All Data'!$AF:$AF,MATCH(F106,'All Data'!$R:$R,0)),\"\")","v":""},{"$f":"\nIF(F106=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(F106,'All Data'!$R:$R,0)))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX('All Data'!AX:AX,MATCH(F106,'All Data'!R:R,0))),\"\")","v":""},null,"@","@","(-T)"]

{"sheet":"Disclaimer","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"All Data","index":3,"n_rows":4782,"n_cols":102,"rows_kept":1125,"cut":true,"hidden":true,"merged":[[8,68,8,70]],"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
[]
[]
[]
[]
[]
[]
[]
[]
["add","add","ref",null,null,"ref",null,null,"ref","add","add","add","ref",null,null,null,null,"ref","ref",null,null,"ref","ref","ref","ref","ref","ref","ref","ref","ref",null,"ref","ref/add","add","add","ref","ref","ref",null,null,null,null,null,"Deleted","Deleted","Deleted","Deleted","Deleted","Deleted",null,null,"Add for poly",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!*2","v":{"$error":"#REF!"}},{"$f":"#REF!*2","v":{"$error":"#REF!"}},{"$f":"#REF!*2","v":{"$error":"#REF!"}},{"$f":"#REF!*2","v":{"$error":"#REF!"}}]
["Jump","Maker","Max Height (mm)",null,"Cross PN Result","Status","Maker","Country","Type","Shape","Category","Product","Series","Automotive Grade","V (group)","C (group)","H (rough)","Part Number","Size (mm)","Height (mm)","H Tolerance (mm)","Max Height (mm)","Voltage (V)","Cap. (uF)","ESR (mOhm)","Ripple Current (mArms)","Ripple Temp.","ref ESL (nH)","Temp Range (deg.C)","Endurance","Endurance (with Category V)","Number of Terminals","ESR Freq.","ESL Freq.","Ripple Current (Arms)","DF","LC (uA)","MPQ (pcs)","Substitute","Size Code","T lower (deg.C)","T upper (deg.C)","Remarks","列10","列11","列12","列13","列14","列15","PN URL","IM URL","Ripple Freq.","列0","列142","列2","列3","列4","列5","列6","列7","列8","列9","列112"]
["P SP","Panasonic",null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 180","≤ 2","EEFSX0D181ER","7.3x4.3(D)",1.9,null,2,2,180,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,36,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D181ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SR","No","≤  2","≤ 220","≤ 1","EEFSR0D221R4","7.3x4.3(D)",1,null,1,2,220,4.5,8500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",8.5,0.06,44,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSR0D221R4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LR","No","≤  2","≤ 220","≤ 1","EEFLR0D221R4","7.3x4.3(D)",1,null,1,2,220,4.5,8500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",8.5,0.06,44,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLR0D221R4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SR","No","≤  2","≤ 220","≤ 1","EEFSR0D221R","7.3x4.3(D)",1,null,1,2,220,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,44,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSR0D221R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SS","No","≤  2","≤ 220","≤ 1.5","EEFSS0D221R","7.3x4.3(D)",1.1000000000000001,null,1.2,2,220,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,44,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSS0D221R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LR","No","≤  2","≤ 220","≤ 1","EEFLR0D221R","7.3x4.3(D)",1,null,1,2,220,6,7500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",7.5,0.06,44,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLR0D221R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LS","No","≤  2","≤ 220","≤ 1.5","EEFLS0D221R","7.3x4.3(D)",1.1000000000000001,null,1.2,2,220,6,7500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",7.5,0.06,44,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLS0D221R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 220","≤ 2","EEFSX0D221ER","7.3x4.3(D)",1.9,null,2,2,220,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,44,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D221ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  2","≤ 220","≤ 2","EEFCX0D221R","7.3x4.3(D)",1.9,null,2,2,220,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,44,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D221R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 270","≤ 2","EEFSX0D271E4","7.3x4.3(D)",1.9,null,2,2,270,4.5,8500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",8.5,0.06,54,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D271E4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 270","≤ 2","EEFSX0D271XE","7.3x4.3(D)",1.9,null,2,2,270,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,54,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D271XE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 270","≤ 2","EEFSX0D271ER","7.3x4.3(D)",1.9,null,2,2,270,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,54,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D271ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  2","≤ 270","≤ 2","EEFCX0D271XR","7.3x4.3(D)",1.9,null,2,2,270,12,5600,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.6,0.06,54,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D271XR","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","GX","No","≤  2","≤ 330","≤ 2","EEFGX0D331R","7.3x4.3(D)",1.9,null,2,2,330,3,10200,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",10.199999999999999,0.06,66,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0D331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 330","≤ 2","EEFSX0D331E4","7.3x4.3(D)",1.9,null,2,2,330,4.5,8500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",8.5,0.06,66,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D331E4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LX","No","≤  2","≤ 330","≤ 2","EEFLX0D331R4","7.3x4.3(D)",1.9,null,2,2,330,4.5,8500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",8.5,0.06,66,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0D331R4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","ST","No","≤  2","≤ 330","≤ 1.5","EEFST0D331R","7.3x4.3(D)",1.4,null,1.5,2,330,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,66,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFST0D331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 330","≤ 2","EEFSX0D331XE","7.3x4.3(D)",1.9,null,2,2,330,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,66,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D331XE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LT","No","≤  2","≤ 330","≤ 1.5","EEFLT0D331R","7.3x4.3(D)",1.4,null,1.5,2,330,6,7500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",7.5,0.06,66,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLT0D331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LX","No","≤  2","≤ 330","≤ 2","EEFLX0D331R","7.3x4.3(D)",1.9,null,2,2,330,6,7500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",7.5,0.06,66,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0D331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 330","≤ 2","EEFSX0D331ER","7.3x4.3(D)",1.9,null,2,2,330,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,66,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D331ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2","≤ 330","≤ 2","EEFJX0D331RE","7.3x4.3(D)",1.9,null,2,2,330,9,6300,"45°C",1.2,"-55 to 125","125°C 3000H(1.6V)","125°C 3000H(1.6V)",2,"100kHz","500MHz",6.3,0.1,66,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0D331RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2","≤ 330","≤ 2","EEFKX0D331RE","7.3x4.3(D)",1.9,null,2,2,330,9,6300,"45°C",1.2,"-55 to 125","125°C 5500H(1.6V)","125°C 5500H(1.6V)",2,"100kHz","500MHz",6.3,0.1,66,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0D331RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  2","≤ 330","≤ 2","EEFTX0D331RE","7.3x4.3(D)",1.9,null,2,2,330,9,6300,"45°C",1.2,"-55 to 135","135°C 5500H(1.6V)","135°C 5500H(1.6V)",2,"100kHz","500MHz",6.3,0.1,66,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0D331RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  2","≤ 330","≤ 2","EEFCX0D331XR","7.3x4.3(D)",1.9,null,2,2,330,12,5600,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.6,0.06,66,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D331XR","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  2","≤ 330","≤ 2","EEFCX0D331R","7.3x4.3(D)",1.9,null,2,2,330,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,66,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 390","≤ 2","EEFSX0D391E4","7.3x4.3(D)",1.9,null,2,2,390,4.5,8500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",8.5,0.06,78,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D391E4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 390","≤ 2","EEFSX0D391XE","7.3x4.3(D)",1.9,null,2,2,390,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,78,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D391XE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 390","≤ 2","EEFSX0D391ER","7.3x4.3(D)",1.9,null,2,2,390,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,78,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D391ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  2","≤ 390","≤ 2","EEFCX0D391R","7.3x4.3(D)",1.9,null,2,2,390,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,78,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D391R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","GX","No","≤  2","≤ 470","≤ 2","EEFGX0D471R","7.3x4.3(D)",1.9,null,2,2,470,3,10200,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",10.199999999999999,0.06,94,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0D471R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2","≤ 470","≤ 2","EEFJX0D471RB","7.3x4.3(D)",1.9,null,2,2,470,3,10200,"45°C",1.2,"-55 to 125","125°C 3000H(1.6V)","125°C 3000H(1.6V)",2,"100kHz","500MHz",10.199999999999999,0.1,94,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0D471RB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2","≤ 470","≤ 2","EEFKX0D471RB","7.3x4.3(D)",1.9,null,2,2,470,3,10200,"45°C",1.2,"-55 to 125","125°C 5500H(1.6V)","125°C 5500H(1.6V)",2,"100kHz","500MHz",10.199999999999999,0.1,94,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0D471RB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  2","≤ 470","≤ 2","EEFTX0D471RB","7.3x4.3(D)",1.9,null,2,2,470,3,10200,"45°C",1.2,"-55 to 135","135°C 5500H(1.6V)","135°C 5500H(1.6V)",2,"100kHz","500MHz",10.199999999999999,0.1,94,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0D471RB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","GX","No","≤  2","≤ 470","≤ 2","EEFGX0D471L","7.3x4.3(D)",1.9,null,2,2,470,3,10200,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",10.199999999999999,0.06,94,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0D471L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 470","≤ 2","EEFSX0D471E4","7.3x4.3(D)",1.9,null,2,2,470,4.5,8500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",8.5,0.06,94,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D471E4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","HX","No","≤  2","≤ 470","≤ 2","EEFHX0D471R4","7.3x4.3(D)",1.9,null,2,2,470,4.5,8500,"45°C",1.2,"-55 to 125","125°C 1000H(1.6V)","125°C 1000H(1.6V)",2,"100kHz","500MHz",8.5,0.1,94,3500,0,"D",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFHX0D471R4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2","≤ 470","≤ 2","EEFJX0D471RC","7.3x4.3(D)",1.9,null,2,2,470,4.5,8500,"45°C",1.2,"-55 to 125","125°C 3000H(1.6V)","125°C 3000H(1.6V)",2,"100kHz","500MHz",8.5,0.1,94,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0D471RC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2","≤ 470","≤ 2","EEFKX0D471RC","7.3x4.3(D)",1.9,null,2,2,470,4.5,8500,"45°C",1.2,"-55 to 125","125°C 5500H(1.6V)","125°C 5500H(1.6V)",2,"100kHz","500MHz",8.5,0.1,94,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0D471RC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  2","≤ 470","≤ 2","EEFTX0D471RC","7.3x4.3(D)",1.9,null,2,2,470,4.5,8500,"45°C",1.2,"-55 to 135","135°C 5500H(1.6V)","135°C 5500H(1.6V)",2,"100kHz","500MHz",8.5,0.1,94,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0D471RC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LX","No","≤  2","≤ 470","≤ 2","EEFLX0D471R4","7.3x4.3(D)",1.9,null,2,2,470,4.5,8500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",8.5,0.06,94,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0D471R4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 470","≤ 2","EEFSX0D471XE","7.3x4.3(D)",1.9,null,2,2,470,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,94,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D471XE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","HX","No","≤  2","≤ 470","≤ 2","EEFHX0D471R6","7.3x4.3(D)",1.9,null,2,2,470,6,7500,"45°C",1.2,"-55 to 125","125°C 1000H(1.6V)","125°C 1000H(1.6V)",2,"100kHz","500MHz",7.5,0.1,94,3500,0,"D",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFHX0D471R6","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LX","No","≤  2","≤ 470","≤ 2","EEFLX0D471R","7.3x4.3(D)",1.9,null,2,2,470,6,7500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",7.5,0.06,94,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0D471R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 470","≤ 2","EEFSX0D471ER","7.3x4.3(D)",1.9,null,2,2,470,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,94,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D471ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","HX","No","≤  2","≤ 470","≤ 2","EEFHX0D471R9","7.3x4.3(D)",1.9,null,2,2,470,9,6300,"45°C",1.2,"-55 to 125","125°C 1000H(1.6V)","125°C 1000H(1.6V)",2,"100kHz","500MHz",6.3,0.1,94,3500,0,"D",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFHX0D471R9","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2","≤ 470","≤ 2","EEFJX0D471RE","7.3x4.3(D)",1.9,null,2,2,470,9,6300,"45°C",1.2,"-55 to 125","125°C 3000H(1.6V)","125°C 3000H(1.6V)",2,"100kHz","500MHz",6.3,0.1,94,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0D471RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2","≤ 470","≤ 2","EEFKX0D471RE","7.3x4.3(D)",1.9,null,2,2,470,9,6300,"45°C",1.2,"-55 to 125","125°C 5500H(1.6V)","125°C 5500H(1.6V)",2,"100kHz","500MHz",6.3,0.1,94,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0D471RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  2","≤ 470","≤ 2","EEFTX0D471RE","7.3x4.3(D)",1.9,null,2,2,470,9,6300,"45°C",1.2,"-55 to 135","135°C 5500H(1.6V)","135°C 5500H(1.6V)",2,"100kHz","500MHz",6.3,0.1,94,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0D471RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  2","≤ 470","≤ 2","EEFCX0D471R","7.3x4.3(D)",1.9,null,2,2,470,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,94,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D471R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","HX","No","≤  2","≤ 470","≤ 2","EEFHX0D471R","7.3x4.3(D)",1.9,null,2,2,470,15,5100,"45°C",1.2,"-55 to 125","125°C 1000H(1.6V)","125°C 1000H(1.6V)",2,"100kHz","500MHz",5.0999999999999996,0.1,94,3500,0,"D",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFHX0D471R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","GX","No","≤  2","≤ 560","≤ 2","EEFGX0D561R","7.3x4.3(D)",1.9,null,2,2,560,3,10200,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",10.199999999999999,0.06,112,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0D561R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JZ","No","≤  2","≤ 560","≤ 2.5","EEFJZ0D561RB","7.3x4.3(D)",2.2000000000000002,null,2.2999999999999998,2,560,3,10200,"45°C",1.2,"-55 to 125","125°C 3000H(1.6V)","125°C 3000H(1.6V)",2,"100kHz","500MHz",10.199999999999999,0.1,112,3000,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJZ0D561RB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KZ","No","≤  2","≤ 560","≤ 2.5","EEFKZ0D561RB","7.3x4.3(D)",2.2000000000000002,null,2.2999999999999998,2,560,3,10200,"45°C",1.2,"-55 to 125","125°C 5500H(1.6V)","125°C 5500H(1.6V)",2,"100kHz","500MHz",10.199999999999999,0.1,112,3000,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKZ0D561RB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TZ","No","≤  2","≤ 560","≤ 2.5","EEFTZ0D561RB","7.3x4.3(D)",2.2000000000000002,null,2.2999999999999998,2,560,3,10200,"45°C",1.2,"-55 to 135","135°C 5500H(1.6V)","135°C 5500H(1.6V)",2,"100kHz","500MHz",10.199999999999999,0.1,112,3000,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTZ0D561RB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","GX","No","≤  2","≤ 560","≤ 2","EEFGX0D561L","7.3x4.3(D)",1.9,null,2,2,560,3,10200,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",10.199999999999999,0.06,112,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0D561L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2","≤ 560","≤ 2","EEFSX0D561E4","7.3x4.3(D)",1.9,null,2,2,560,4.5,8500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",8.5,0.06,112,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0D561E4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JZ","No","≤  2","≤ 560","≤ 2.5","EEFJZ0D561RC","7.3x4.3(D)",2.2000000000000002,null,2.2999999999999998,2,560,4.5,8500,"45°C",1.2,"-55 to 125","125°C 3000H(1.6V)","125°C 3000H(1.6V)",2,"100kHz","500MHz",8.5,0.1,112,3000,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJZ0D561RC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KZ","No","≤  2","≤ 560","≤ 2.5","EEFKZ0D561RC","7.3x4.3(D)",2.2000000000000002,null,2.2999999999999998,2,560,4.5,8500,"45°C",1.2,"-55 to 125","125°C 5500H(1.6V)","125°C 5500H(1.6V)",2,"100kHz","500MHz",8.5,0.1,112,3000,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKZ0D561RC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TZ","No","≤  2","≤ 560","≤ 2.5","EEFTZ0D561RC","7.3x4.3(D)",2.2000000000000002,null,2.2999999999999998,2,560,4.5,8500,"45°C",1.2,"-55 to 135","135°C 5500H(1.6V)","135°C 5500H(1.6V)",2,"100kHz","500MHz",8.5,0.1,112,3000,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTZ0D561RC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LX","No","≤  2","≤ 560","≤ 2","EEFLX0D561R4","7.3x4.3(D)",1.9,null,2,2,560,4.5,8500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",8.5,0.06,112,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0D561R4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LX","No","≤  2","≤ 560","≤ 2","EEFLX0D561R","7.3x4.3(D)",1.9,null,2,2,560,6,7500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",7.5,0.06,112,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0D561R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JZ","No","≤  2","≤ 560","≤ 2.5","EEFJZ0D561RE","7.3x4.3(D)",2.2000000000000002,null,2.2999999999999998,2,560,9,6300,"45°C",1.2,"-55 to 125","125°C 3000H(1.6V)","125°C 3000H(1.6V)",2,"100kHz","500MHz",6.3,0.1,112,3000,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJZ0D561RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KZ","No","≤  2","≤ 560","≤ 2.5","EEFKZ0D561RE","7.3x4.3(D)",2.2000000000000002,null,2.2999999999999998,2,560,9,6300,"45°C",1.2,"-55 to 125","125°C 5500H(1.6V)","125°C 5500H(1.6V)",2,"100kHz","500MHz",6.3,0.1,112,3000,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKZ0D561RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TZ","No","≤  2","≤ 560","≤ 2.5","EEFTZ0D561RE","7.3x4.3(D)",2.2000000000000002,null,2.2999999999999998,2,560,9,6300,"45°C",1.2,"-55 to 135","135°C 5500H(1.6V)","135°C 5500H(1.6V)",2,"100kHz","500MHz",6.3,0.1,112,3000,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTZ0D561RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  2","≤ 560","≤ 2","EEFCX0D561R","7.3x4.3(D)",1.9,null,2,2,560,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,112,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0D561R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","GY","No","≤  2","≤ 820","≤ 3","EEFGY0D821R","7.3x4.3(D)",2.8,null,3,2,820,3,10200,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",10.199999999999999,0.06,164,2000,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGY0D821R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 150","≤ 2","EEFSX0E151ER","7.3x4.3(D)",1.9,null,2,2.5,150,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,37.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E151ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SR","No","≤  2.5","≤ 180","≤ 1","EEFSR0E181R4","7.3x4.3(D)",1,null,1,2.5,180,4.5,8500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",8.5,0.06,45,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSR0E181R4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LR","No","≤  2.5","≤ 180","≤ 1","EEFLR0E181R4","7.3x4.3(D)",1,null,1,2.5,180,4.5,8500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",8.5,0.06,45,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLR0E181R4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SR","No","≤  2.5","≤ 180","≤ 1","EEFSR0E181R","7.3x4.3(D)",1,null,1,2.5,180,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,45,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSR0E181R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SS","No","≤  2.5","≤ 180","≤ 1.5","EEFSS0E181R","7.3x4.3(D)",1.1000000000000001,null,1.2,2.5,180,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,45,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSS0E181R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LR","No","≤  2.5","≤ 180","≤ 1","EEFLR0E181R","7.3x4.3(D)",1,null,1,2.5,180,6,7500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",7.5,0.06,45,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLR0E181R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LS","No","≤  2.5","≤ 180","≤ 1.5","EEFLS0E181R","7.3x4.3(D)",1.1000000000000001,null,1.2,2.5,180,6,7500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",7.5,0.06,45,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLS0E181R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 180","≤ 2","EEFSX0E181ER","7.3x4.3(D)",1.9,null,2,2.5,180,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,45,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E181ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 220","≤ 2","EEFSX0E221E7","7.3x4.3(D)",1.9,null,2,2.5,220,7,7000,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7,0.06,55,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E221E7","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 220","≤ 2","EEFSX0E221ER","7.3x4.3(D)",1.9,null,2,2.5,220,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,55,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E221ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2.5","≤ 220","≤ 2","EEFJX0E221RE","7.3x4.3(D)",1.9,null,2,2.5,220,9,6300,"45°C",1.2,"-55 to 125","125°C 3000H(2V)","125°C 3000H(2V)",2,"100kHz","500MHz",6.3,0.1,55,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0E221RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2.5","≤ 220","≤ 2","EEFKX0E221RE","7.3x4.3(D)",1.9,null,2,2.5,220,9,6300,"45°C",1.2,"-55 to 125","125°C 5500H(2V)","125°C 5500H(2V)",2,"100kHz","500MHz",6.3,0.1,55,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0E221RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  2.5","≤ 220","≤ 2","EEFTX0E221RE","7.3x4.3(D)",1.9,null,2,2.5,220,9,6300,"45°C",1.2,"-55 to 135","135°C 5500H(2V)","135°C 5500H(2V)",2,"100kHz","500MHz",6.3,0.1,55,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0E221RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  2.5","≤ 220","≤ 2","EEFCX0E221R","7.3x4.3(D)",1.9,null,2,2.5,220,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,55,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0E221R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","ST","No","≤  2.5","≤ 270","≤ 1.5","EEFST0E271R","7.3x4.3(D)",1.4,null,1.5,2.5,270,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,67.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFST0E271R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LT","No","≤  2.5","≤ 270","≤ 1.5","EEFLT0E271R","7.3x4.3(D)",1.4,null,1.5,2.5,270,6,7500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",7.5,0.06,67.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLT0E271R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 270","≤ 2","EEFSX0E271E7","7.3x4.3(D)",1.9,null,2,2.5,270,7,7000,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7,0.06,67.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E271E7","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","GX","No","≤  2.5","≤ 330","≤ 2","EEFGX0E331R","7.3x4.3(D)",1.9,null,2,2.5,330,3,10200,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",10.199999999999999,0.06,82.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0E331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 330","≤ 2","EEFSX0E331E4","7.3x4.3(D)",1.9,null,2,2.5,330,4.5,8500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",8.5,0.06,82.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E331E4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","HX","No","≤  2.5","≤ 330","≤ 2","EEFHX0E331R4","7.3x4.3(D)",1.9,null,2,2.5,330,4.5,8500,"45°C",1.2,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","500MHz",8.5,0.1,82.5,3500,0,"D",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFHX0E331R4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LX","No","≤  2.5","≤ 330","≤ 2","EEFLX0E331R4","7.3x4.3(D)",1.9,null,2,2.5,330,4.5,8500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",8.5,0.06,82.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0E331R4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 330","≤ 2","EEFSX0E331XE","7.3x4.3(D)",1.9,null,2,2.5,330,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,82.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E331XE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","HX","No","≤  2.5","≤ 330","≤ 2","EEFHX0E331R6","7.3x4.3(D)",1.9,null,2,2.5,330,6,7500,"45°C",1.2,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","500MHz",7.5,0.1,82.5,3500,0,"D",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFHX0E331R6","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LX","No","≤  2.5","≤ 330","≤ 2","EEFLX0E331R","7.3x4.3(D)",1.9,null,2,2.5,330,6,7500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",7.5,0.06,82.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0E331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 330","≤ 2","EEFSX0E331ER","7.3x4.3(D)",1.9,null,2,2.5,330,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,82.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E331ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","HX","No","≤  2.5","≤ 330","≤ 2","EEFHX0E331R9","7.3x4.3(D)",1.9,null,2,2.5,330,9,6300,"45°C",1.2,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","500MHz",6.3,0.1,82.5,3500,0,"D",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFHX0E331R9","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2.5","≤ 330","≤ 2","EEFJX0E331RE","7.3x4.3(D)",1.9,null,2,2.5,330,9,6300,"45°C",1.2,"-55 to 125","125°C 3000H(2V)","125°C 3000H(2V)",2,"100kHz","500MHz",6.3,0.1,82.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0E331RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2.5","≤ 330","≤ 2","EEFKX0E331RE","7.3x4.3(D)",1.9,null,2,2.5,330,9,6300,"45°C",1.2,"-55 to 125","125°C 5500H(2V)","125°C 5500H(2V)",2,"100kHz","500MHz",6.3,0.1,82.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0E331RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  2.5","≤ 330","≤ 2","EEFTX0E331RE","7.3x4.3(D)",1.9,null,2,2.5,330,9,6300,"45°C",1.2,"-55 to 135","135°C 5500H(2V)","135°C 5500H(2V)",2,"100kHz","500MHz",6.3,0.1,82.5,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0E331RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  2.5","≤ 330","≤ 2","EEFCX0E331R","7.3x4.3(D)",1.9,null,2,2.5,330,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,82.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0E331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","HX","No","≤  2.5","≤ 330","≤ 2","EEFHX0E331R","7.3x4.3(D)",1.9,null,2,2.5,330,15,5100,"45°C",1.2,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","500MHz",5.0999999999999996,0.1,82.5,3500,0,"D",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFHX0E331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2.5","≤ 390","≤ 2","EEFJX0E391RB","7.3x4.3(D)",1.9,null,2,2.5,390,3,10200,"45°C",1.2,"-55 to 125","125°C 3000H(2V)","125°C 3000H(2V)",2,"100kHz","500MHz",10.199999999999999,0.1,97.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0E391RB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2.5","≤ 390","≤ 2","EEFKX0E391RB","7.3x4.3(D)",1.9,null,2,2.5,390,3,10200,"45°C",1.2,"-55 to 125","125°C 5500H(2V)","125°C 5500H(2V)",2,"100kHz","500MHz",10.199999999999999,0.1,97.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0E391RB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  2.5","≤ 390","≤ 2","EEFTX0E391RB","7.3x4.3(D)",1.9,null,2,2.5,390,3,10200,"45°C",1.2,"-55 to 135","135°C 5500H(2V)","135°C 5500H(2V)",2,"100kHz","500MHz",10.199999999999999,0.1,97.5,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0E391RB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 390","≤ 2","EEFSX0E391E4","7.3x4.3(D)",1.9,null,2,2.5,390,4.5,8500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",8.5,0.06,97.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E391E4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2.5","≤ 390","≤ 2","EEFJX0E391RC","7.3x4.3(D)",1.9,null,2,2.5,390,4.5,8500,"45°C",1.2,"-55 to 125","125°C 3000H(2V)","125°C 3000H(2V)",2,"100kHz","500MHz",8.5,0.1,97.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0E391RC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2.5","≤ 390","≤ 2","EEFKX0E391RC","7.3x4.3(D)",1.9,null,2,2.5,390,4.5,8500,"45°C",1.2,"-55 to 125","125°C 5500H(2V)","125°C 5500H(2V)",2,"100kHz","500MHz",8.5,0.1,97.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0E391RC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  2.5","≤ 390","≤ 2","EEFTX0E391RC","7.3x4.3(D)",1.9,null,2,2.5,390,4.5,8500,"45°C",1.2,"-55 to 135","135°C 5500H(2V)","135°C 5500H(2V)",2,"100kHz","500MHz",8.5,0.1,97.5,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0E391RC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 390","≤ 2","EEFSX0E391XE","7.3x4.3(D)",1.9,null,2,2.5,390,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,97.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E391XE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 390","≤ 2","EEFSX0E391ER","7.3x4.3(D)",1.9,null,2,2.5,390,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,97.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E391ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2.5","≤ 390","≤ 2","EEFJX0E391RE","7.3x4.3(D)",1.9,null,2,2.5,390,9,6300,"45°C",1.2,"-55 to 125","125°C 3000H(2V)","125°C 3000H(2V)",2,"100kHz","500MHz",6.3,0.1,97.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0E391RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2.5","≤ 390","≤ 2","EEFKX0E391RE","7.3x4.3(D)",1.9,null,2,2.5,390,9,6300,"45°C",1.2,"-55 to 125","125°C 5500H(2V)","125°C 5500H(2V)",2,"100kHz","500MHz",6.3,0.1,97.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0E391RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  2.5","≤ 390","≤ 2","EEFTX0E391RE","7.3x4.3(D)",1.9,null,2,2.5,390,9,6300,"45°C",1.2,"-55 to 135","135°C 5500H(2V)","135°C 5500H(2V)",2,"100kHz","500MHz",6.3,0.1,97.5,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0E391RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  2.5","≤ 390","≤ 2","EEFCX0E391R","7.3x4.3(D)",1.9,null,2,2.5,390,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,97.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0E391R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","GX","No","≤  2.5","≤ 470","≤ 2","EEFGX0E471R","7.3x4.3(D)",1.9,null,2,2.5,470,3,10200,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",10.199999999999999,0.06,117.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0E471R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2.5","≤ 470","≤ 2","EEFJX0E471RB","7.3x4.3(D)",1.9,null,2,2.5,470,3,10200,"45°C",1.2,"-55 to 125","125°C 3000H(2V)","125°C 3000H(2V)",2,"100kHz","500MHz",10.199999999999999,0.1,117.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0E471RB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2.5","≤ 470","≤ 2","EEFKX0E471RB","7.3x4.3(D)",1.9,null,2,2.5,470,3,10200,"45°C",1.2,"-55 to 125","125°C 5500H(2V)","125°C 5500H(2V)",2,"100kHz","500MHz",10.199999999999999,0.1,117.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0E471RB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","GX","No","≤  2.5","≤ 470","≤ 2","EEFGX0E471L","7.3x4.3(D)",1.9,null,2,2.5,470,3,10200,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",10.199999999999999,0.06,117.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGX0E471L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 470","≤ 2","EEFSX0E471E4","7.3x4.3(D)",1.9,null,2,2.5,470,4.5,8500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",8.5,0.06,117.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E471E4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2.5","≤ 470","≤ 2","EEFJX0E471RC","7.3x4.3(D)",1.9,null,2,2.5,470,4.5,8500,"45°C",1.2,"-55 to 125","125°C 3000H(2V)","125°C 3000H(2V)",2,"100kHz","500MHz",8.5,0.1,117.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0E471RC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2.5","≤ 470","≤ 2","EEFKX0E471RC","7.3x4.3(D)",1.9,null,2,2.5,470,4.5,8500,"45°C",1.2,"-55 to 125","125°C 5500H(2V)","125°C 5500H(2V)",2,"100kHz","500MHz",8.5,0.1,117.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0E471RC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LX","No","≤  2.5","≤ 470","≤ 2","EEFLX0E471R4","7.3x4.3(D)",1.9,null,2,2.5,470,4.5,8500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",8.5,0.06,117.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0E471R4","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 470","≤ 2","EEFSX0E471XE","7.3x4.3(D)",1.9,null,2,2.5,470,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,117.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E471XE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LX","No","≤  2.5","≤ 470","≤ 2","EEFLX0E471R","7.3x4.3(D)",1.9,null,2,2.5,470,6,7500,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",7.5,0.06,117.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLX0E471R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  2.5","≤ 470","≤ 2","EEFSX0E471ER","7.3x4.3(D)",1.9,null,2,2.5,470,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,117.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0E471ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  2.5","≤ 470","≤ 2","EEFJX0E471RE","7.3x4.3(D)",1.9,null,2,2.5,470,9,6300,"45°C",1.2,"-55 to 125","125°C 3000H(2V)","125°C 3000H(2V)",2,"100kHz","500MHz",6.3,0.1,117.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0E471RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  2.5","≤ 470","≤ 2","EEFKX0E471RE","7.3x4.3(D)",1.9,null,2,2.5,470,9,6300,"45°C",1.2,"-55 to 125","125°C 5500H(2V)","125°C 5500H(2V)",2,"100kHz","500MHz",6.3,0.1,117.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0E471RE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  2.5","≤ 470","≤ 2","EEFCX0E471R","7.3x4.3(D)",1.9,null,2,2.5,470,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,117.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0E471R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","GY","No","≤  2.5","≤ 680","≤ 3","EEFGY0E681R","7.3x4.3(D)",2.8,null,3,2.5,680,3,10200,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",10.199999999999999,0.06,170,2000,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFGY0E681R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  4","≤  82","≤ 2","EEFSX0G820ER","7.3x4.3(D)",1.9,null,2,4,82,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,32.799999999999997,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0G820ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  4","≤ 100","≤ 2","EEFSX0G101ER","7.3x4.3(D)",1.9,null,2,4,100,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,40,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0G101ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SR","No","≤  4","≤ 120","≤ 1","EEFSR0G121R","7.3x4.3(D)",1,null,1,4,120,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,48,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSR0G121R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LR","No","≤  4","≤ 120","≤ 1","EEFLR0G121R","7.3x4.3(D)",1,null,1,4,120,9,6300,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",6.3,0.06,48,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLR0G121R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CS","No","≤  4","≤ 120","≤ 1.5","EEFCS0G121R","7.3x4.3(D)",1.1000000000000001,null,1.2,4,120,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,48,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCS0G121R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  4","≤ 150","≤ 2","EEFSX0G151E7","7.3x4.3(D)",1.9,null,2,4,150,7,7000,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7,0.06,60,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0G151E7","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  4","≤ 150","≤ 2","EEFSX0G151ER","7.3x4.3(D)",1.9,null,2,4,150,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,60,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0G151ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  4","≤ 150","≤ 2","EEFCX0G151R","7.3x4.3(D)",1.9,null,2,4,150,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,60,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0G151R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  4","≤ 150","≤ 2","EEFJX0G151RF","7.3x4.3(D)",1.9,null,2,4,150,15,5100,"45°C",1.2,"-55 to 125","125°C 3000H(3.2V)","125°C 3000H(3.2V)",2,"100kHz","500MHz",5.0999999999999996,0.1,60,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0G151RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  4","≤ 150","≤ 2","EEFKX0G151RF","7.3x4.3(D)",1.9,null,2,4,150,15,5100,"45°C",1.2,"-55 to 125","125°C 5500H(3.2V)","125°C 5500H(3.2V)",2,"100kHz","500MHz",5.0999999999999996,0.1,60,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0G151RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  4","≤ 150","≤ 2","EEFTX0G151RF","7.3x4.3(D)",1.9,null,2,4,150,15,5100,"45°C",1.2,"-55 to 135","135°C 5500H(3.2V)","135°C 5500H(3.2V)",2,"100kHz","500MHz",5.0999999999999996,0.1,60,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0G151RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  4","≤ 180","≤ 2","EEFSX0G181ER","7.3x4.3(D)",1.9,null,2,4,180,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,72,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0G181ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  4","≤ 180","≤ 2","EEFCX0G181XR","7.3x4.3(D)",1.9,null,2,4,180,12,5600,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.6,0.06,72,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0G181XR","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CT","No","≤  4","≤ 180","≤ 1.5","EEFCT0G181R","7.3x4.3(D)",1.4,null,1.5,4,180,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,72,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCT0G181R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  4","≤ 180","≤ 2","EEFCX0G181R","7.3x4.3(D)",1.9,null,2,4,180,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,72,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0G181R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  4","≤ 180","≤ 2","EEFJX0G181RF","7.3x4.3(D)",1.9,null,2,4,180,15,5100,"45°C",1.2,"-55 to 125","125°C 3000H(3.2V)","125°C 3000H(3.2V)",2,"100kHz","500MHz",5.0999999999999996,0.1,72,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0G181RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  4","≤ 180","≤ 2","EEFKX0G181RF","7.3x4.3(D)",1.9,null,2,4,180,15,5100,"45°C",1.2,"-55 to 125","125°C 5500H(3.2V)","125°C 5500H(3.2V)",2,"100kHz","500MHz",5.0999999999999996,0.1,72,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0G181RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  4","≤ 180","≤ 2","EEFTX0G181RF","7.3x4.3(D)",1.9,null,2,4,180,15,5100,"45°C",1.2,"-55 to 135","135°C 5500H(3.2V)","135°C 5500H(3.2V)",2,"100kHz","500MHz",5.0999999999999996,0.1,72,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0G181RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  4","≤ 220","≤ 2","EEFSX0G221ER","7.3x4.3(D)",1.9,null,2,4,220,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,88,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0G221ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  4","≤ 220","≤ 2","EEFCX0G221XR","7.3x4.3(D)",1.9,null,2,4,220,12,5600,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.6,0.06,88,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0G221XR","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  4","≤ 220","≤ 2","EEFCX0G221R","7.3x4.3(D)",1.9,null,2,4,220,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,88,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0G221R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  4","≤ 220","≤ 2","EEFJX0G221RF","7.3x4.3(D)",1.9,null,2,4,220,15,5100,"45°C",1.2,"-55 to 125","125°C 3000H(3.2V)","125°C 3000H(3.2V)",2,"100kHz","500MHz",5.0999999999999996,0.1,88,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0G221RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  4","≤ 220","≤ 2","EEFKX0G221RF","7.3x4.3(D)",1.9,null,2,4,220,15,5100,"45°C",1.2,"-55 to 125","125°C 5500H(3.2V)","125°C 5500H(3.2V)",2,"100kHz","500MHz",5.0999999999999996,0.1,88,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0G221RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  4","≤ 220","≤ 2","EEFTX0G221RF","7.3x4.3(D)",1.9,null,2,4,220,15,5100,"45°C",1.2,"-55 to 135","135°C 5500H(3.2V)","135°C 5500H(3.2V)",2,"100kHz","500MHz",5.0999999999999996,0.1,88,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0G221RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  4","≤ 270","≤ 2","EEFSX0G271ER","7.3x4.3(D)",1.9,null,2,4,270,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,108,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0G271ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  4","≤ 270","≤ 2","EEFCX0G271R","7.3x4.3(D)",1.9,null,2,4,270,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,108,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0G271R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  4","≤ 330","≤ 2","EEFSX0G331XE","7.3x4.3(D)",1.9,null,2,4,330,6,7500,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7.5,0.06,132,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0G331XE","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  4","≤ 330","≤ 2","EEFSX0G331ER","7.3x4.3(D)",1.9,null,2,4,330,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,132,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0G331ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  4","≤ 330","≤ 2","EEFCX0G331R","7.3x4.3(D)",1.9,null,2,4,330,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.1,247.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0G331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SY","No","≤  4","≤ 470","≤ 3","ECGSY0G471R","7.3x4.3(D)",2.8,null,3,4,470,9,6300,"45°C",1.2,"-55 to  85","_85°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,188,2000,0,"D",-55,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/ECGSY0G471R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CY","No","≤  4","≤ 470","≤ 3","ECGCY0G471R","7.3x4.3(D)",2.8,null,3,4,470,15,5100,"45°C",1.2,"-55 to  85","_85°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,188,2000,0,"D",-55,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/ECGCY0G471R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SR","No","≤  6.3","≤  68","≤ 1","EEFSR0J680R","7.3x4.3(D)",1,null,1,6.3,68,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,42.8,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSR0J680R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","LR","No","≤  6.3","≤  68","≤ 1","EEFLR0J680R","7.3x4.3(D)",1,null,1,6.3,68,9,6300,"45°C",0.5,"-55 to 105","105°C 2000H","-",3,"100kHz","500MHz",6.3,0.06,42.8,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFLR0J680R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CS","No","≤  6.3","≤  68","≤ 1.5","EEFCS0J680R","7.3x4.3(D)",1.1000000000000001,null,1.2,6.3,68,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,42.8,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCS0J680R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CT","No","≤  6.3","≤ 100","≤ 1.5","EEFCT0J101R","7.3x4.3(D)",1.4,null,1.5,6.3,100,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,63,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCT0J101R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  6.3","≤ 100","≤ 2","EEFCX0J101R","7.3x4.3(D)",1.9,null,2,6.3,100,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,63,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0J101R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  6.3","≤ 120","≤ 2","EEFSX0J121E7","7.3x4.3(D)",1.9,null,2,6.3,120,7,7000,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",7,0.06,75.599999999999994,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0J121E7","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  6.3","≤ 120","≤ 2","EEFCX0J121R","7.3x4.3(D)",1.9,null,2,6.3,120,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,75.599999999999994,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0J121R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  6.3","≤ 120","≤ 2","EEFJX0J121RF","7.3x4.3(D)",1.9,null,2,6.3,120,15,5100,"45°C",1.2,"-55 to 125","125°C 3000H(5V)","125°C 3000H(5V)",2,"100kHz","500MHz",5.0999999999999996,0.1,75.599999999999994,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0J121RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  6.3","≤ 120","≤ 2","EEFKX0J121RF","7.3x4.3(D)",1.9,null,2,6.3,120,15,5100,"45°C",1.2,"-55 to 125","125°C 5500H(5V)","125°C 5500H(5V)",2,"100kHz","500MHz",5.0999999999999996,0.1,75.599999999999994,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0J121RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  6.3","≤ 120","≤ 2","EEFTX0J121RF","7.3x4.3(D)",1.9,null,2,6.3,120,15,5100,"45°C",1.2,"-55 to 135","135°C 5500H(5V)","135°C 5500H(5V)",2,"100kHz","500MHz",5.0999999999999996,0.1,75.599999999999994,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0J121RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  6.3","≤ 150","≤ 2","EEFSX0J151ER","7.3x4.3(D)",1.9,null,2,6.3,150,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,94.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0J151ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  6.3","≤ 150","≤ 2","EEFCX0J151XR","7.3x4.3(D)",1.9,null,2,6.3,150,12,5600,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.6,0.06,94.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0J151XR","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  6.3","≤ 150","≤ 2","EEFCX0J151R","7.3x4.3(D)",1.9,null,2,6.3,150,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,94.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0J151R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","JX","No","≤  6.3","≤ 150","≤ 2","EEFJX0J151RF","7.3x4.3(D)",1.9,null,2,6.3,150,15,5100,"45°C",1.2,"-55 to 125","125°C 3000H(5V)","125°C 3000H(5V)",2,"100kHz","500MHz",5.0999999999999996,0.1,94.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFJX0J151RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","KX","No","≤  6.3","≤ 150","≤ 2","EEFKX0J151RF","7.3x4.3(D)",1.9,null,2,6.3,150,15,5100,"45°C",1.2,"-55 to 125","125°C 5500H(5V)","125°C 5500H(5V)",2,"100kHz","500MHz",5.0999999999999996,0.1,94.5,3500,0,"D",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFKX0J151RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","TX","No","≤  6.3","≤ 150","≤ 2","EEFTX0J151RF","7.3x4.3(D)",1.9,null,2,6.3,150,15,5100,"45°C",1.2,"-55 to 135","135°C 5500H(5V)","135°C 5500H(5V)",2,"100kHz","500MHz",5.0999999999999996,0.1,94.5,3500,0,"D",-55,135,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFTX0J151RF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  6.3","≤ 180","≤ 2","EEFSX0J181ER","7.3x4.3(D)",1.9,null,2,6.3,180,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,113.4,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0J181ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  6.3","≤ 180","≤ 2","EEFCX0J181R","7.3x4.3(D)",1.9,null,2,6.3,180,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,113.4,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0J181R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SX","No","≤  6.3","≤ 220","≤ 2","EEFSX0J221ER","7.3x4.3(D)",1.9,null,2,6.3,220,9,6300,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,207.9,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFSX0J221ER","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CX","No","≤  6.3","≤ 220","≤ 2","EEFCX0J221R","7.3x4.3(D)",1.9,null,2,6.3,220,15,5100,"45°C",1.2,"-55 to 105","105°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.1,247.5,3500,0,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/EEFCX0J221R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","SY","No","≤  6.3","≤ 330","≤ 3","ECGSY0J331R","7.3x4.3(D)",2.8,null,3,6.3,330,9,6300,"45°C",1.2,"-55 to  85","_85°C 2000H","-",2,"100kHz","500MHz",6.3,0.06,207.9,2000,0,"D",-55,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/ECGSY0J331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Al","SP-Cap","CY","No","≤  6.3","≤ 330","≤ 3","ECGCY0J331R","7.3x4.3(D)",2.8,null,3,6.3,330,15,5100,"45°C",1.2,"-55 to  85","_85°C 2000H","-",2,"100kHz","500MHz",5.0999999999999996,0.06,207.9,2000,0,"D",-55,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/SP-Cap/models/ECGCY0J331R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-GX.jpg","100kHz"]
["P POS",null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPSF","No","≤  2","≤ 270","≤ 2","2TPSF270M6E","3.5x2.8(B)",1.9,null,2,2,270,6,3200,"45°C",0.7,"-55 to 105","105°C 1000H","-",2,"500kHz","10MHz",3.2,0.08,108,2000,0,"B2S",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2TPSF270M6E","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPSF","No","≤  2","≤ 270","≤ 2","2TPSF270M9G","3.5x2.8(B)",1.9,null,2,2,270,9,2400,"45°C",0.7,"-55 to 105","105°C 1000H","-",2,"300kHz","10MHz",2.4,0.08,108,2000,0,"B2S",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2TPSF270M9G","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2","≤ 470","≤ 2","2TPE470MAJGB","3.5x2.8(B)",1.9,null,2,2,470,11,2300,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"300kHz","10MHz",2.2999999999999998,0.1,188,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2TPE470MAJGB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2","≤ 470","≤ 2","2TPE470MAFB","3.5x2.8(B)",1.9,null,2,2,470,15,2300,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",2.2999999999999998,0.1,188,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2TPE470MAFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 220","≤ 2","2R5TPE220M9","7.3x4.3(D)",1.8,null,1.9,2.5,220,9,3900,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.9,0.1,55,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE220M9","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  2.5","≤ 220","≤ 2","2R5TAE220M9","7.3x4.3(D)",1.8,null,1.9,2.5,220,9,3900,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.9,0.1,110,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TAE220M9","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 220","≤ 2","2R5TPE220MAFB","3.5x2.8(B)",1.9,null,2,2.5,220,15,2000,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",2,0.08,110,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE220MAFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 220","≤ 2","2R5TPE220MFGB","3.5x2.8(B)",1.9,null,2,2.5,220,15,1800,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"300kHz","10MHz",1.8,0.08,110,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE220MFGB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 220","≤ 2","2R5TPE220MF","7.3x4.3(D)",1.8,null,1.9,2.5,220,15,3100,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,55,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE220MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  2.5","≤ 220","≤ 2","2R5TAE220MF","7.3x4.3(D)",1.8,null,1.9,2.5,220,15,3100,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,55,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TAE220MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 220","≤ 2","2R5TPE220MI","7.3x4.3(D)",1.8,null,1.9,2.5,220,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,55,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE220MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 220","≤ 2","2R5TPE220MLB","3.5x2.8(B)",1.9,null,2,2.5,220,21,1700,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.7,0.08,55,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE220MLB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 220","≤ 2","2R5TPE220MAPB","3.5x2.8(B)",1.9,null,2,2.5,220,25,1600,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.6,0.08,55,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE220MAPB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  2.5","≤ 220","≤ 2","2R5TAE220M","7.3x4.3(D)",1.8,null,1.9,2.5,220,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,55,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TAE220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 220","≤ 2","2R5TPE220M","7.3x4.3(D)",1.8,null,1.9,2.5,220,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,55,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPS","No","≤  2.5","≤ 220","≤ 1.5","ETPS220MUD","3.5x2.8(B)",1.1000000000000001,null,1.2,2.5,220,30,1400,"45°C",1.1000000000000001,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,55,2500,0,"B1S",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETPS220MUD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 220","≤ 2","2R5TPE220MUB","3.5x2.8(B)",1.9,null,2,2.5,220,30,1400,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,55,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE220MUB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 220","≤ 2","2R5TPE220MAZB","3.5x2.8(B)",1.9,null,2,2.5,220,35,1400,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,55,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE220MAZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 220","≤ 2","2R5TPE220MZB","3.5x2.8(B)",1.9,null,2,2.5,220,35,1400,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,55,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE220MZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THC","No","≤  2.5","≤ 220","≤ 2","2R5THC220M","7.3x4.3(D)",1.9,null,2,2.5,220,45,1700,"45°C",2,"-55 to 125","125°C 1000H(1.6V)","125°C 1000H(1.6V)",2,"100kHz","10MHz",1.7,0.1,55,3000,0,"D2",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5THC220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPSF","No","≤  2.5","≤ 270","≤ 2","ETPSF270M6E","3.5x2.8(B)",1.9,null,2,2.5,270,6,3200,"45°C",0.7,"-55 to 105","105°C 1000H","-",2,"500kHz","10MHz",3.2,0.1,135,2000,0,"B2S",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETPSF270M6E","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 330","≤ 2","2R5TPE330M7","7.3x4.3(D)",1.8,null,1.9,2.5,330,7,4400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.1,82.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE330M7","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 330","≤ 2","ETPE330MA9GB","3.5x2.8(B)",1.9,null,2,2.5,330,9,3200,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"300kHz","10MHz",3.2,0.08,165,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETPE330MA9GB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 330","≤ 2","ETPE330M9GB","3.5x2.8(B)",1.9,null,2,2.5,330,9,3200,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",3.2,0.08,165,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETPE330M9GB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 330","≤ 2","2R5TPE330M9","7.3x4.3(D)",1.8,null,1.9,2.5,330,9,3900,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.9,0.1,82.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE330M9","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  2.5","≤ 330","≤ 2","ETCE330M9GB","3.5x2.8(B)",1.9,null,2,2.5,330,9,3200,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"300kHz","10MHz",3.2,0.08,165,2000,0,"B2",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETCE330M9GB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 330","≤ 2","2R5TPE330MC","7.3x4.3(D)",1.8,null,1.9,2.5,330,12,3500,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.5,0.1,82.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE330MC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 330","≤ 2","ETPE330MFB","3.5x2.8(B)",1.9,null,2,2.5,330,15,2700,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",2.7,0.08,165,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETPE330MFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 330","≤ 2","2R5TPE330MF","7.3x4.3(D)",1.8,null,1.9,2.5,330,15,3100,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,82.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE330MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  2.5","≤ 330","≤ 2","2R5TAE330MF","7.3x4.3(D)",1.8,null,1.9,2.5,330,15,3100,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,82.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TAE330MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THE","No","≤  2.5","≤ 330","≤ 2","2R5THE330MF","7.3x4.3(D)",1.8,null,1.9,2.5,330,15,3100,"45°C",1.8,"-55 to 125","125°C 1000H(1.6V)","125°C 1000H(1.6V)",2,"100kHz","10MHz",3.1,0.1,82.5,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5THE330MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 330","≤ 2","ETPE330MIB","3.5x2.8(B)",1.9,null,2,2.5,330,18,2450,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",2.4500000000000002,0.08,165,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETPE330MIB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 330","≤ 2","2R5TPE330MI","7.3x4.3(D)",1.8,null,1.9,2.5,330,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,82.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE330MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  2.5","≤ 330","≤ 2","2R5TAE330MI","7.3x4.3(D)",1.8,null,1.9,2.5,330,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,82.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TAE330MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THE","No","≤  2.5","≤ 330","≤ 2","2R5THE330MI","7.3x4.3(D)",1.8,null,1.9,2.5,330,18,2800,"45°C",1.8,"-55 to 125","125°C 1000H(1.6V)","125°C 1000H(1.6V)",2,"100kHz","10MHz",2.8,0.1,82.5,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5THE330MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  2.5","≤ 330","≤ 2","2R5TAE330M","7.3x4.3(D)",1.8,null,1.9,2.5,330,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,82.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TAE330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 330","≤ 2","2R5TPE330M","7.3x4.3(D)",1.8,null,1.9,2.5,330,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,82.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THE","No","≤  2.5","≤ 330","≤ 2","2R5THE330M","7.3x4.3(D)",1.8,null,1.9,2.5,330,25,2400,"45°C",1.8,"-55 to 125","125°C 1000H(1.6V)","125°C 1000H(1.6V)",2,"100kHz","10MHz",2.4,0.1,82.5,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5THE330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPS","No","≤  2.5","≤ 330","≤ 1.5","ETPS330MUD","3.5x2.8(B)",1.1000000000000001,null,1.2,2.5,330,30,1400,"45°C",1.1000000000000001,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,82.5,2500,0,"B1S",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETPS330MUD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 330","≤ 2","2R5TPE330MAZB","3.5x2.8(B)",1.9,null,2,2.5,330,35,1400,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,82.5,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE330MAZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  2.5","≤ 470","≤ 3","2R5TPF470M6L","7.3x4.3(D)",2.8,null,3,2.5,470,6,4400,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.1,117.5,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPF470M6L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 470","≤ 2","2R5TPE470M7","7.3x4.3(D)",1.8,null,1.9,2.5,470,7,4400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.1,117.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE470M7","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  2.5","≤ 470","≤ 3","2R5TPF470M7L","7.3x4.3(D)",2.8,null,3,2.5,470,7,4400,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.1,117.5,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPF470M7L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 470","≤ 2","2R5TPE470M9","7.3x4.3(D)",1.8,null,1.9,2.5,470,9,3900,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.9,0.1,117.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE470M9","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  2.5","≤ 470","≤ 3","2R5TPF470M9L","7.3x4.3(D)",2.8,null,3,2.5,470,9,3850,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.85,0.1,117.5,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPF470M9L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  2.5","≤ 470","≤ 3","2R5TPF470ML","7.3x4.3(D)",2.8,null,3,2.5,470,10,4400,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.1,117.5,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPF470ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 470","≤ 2","2R5TPE470MC","7.3x4.3(D)",1.8,null,1.9,2.5,470,12,3500,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.5,0.1,117.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE470MC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 470","≤ 2","2R5TPE470MF","7.3x4.3(D)",1.8,null,1.9,2.5,470,15,3100,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,117.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE470MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  2.5","≤ 470","≤ 2","2R5TAE470MF","7.3x4.3(D)",1.8,null,1.9,2.5,470,15,3100,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,117.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TAE470MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 470","≤ 2","2R5TPE470MI","7.3x4.3(D)",1.8,null,1.9,2.5,470,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,117.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE470MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  2.5","≤ 470","≤ 2","2R5TAE470M","7.3x4.3(D)",1.8,null,1.9,2.5,470,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,117.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TAE470M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  2.5","≤ 680","≤ 4","ETPF680M5H","7.3x4.3(D)",3.8,null,4,2.5,680,5,6100,"45°C",2.5,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",6.1,0.1,170,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETPF680M5H","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  2.5","≤ 680","≤ 4","ETCF680M5H","7.3x4.3(D)",3.8,null,4,2.5,680,5,6100,"45°C",2.5,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","10MHz",6.1,0.1,170,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETCF680M5H","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  2.5","≤ 680","≤ 3","2R5TPF680M6L","7.3x4.3(D)",2.8,null,3,2.5,680,6,4400,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.1,170,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPF680M6L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  2.5","≤ 680","≤ 3","ETCF680M6L","7.3x4.3(D)",2.8,null,3,2.5,680,6,4400,"45°C",2,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","10MHz",4.4000000000000004,0.1,170,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETCF680M6L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  2.5","≤ 680","≤ 3","2R5TPF680M7L","7.3x4.3(D)",2.8,null,3,2.5,680,7,4400,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.1,170,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPF680M7L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  2.5","≤ 680","≤ 3","ETCF680M7L","7.3x4.3(D)",2.8,null,3,2.5,680,7,4400,"45°C",2,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","10MHz",4.4000000000000004,0.1,170,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETCF680M7L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  2.5","≤ 680","≤ 3","2R5TPF680ML","7.3x4.3(D)",2.8,null,3,2.5,680,10,4400,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.1,170,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPF680ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  2.5","≤ 680","≤ 3","ETCF680ML","7.3x4.3(D)",2.8,null,3,2.5,680,10,4400,"45°C",2,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","10MHz",4.4000000000000004,0.1,170,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETCF680ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 680","≤ 3","2R5TPE680MCL","7.3x4.3(D)",2.8,null,3,2.5,680,12,3500,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.5,0.1,170,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE680MCL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  2.5","≤ 680","≤ 3","ETCE680MCL","7.3x4.3(D)",2.8,null,3,2.5,680,12,3500,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","10MHz",3.5,0.1,170,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETCE680MCL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 680","≤ 3","2R5TPE680MFL","7.3x4.3(D)",2.8,null,3,2.5,680,15,3100,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,170,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE680MFL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  2.5","≤ 680","≤ 3","2R5TAE680MFL","7.3x4.3(D)",2.8,null,3,2.5,680,15,3100,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,170,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TAE680MFL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  2.5","≤ 680","≤ 3","ETCE680MFL","7.3x4.3(D)",2.8,null,3,2.5,680,15,3100,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","10MHz",3.1,0.1,170,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETCE680MFL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  2.5","≤ 680","≤ 3","2R5TAE680ML","7.3x4.3(D)",2.8,null,3,2.5,680,25,2400,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,170,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TAE680ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  2.5","≤ 680","≤ 4","ETPF680MPH","7.3x4.3(D)",3.8,null,4,2.5,680,25,2700,"45°C",2.5,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.7,0.1,170,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETPF680MPH","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤ 680","≤ 3","2R5TPE680MWL","7.3x4.3(D)",2.8,null,3,2.5,680,40,1850,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.85,0.1,170,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE680MWL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  2.5","≤1000","≤ 4","ETPF1000M5H","7.3x4.3(D)",3.8,null,4,2.5,1000,5,6100,"45°C",2.5,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",6.1,0.1,250,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETPF1000M5H","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  2.5","≤1000","≤ 4","ETCF1000M5H","7.3x4.3(D)",3.8,null,4,2.5,1000,5,6100,"45°C",2.5,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","10MHz",6.1,0.1,250,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETCF1000M5H","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  2.5","≤1000","≤ 4","ETPF1000M6H","7.3x4.3(D)",3.8,null,4,2.5,1000,6,5600,"45°C",2.5,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",5.6,0.1,250,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETPF1000M6H","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  2.5","≤1000","≤ 4","ETCF1000M6H","7.3x4.3(D)",3.8,null,4,2.5,1000,6,5600,"45°C",2.5,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","10MHz",5.6,0.1,250,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETCF1000M6H","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤1000","≤ 4","2R5TPE1000MF","7.3x4.3(D)",3.8,null,4,2.5,1000,15,3900,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.9,0.15,250,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE1000MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  2.5","≤1000","≤ 4","ETCE1000MF","7.3x4.3(D)",3.8,null,4,2.5,1000,15,3900,"45°C",2.6,"-55 to 125","125°C 1000H(2V)","125°C 1000H(2V)",2,"100kHz","10MHz",3.9,0.15,250,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/ETCE1000MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤1500","≤ 4","2R5TPE1500MC","7.3x4.3(D)",3.8,null,4,2.5,1500,12,4400,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.15,375,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE1500MC","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  2.5","≤1500","≤ 4","2R5TPE1500MF","7.3x4.3(D)",3.8,null,4,2.5,1500,15,3900,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.9,0.15,375,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/2R5TPE1500MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤  4","≤  68","≤ 2","4TPB68M","3.5x2.8(B)",1.9,null,2,4,68,70,1100,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.1000000000000001,0.08,27.2,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPB68M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 100","≤ 2","4TPE100MZB","3.5x2.8(B)",1.9,null,2,4,100,35,1400,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,40,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE100MZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 100","≤ 2","4TPE100MWB","3.5x2.8(B)",1.9,null,2,4,100,40,1300,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.3,0.08,40,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE100MWB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  4","≤ 100","≤ 2","4TAB100M","3.5x2.8(B)",1.9,null,2,4,100,70,1100,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.1000000000000001,0.08,40,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TAB100M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 100","≤ 2","4TPE100MBB","3.5x2.8(B)",1.9,null,2,4,100,70,950,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",0.95,0.08,40,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE100MBB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 150","≤ 2","4TPE150MI","7.3x4.3(D)",1.8,null,1.9,4,150,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,60,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE150MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  4","≤ 150","≤ 2","4TCE150MI","7.3x4.3(D)",1.8,null,1.9,4,150,18,2800,"45°C",1.8,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",2.8,0.1,60,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCE150MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 150","≤ 2","4TPE150MAZB","3.5x2.8(B)",1.9,null,2,4,150,35,1400,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,60,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE150MAZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 220","≤ 2","4TPE220MF","7.3x4.3(D)",1.8,null,1.9,4,220,15,3100,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,88,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE220MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  4","≤ 220","≤ 2","4TCE220MF","7.3x4.3(D)",1.8,null,1.9,4,220,15,3100,"45°C",1.8,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",3.1,0.1,88,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCE220MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THE","No","≤  4","≤ 220","≤ 2","4THE220MF","7.3x4.3(D)",1.8,null,1.9,4,220,15,3100,"45°C",1.8,"-55 to 125","125°C 1000H(2.5V)","125°C 1000H(2.5V)",2,"100kHz","10MHz",3.1,0.1,88,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4THE220MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 220","≤ 2","4TPE220MI","7.3x4.3(D)",1.8,null,1.9,4,220,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,88,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE220MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  4","≤ 220","≤ 2","4TAE220MI","7.3x4.3(D)",1.8,null,1.9,4,220,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,88,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TAE220MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  4","≤ 220","≤ 2","4TCE220MI","7.3x4.3(D)",1.8,null,1.9,4,220,18,2800,"45°C",1.8,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",2.8,0.1,88,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCE220MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THE","No","≤  4","≤ 220","≤ 2","4THE220MI","7.3x4.3(D)",1.8,null,1.9,4,220,18,2800,"45°C",1.8,"-55 to 125","125°C 1000H(2.5V)","125°C 1000H(2.5V)",2,"100kHz","10MHz",2.8,0.1,88,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4THE220MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 220","≤ 2","4TPE220M","7.3x4.3(D)",1.8,null,1.9,4,220,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,88,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  4","≤ 220","≤ 2","4TAE220M","7.3x4.3(D)",1.8,null,1.9,4,220,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,88,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TAE220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  4","≤ 220","≤ 2","4TCE220M","7.3x4.3(D)",1.8,null,1.9,4,220,25,2400,"45°C",1.8,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",2.4,0.1,88,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCE220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THE","No","≤  4","≤ 220","≤ 2","4THE220M","7.3x4.3(D)",1.8,null,1.9,4,220,25,2400,"45°C",1.8,"-55 to 125","125°C 1000H(2.5V)","125°C 1000H(2.5V)",2,"100kHz","10MHz",2.4,0.1,88,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4THE220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPS","No","≤  4","≤ 220","≤ 1.5","4TPS220MUD","3.5x2.8(B)",1.1000000000000001,null,1.2,4,220,30,1400,"45°C",1.1000000000000001,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,88,2500,0,"B1S",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPS220MUD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 220","≤ 2","4TPE220MAZB","3.5x2.8(B)",1.9,null,2,4,220,35,1400,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,88,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE220MAZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 220","≤ 2","4TPE220MZB","3.5x2.8(B)",1.9,null,2,4,220,35,1350,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.35,0.08,88,2000,0,"B2",-55,105,"→4TPE220MAZB",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE220MZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 220","≤ 2","4TPE220MVB","3.5x2.8(B)",1.9,null,2,4,220,45,1150,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.1499999999999999,0.08,88,2000,0,"B2",-55,105,"→4TPE220MAZB",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE220MVB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 220","≤ 2","4TPE220MV","7.3x4.3(D)",1.8,null,1.9,4,220,45,1750,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.75,0.1,88,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE220MV","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 220","≤ 2","4TPE220MBB","3.5x2.8(B)",1.9,null,2,4,220,70,950,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",0.95,0.08,88,2000,0,"B2",-55,105,"→4TPE220MAZB",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE220MBB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  4","≤ 330","≤ 3","4TPF330M9L","7.3x4.3(D)",2.8,null,3,4,330,9,3900,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.9,0.1,132,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPF330M9L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  4","≤ 330","≤ 3","4TPF330ML","7.3x4.3(D)",2.8,null,3,4,330,12,4000,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4,0.1,132,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPF330ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  4","≤ 330","≤ 3","4TCF330ML","7.3x4.3(D)",2.8,null,3,4,330,12,4000,"45°C",2,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",4,0.1,132,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCF330ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  4","≤ 330","≤ 3","4TPF330MFL","7.3x4.3(D)",2.8,null,3,4,330,15,3550,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.55,0.1,132,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPF330MFL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 330","≤ 2","4TPE330MI","7.3x4.3(D)",1.8,null,1.9,4,330,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,132,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE330MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  4","≤ 330","≤ 2","4TCE330MI","7.3x4.3(D)",1.8,null,1.9,4,330,18,2800,"45°C",1.8,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",2.8,0.1,132,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCE330MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 330","≤ 2","4TPE330M","7.3x4.3(D)",1.8,null,1.9,4,330,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,132,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  4","≤ 330","≤ 2","4TCE330M","7.3x4.3(D)",1.8,null,1.9,4,330,25,2400,"45°C",1.8,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",2.4,0.1,132,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCE330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 330","≤ 2","4TPE330MW","7.3x4.3(D)",1.8,null,1.9,4,330,40,1850,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.85,0.1,132,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE330MW","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THB","No","≤  4","≤ 330","≤ 3","4THB330ML","7.3x4.3(D)",2.8,null,3,4,330,40,2000,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(2.5V)","125°C 1000H(2.5V)",2,"100kHz","10MHz",2,0.1,132,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4THB330ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  4","≤ 470","≤ 3","4TPF470ML","7.3x4.3(D)",2.8,null,3,4,470,10,4400,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.1,188,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPF470ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  4","≤ 470","≤ 3","4TCF470ML","7.3x4.3(D)",2.8,null,3,4,470,10,4400,"45°C",2,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",4.4000000000000004,0.1,188,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCF470ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 470","≤ 3","4TPE470MCL","7.3x4.3(D)",2.8,null,3,4,470,12,3500,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.5,0.1,188,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE470MCL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  4","≤ 470","≤ 3","4TCE470MCL","7.3x4.3(D)",2.8,null,3,4,470,12,3500,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",3.5,0.1,188,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCE470MCL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 470","≤ 3","4TPE470MFL","7.3x4.3(D)",2.8,null,3,4,470,15,3100,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,188,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE470MFL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  4","≤ 470","≤ 3","4TCE470MFL","7.3x4.3(D)",2.8,null,3,4,470,15,3100,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",3.1,0.1,188,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCE470MFL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 470","≤ 3","4TPE470MIL","7.3x4.3(D)",2.8,null,3,4,470,18,2800,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,188,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE470MIL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  4","≤ 470","≤ 3","4TAE470MIL","7.3x4.3(D)",2.8,null,3,4,470,18,2800,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,188,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TAE470MIL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  4","≤ 470","≤ 3","4TCE470MIL","7.3x4.3(D)",2.8,null,3,4,470,18,2800,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",2.8,0.1,188,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCE470MIL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 470","≤ 3","4TPE470ML","7.3x4.3(D)",2.8,null,3,4,470,25,2400,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,188,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE470ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  4","≤ 470","≤ 3","4TAE470ML","7.3x4.3(D)",2.8,null,3,4,470,25,2400,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,188,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TAE470ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  4","≤ 470","≤ 3","4TCE470ML","7.3x4.3(D)",2.8,null,3,4,470,25,2400,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",2.4,0.1,188,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCE470ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  4","≤ 470","≤ 3","4TPE470MWL","7.3x4.3(D)",2.8,null,3,4,470,40,1850,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.85,0.1,188,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPE470MWL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  4","≤ 680","≤ 4","4TPF680MAH","7.3x4.3(D)",3.8,null,4,4,680,10,4400,"45°C",2.5,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.1,272,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPF680MAH","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  4","≤ 680","≤ 4","4TCF680MAH","7.3x4.3(D)",3.8,null,4,4,680,10,4400,"45°C",2.5,"-55 to 125","125°C 1000H(3.2V)","125°C 1000H(3.2V)",2,"100kHz","10MHz",4.4000000000000004,0.1,272,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TCF680MAH","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  4","≤ 680","≤ 4","4TPF680MFH","7.3x4.3(D)",3.8,null,4,4,680,15,3550,"45°C",2.5,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.55,0.1,272,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPF680MFH","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  4","≤ 680","≤ 4","4TPF680MZH","7.3x4.3(D)",3.8,null,4,4,680,35,2350,"45°C",2.5,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.35,0.1,272,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/4TPF680MZH","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤  6.3","≤  33","≤ 2","6TPB33M","3.5x2.8(B)",1.9,null,2,6.3,33,70,1100,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.1000000000000001,0.08,20.8,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPB33M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  6.3","≤  47","≤ 2","6TAB47M","3.5x2.8(B)",1.9,null,2,6.3,47,70,1100,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.1000000000000001,0.08,29.6,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TAB47M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  6.3","≤  68","≤ 2","6TAB68M","3.5x2.8(B)",1.9,null,2,6.3,68,70,1100,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.1000000000000001,0.08,42.8,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TAB68M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤  6.3","≤  68","≤ 2","6TPB68M","3.5x2.8(B)",1.9,null,2,6.3,68,70,1100,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.1000000000000001,0.08,42.8,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPB68M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 100","≤ 2","6TPE100MI","7.3x4.3(D)",1.8,null,1.9,6.3,100,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,63,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE100MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 100","≤ 2","6TCE100MI","7.3x4.3(D)",1.8,null,1.9,6.3,100,18,2800,"45°C",1.8,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",2.8,0.1,63,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE100MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 100","≤ 2","6TPE100MPB","3.5x2.8(B)",1.9,null,2,6.3,100,25,1600,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.6,0.08,63,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE100MPB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 100","≤ 2","6TPE100M","7.3x4.3(D)",1.8,null,1.9,6.3,100,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,63,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE100M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 100","≤ 2","6TCE100M","7.3x4.3(D)",1.8,null,1.9,6.3,100,25,2400,"45°C",1.8,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",2.4,0.1,63,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE100M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 100","≤ 2","6TPE100MAZB","3.5x2.8(B)",1.9,null,2,6.3,100,35,1400,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,63,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE100MAZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 100","≤ 2","6TPE100MZB","3.5x2.8(B)",1.9,null,2,6.3,100,35,1400,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,63,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE100MZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 100","≤ 2","6TPE100MWB","3.5x2.8(B)",1.9,null,2,6.3,100,40,1300,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.3,0.08,63,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE100MWB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 100","≤ 2","6TPE100MW","7.3x4.3(D)",1.8,null,1.9,6.3,100,40,1850,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.85,0.1,63,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE100MW","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 100","≤ 2","6TPE100MVB","3.5x2.8(B)",1.9,null,2,6.3,100,45,1200,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.2,0.08,63,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE100MVB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 100","≤ 2","6TPE100MBB","3.5x2.8(B)",1.9,null,2,6.3,100,70,950,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",0.95,0.08,63,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE100MBB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 120","≤ 2","6TPE120MAZB","3.5x2.8(B)",1.9,null,2,6.3,120,35,1400,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,75.599999999999994,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE120MAZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 150","≤ 2","6TPE150MF","7.3x4.3(D)",1.8,null,1.9,6.3,150,15,3100,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,94.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE150MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 150","≤ 2","6TCE150MF","7.3x4.3(D)",1.8,null,1.9,6.3,150,15,3100,"45°C",1.8,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",3.1,0.1,94.5,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE150MF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 150","≤ 2","6TPE150MI","7.3x4.3(D)",1.8,null,1.9,6.3,150,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,94.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE150MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 150","≤ 2","6TCE150MI","7.3x4.3(D)",1.8,null,1.9,6.3,150,18,2800,"45°C",1.8,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",2.8,0.1,94.5,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE150MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THE","No","≤  6.3","≤ 150","≤ 2","6THE150MI","7.3x4.3(D)",1.8,null,1.9,6.3,150,18,2800,"45°C",1.8,"-55 to 125","125°C 1000H(4V)","125°C 1000H(4V)",2,"100kHz","10MHz",2.8,0.1,94.5,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6THE150MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 150","≤ 2","6TPE150MAPB","3.5x2.8(B)",1.9,null,2,6.3,150,25,1600,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.6,0.08,94.5,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE150MAPB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 150","≤ 2","6TPE150M","7.3x4.3(D)",1.8,null,1.9,6.3,150,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,94.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE150M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  6.3","≤ 150","≤ 2","6TAE150M","7.3x4.3(D)",1.8,null,1.9,6.3,150,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,94.5,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TAE150M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  6.3","≤ 150","≤ 3","6TPF150MPL","7.3x4.3(D)",2.8,null,3,6.3,150,25,2750,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.75,0.1,94.5,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPF150MPL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TV","Yes","≤  6.3","≤ 150","≤ 2","6TVE150M","7.3x4.3(D)",1.8,null,1.9,6.3,150,25,2400,"45°C",1.8,"-55 to 125","105°C 2000H","125°C 1000H(4V)",2,"100kHz","10MHz",2.4,0.1,94.5,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TVE150M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 150","≤ 2","6TCE150M","7.3x4.3(D)",1.8,null,1.9,6.3,150,25,2400,"45°C",1.8,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",2.4,0.1,94.5,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE150M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THE","No","≤  6.3","≤ 150","≤ 2","6THE150M","7.3x4.3(D)",1.8,null,1.9,6.3,150,25,2400,"45°C",1.8,"-55 to 125","125°C 1000H(4V)","125°C 1000H(4V)",2,"100kHz","10MHz",2.4,0.1,94.5,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6THE150M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPS","No","≤  6.3","≤ 150","≤ 1.5","6TPS150MUD","3.5x2.8(B)",1.1000000000000001,null,1.2,6.3,150,30,1400,"45°C",1.1000000000000001,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,94.5,2500,0,"B1S",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPS150MUD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 150","≤ 2","6TPE150MAZB","3.5x2.8(B)",1.9,null,2,6.3,150,35,1400,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,94.5,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE150MAZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPS","No","≤  6.3","≤ 150","≤ 1.5","6TPS150MZD","3.5x2.8(B)",1.1000000000000001,null,1.2,6.3,150,35,1250,"45°C",1.1000000000000001,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.25,0.1,94.5,2500,0,"B1S",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPS150MZD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  6.3","≤ 220","≤ 3","6TPF220M6L","7.3x4.3(D)",2.8,null,3,6.3,220,6,5550,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",5.55,0.1,138.6,2500,0,"D3L",-55,105,"→6TPF330M9L",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPF220M6L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  6.3","≤ 220","≤ 3","6TPF220M9L","7.3x4.3(D)",2.8,null,3,6.3,220,9,4600,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.5999999999999996,0.1,138.6,2500,0,"D3L",-55,105,"→6TPF330M9L",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPF220M9L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  6.3","≤ 220","≤ 3","6TCF220M9L","7.3x4.3(D)",2.8,null,3,6.3,220,9,4600,"45°C",2,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",4.5999999999999996,0.1,138.6,2500,0,"D3L",-55,125,"→6TPF330M9L",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCF220M9L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  6.3","≤ 220","≤ 3","6TPF220ML","7.3x4.3(D)",2.8,null,3,6.3,220,12,4000,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4,0.1,138.6,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPF220ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  6.3","≤ 220","≤ 3","6TCF220ML","7.3x4.3(D)",2.8,null,3,6.3,220,12,4000,"45°C",2,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",4,0.1,138.6,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCF220ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  6.3","≤ 220","≤ 3","6TPF220MFL","7.3x4.3(D)",2.8,null,3,6.3,220,15,3550,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.55,0.1,138.6,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPF220MFL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 220","≤ 2","6TPE220MI","7.3x4.3(D)",1.8,null,1.9,6.3,220,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,138.6,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE220MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  6.3","≤ 220","≤ 2","6TAE220MI","7.3x4.3(D)",1.8,null,1.9,6.3,220,18,2800,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,138.6,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TAE220MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 220","≤ 3","6TPE220MIL","7.3x4.3(D)",2.8,null,3,6.3,220,18,2800,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,138.6,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE220MIL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 220","≤ 2","6TCE220MI","7.3x4.3(D)",1.8,null,1.9,6.3,220,18,2800,"45°C",1.8,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",2.8,0.1,138.6,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE220MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 220","≤ 2","6TPE220MAPB","3.5x2.8(B)",1.9,null,2,6.3,220,25,1600,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.6,0.1,138.6,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE220MAPB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 220","≤ 2","6TPE220MAP","7.3x4.3(D)",1.8,null,1.9,6.3,220,25,2400,"45°C",1.8,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",2.4,0.1,138.6,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE220MAP","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 220","≤ 2","6TPE220M","7.3x4.3(D)",1.8,null,1.9,6.3,220,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,138.6,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  6.3","≤ 220","≤ 2","6TAE220M","7.3x4.3(D)",1.8,null,1.9,6.3,220,25,2400,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,138.6,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TAE220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  6.3","≤ 220","≤ 3","6TPF220MPL","7.3x4.3(D)",2.8,null,3,6.3,220,25,2750,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.75,0.1,138.6,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPF220MPL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 220","≤ 2","6TCE220M","7.3x4.3(D)",1.8,null,1.9,6.3,220,25,2400,"45°C",1.8,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",2.4,0.1,138.6,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 220","≤ 2","6TPE220MAZB","3.5x2.8(B)",1.9,null,2,6.3,220,35,1400,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.4,0.1,138.6,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE220MAZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 220","≤ 2","6TPE220MZB","3.5x2.8(B)",1.9,null,2,6.3,220,35,1350,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.35,0.08,138.6,2000,0,"B2",-55,105,"→6TPE220MAZB",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE220MZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 220","≤ 2","6TPE220MW","7.3x4.3(D)",1.8,null,1.9,6.3,220,40,1850,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.85,0.1,138.6,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE220MW","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THB","No","≤  6.3","≤ 220","≤ 3","6THB220ML","7.3x4.3(D)",2.8,null,3,6.3,220,40,2000,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(4V)","125°C 1000H(4V)",2,"100kHz","10MHz",2,0.1,138.6,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6THB220ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 220","≤ 2","6TPE220MVB","3.5x2.8(B)",1.9,null,2,6.3,220,45,1150,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.1499999999999999,0.08,138.6,2000,0,"B2",-55,105,"→6TPE220MAZB",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE220MVB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤  6.3","≤ 220","≤ 3","6TPB220MTL","7.3x4.3(D)",2.8,null,3,6.3,220,50,1750,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.75,0.1,138.6,2500,0,"D3L",-55,105,"→6TPE220M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPB220MTL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 220","≤ 2","6TPE220MBB","3.5x2.8(B)",1.9,null,2,6.3,220,70,950,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",0.95,0.08,138.6,2000,0,"B2",-55,105,"→6TPE220MAZB",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE220MBB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  6.3","≤ 330","≤ 3","6TPF330M9L","7.3x4.3(D)",2.8,null,3,6.3,330,9,3900,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.9,0.1,207.9,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPF330M9L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 330","≤ 3","6TPE330MA9EL","7.3x4.3(D)",2.8,null,3,6.3,330,9,3900,"45°C",2.2999999999999998,"-55 to 105","_85°C 1000H","-",2,"500kHz","10MHz",3.9,0.1,207.9,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE330MA9EL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  6.3","≤ 330","≤ 3","6TCF330M9L","7.3x4.3(D)",2.8,null,3,6.3,330,9,3900,"45°C",2,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",3.9,0.1,207.9,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCF330M9L","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  6.3","≤ 330","≤ 3","6TPF330MAL","7.3x4.3(D)",2.8,null,3,6.3,330,10,3650,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.65,0.1,207.9,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPF330MAL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 330","≤ 3","6TPE330MFL","7.3x4.3(D)",2.8,null,3,6.3,330,15,3100,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.1,0.1,207.9,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE330MFL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 330","≤ 3","6TCE330MFL","7.3x4.3(D)",2.8,null,3,6.3,330,15,3100,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",3.1,0.1,207.9,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE330MFL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 330","≤ 3","6TPE330MIL","7.3x4.3(D)",2.8,null,3,6.3,330,18,2800,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,207.9,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE330MIL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 330","≤ 3","6TCE330MIL","7.3x4.3(D)",2.8,null,3,6.3,330,18,2800,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",2.8,0.1,207.9,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE330MIL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 330","≤ 2","6TPE330MAP","7.3x4.3(D)",1.8,null,1.9,6.3,330,25,2400,"45°C",1.8,"-55 to 105","_85°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,207.9,3000,0,"D2E",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE330MAP","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 330","≤ 3","6TPE330ML","7.3x4.3(D)",2.8,null,3,6.3,330,25,2400,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,207.9,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE330ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤  6.3","≤ 330","≤ 3","6TAE330ML","7.3x4.3(D)",2.8,null,3,6.3,330,25,2400,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,207.9,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TAE330ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 330","≤ 3","6TCE330ML","7.3x4.3(D)",2.8,null,3,6.3,330,25,2400,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",2.4,0.1,207.9,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE330ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤  6.3","≤ 330","≤ 3","6TPB330MAL","7.3x4.3(D)",2.8,null,3,6.3,330,40,2000,"45°C",2.2999999999999998,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",2,0.1,207.9,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPB330MAL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤  6.3","≤ 330","≤ 3","6TPB330ML","7.3x4.3(D)",2.8,null,3,6.3,330,40,2000,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2,0.1,207.9,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPB330ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤  6.3","≤ 330","≤ 4","6TPB330M","7.3x4.3(D)",3.8,null,4,6.3,330,40,3000,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3,0.1,207.9,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPB330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THB","No","≤  6.3","≤ 330","≤ 4","6THB330M","7.3x4.3(D)",3.8,null,4,6.3,330,40,3000,"45°C",2.6,"-55 to 125","125°C 1000H(4V)","125°C 1000H(4V)",2,"100kHz","10MHz",3,0.1,207.9,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6THB330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤  6.3","≤ 330","≤ 3","6TPB330MVL","7.3x4.3(D)",2.8,null,3,6.3,330,45,1850,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.85,0.1,207.9,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPB330MVL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  6.3","≤ 470","≤ 4","6TPF470MAH","7.3x4.3(D)",3.8,null,4,6.3,470,10,4400,"45°C",2.5,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",4.4000000000000004,0.1,296.10000000000002,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPF470MAH","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤  6.3","≤ 470","≤ 4","6TCF470MAH","7.3x4.3(D)",3.8,null,4,6.3,470,10,4400,"45°C",2.5,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",4.4000000000000004,0.1,296.10000000000002,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCF470MAH","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤  6.3","≤ 470","≤ 4","6TPF470MFH","7.3x4.3(D)",3.8,null,4,6.3,470,15,3550,"45°C",2.5,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.55,0.1,296.10000000000002,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPF470MFH","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 470","≤ 4","6TPE470MI","7.3x4.3(D)",3.8,null,4,6.3,470,18,3500,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.5,0.15,296.10000000000002,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE470MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 470","≤ 4","6TCE470MI","7.3x4.3(D)",3.8,null,4,6.3,470,18,3500,"45°C",2.6,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",3.5,0.15,296.10000000000002,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE470MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 470","≤ 4","6TPE470M","7.3x4.3(D)",3.8,null,4,6.3,470,25,3000,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3,0.15,296.10000000000002,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE470M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 470","≤ 4","6TCE470M","7.3x4.3(D)",3.8,null,4,6.3,470,25,3000,"45°C",2.6,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",3,0.15,296.10000000000002,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE470M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤  6.3","≤ 470","≤ 4","6TPB470M","7.3x4.3(D)",3.8,null,4,6.3,470,35,3000,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3,0.15,296.10000000000002,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPB470M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 470","≤ 4","6TPE470MZ","7.3x4.3(D)",3.8,null,4,6.3,470,35,2500,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.5,0.1,296.10000000000002,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE470MZ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THB","No","≤  6.3","≤ 470","≤ 4","6THB470M","7.3x4.3(D)",3.8,null,4,6.3,470,35,3000,"45°C",2.6,"-55 to 125","125°C 1000H(4V)","125°C 1000H(4V)",2,"100kHz","10MHz",3,0.15,296.10000000000002,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6THB470M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 470","≤ 4","6TPE470MW","7.3x4.3(D)",3.8,null,4,6.3,470,40,2350,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.35,0.1,296.10000000000002,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE470MW","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 680","≤ 4","6TPE680MI","7.3x4.3(D)",3.8,null,4,6.3,680,18,3500,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.5,0.15,428.4,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE680MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 680","≤ 4","6TCE680MI","7.3x4.3(D)",3.8,null,4,6.3,680,18,3500,"45°C",2.6,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",3.5,0.15,428.4,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE680MI","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤  6.3","≤ 680","≤ 4","6TPE680M","7.3x4.3(D)",3.8,null,4,6.3,680,25,3000,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3,0.15,428.4,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TPE680M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤  6.3","≤ 680","≤ 4","6TCE680M","7.3x4.3(D)",3.8,null,4,6.3,680,25,3000,"45°C",2.6,"-55 to 125","125°C 1000H(5V)","125°C 1000H(5V)",2,"100kHz","10MHz",3,0.15,428.4,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/6TCE680M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤ 10","≤ 100","≤ 2","8TPE100MAZB","3.5x2.8(B)",1.9,null,2,8,100,35,1400,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,80,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/8TPE100MAZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤ 10","≤  33","≤ 2","10TPB33M","3.5x2.8(B)",1.9,null,2,10,33,70,1100,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.1000000000000001,0.08,33,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPB33M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤ 10","≤  47","≤ 2","10TPE47MAZB","3.5x2.8(B)",1.9,null,2,10,47,35,1400,"45°C",1.3,"-55 to 105","_85°C 1000H","-",2,"100kHz","10MHz",1.4,0.08,47,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPE47MAZB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤ 10","≤  47","≤ 2","10TAB47M","3.5x2.8(B)",1.9,null,2,10,47,70,1100,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.1000000000000001,0.08,47,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TAB47M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤ 10","≤  47","≤ 2","10TPB47M","3.5x2.8(B)",1.9,null,2,10,47,70,1100,"45°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1.1000000000000001,0.08,47,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPB47M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TV","Yes","≤ 10","≤  68","≤ 2","10TVE68M","7.3x4.3(D)",1.8,null,1.9,10,68,25,2400,"45°C",1.8,"-55 to 125","105°C 2000H","125°C 1000H(6.3V)",2,"100kHz","10MHz",2.4,0.1,68,3000,0,"D2E",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TVE68M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤ 10","≤  68","≤ 2","10TPE68MW","7.3x4.3(D)",1.8,null,1.9,10,68,40,1850,"45°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.85,0.1,68,3000,0,"D2E",-55,105,"→10TPC100M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPE68MW","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THC","No","≤ 10","≤  68","≤ 2","10THC68M","7.3x4.3(D)",1.9,null,2,10,68,45,1700,"45°C",2,"-55 to 125","125°C 1000H(6.3V)","125°C 1000H(6.3V)",2,"100kHz","10MHz",1.7,0.1,68,3000,0,"D2",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10THC68M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPC","No","≤ 10","≤  68","≤ 2","10TPC68MM","7.3x4.3(D)",1.9,null,2,10,68,60,1450,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.45,0.1,68,3000,0,"D2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPC68MM","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPC","No","≤ 10","≤  68","≤ 2","10TPC68ME","7.3x4.3(D)",1.9,null,2,10,68,100,1100,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.1000000000000001,0.1,68,3000,0,"D2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPC68ME","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPC","No","≤ 10","≤ 100","≤ 2","10TPC100M","7.3x4.3(D)",1.9,null,2,10,100,45,1700,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.7,0.1,100,3000,0,"D2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPC100M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPC","No","≤ 10","≤ 100","≤ 2","10TPC100MT","7.3x4.3(D)",1.9,null,2,10,100,50,1600,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.6,0.1,100,3000,0,"D2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPC100MT","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPC","No","≤ 10","≤ 100","≤ 2","10TPC100MG","7.3x4.3(D)",1.9,null,2,10,100,55,1500,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.5,0.1,100,3000,0,"D2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPC100MG","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPF","No","≤ 10","≤ 150","≤ 3","10TPF150ML","7.3x4.3(D)",2.8,null,3,10,150,15,3600,"45°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3.6,0.1,150,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPF150ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCF","No","≤ 10","≤ 150","≤ 3","10TCF150ML","7.3x4.3(D)",2.8,null,3,10,150,15,3600,"45°C",2,"-55 to 125","125°C 1000H(8V)","125°C 1000H(8V)",2,"100kHz","10MHz",3.6,0.1,150,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TCF150ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤ 10","≤ 150","≤ 3","10TAE150ML","7.3x4.3(D)",2.8,null,3,10,150,25,2400,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,150,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TAE150ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤ 10","≤ 150","≤ 3","10TPE150MPL","7.3x4.3(D)",2.8,null,3,10,150,25,2400,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,150,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPE150MPL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TV","Yes","≤ 10","≤ 150","≤ 3","10TVE150ML","7.3x4.3(D)",2.8,null,3,10,150,25,2400,"45°C",2.2999999999999998,"-55 to 125","105°C 2000H","125°C 1000H(6.3V)",2,"100kHz","10MHz",2.4,0.1,150,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TVE150ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤ 10","≤ 150","≤ 3","10TPB150ML","7.3x4.3(D)",2.8,null,3,10,150,40,2000,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2,0.1,150,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPB150ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤ 10","≤ 150","≤ 3","10TPB150MGL","7.3x4.3(D)",2.8,null,3,10,150,55,1700,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.7,0.1,150,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPB150MGL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤ 10","≤ 220","≤ 3","10TPE220MIL","7.3x4.3(D)",2.8,null,3,10,220,18,2800,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,220,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPE220MIL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤ 10","≤ 220","≤ 3","10TCE220MIL","7.3x4.3(D)",2.8,null,3,10,220,18,2800,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(8V)","125°C 1000H(8V)",2,"100kHz","10MHz",2.8,0.1,220,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TCE220MIL","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤ 10","≤ 220","≤ 3","10TPE220ML","7.3x4.3(D)",2.8,null,3,10,220,25,2400,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,220,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPE220ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TA","Yes","≤ 10","≤ 220","≤ 3","10TAE220ML","7.3x4.3(D)",2.8,null,3,10,220,25,2400,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.4,0.1,220,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TAE220ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤ 10","≤ 220","≤ 3","10TCE220ML","7.3x4.3(D)",2.8,null,3,10,220,25,2400,"45°C",2.2999999999999998,"-55 to 125","125°C 1000H(8V)","125°C 1000H(8V)",2,"100kHz","10MHz",2.4,0.1,220,2500,0,"D3L",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TCE220ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤ 10","≤ 220","≤ 3","10TPB220ML","7.3x4.3(D)",2.8,null,3,10,220,40,2000,"45°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2,0.1,220,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPB220ML","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤ 10","≤ 220","≤ 4","10TPB220M","7.3x4.3(D)",3.8,null,4,10,220,40,3000,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3,0.1,220,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPB220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THB","No","≤ 10","≤ 220","≤ 4","10THB220M","7.3x4.3(D)",3.8,null,4,10,220,40,3000,"45°C",2.6,"-55 to 125","125°C 1000H(6.3V)","125°C 1000H(6.3V)",2,"100kHz","10MHz",3,0.1,220,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10THB220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPE","No","≤ 10","≤ 330","≤ 4","10TPE330M","7.3x4.3(D)",3.8,null,4,10,330,25,3000,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3,0.1,330,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPE330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TCE","No","≤ 10","≤ 330","≤ 4","10TCE330M","7.3x4.3(D)",3.8,null,4,10,330,25,3000,"45°C",2.6,"-55 to 125","125°C 1000H(8V)","125°C 1000H(8V)",2,"100kHz","10MHz",3,0.1,330,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TCE330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤ 10","≤ 330","≤ 4","10TPB330M","7.3x4.3(D)",3.8,null,4,10,330,35,3000,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",3,0.1,330,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPB330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","THB","No","≤ 10","≤ 330","≤ 4","10THB330M","7.3x4.3(D)",3.8,null,4,10,330,35,3000,"45°C",2.6,"-55 to 125","125°C 1000H(6.3V)","125°C 1000H(6.3V)",2,"100kHz","10MHz",3,0.1,330,2000,0,"D4",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10THB330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TPB","No","≤ 10","≤ 330","≤ 4","10TPB330MW","7.3x4.3(D)",3.8,null,4,10,330,40,2800,"45°C",2.6,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",2.8,0.1,330,2000,0,"D4",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/10TPB330MW","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPB.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  15","≤ 2","16TQC15M","3.5x2.8(B)",1.9,null,2,16,15,90,1000,"105°C",1.3,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1,0.1,72,2000,0,"B2",-55,105,"→25TQC15MB",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC15M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  22","≤ 2","16TQC22MYFB","3.5x2.8(B)",1.9,null,2,16,22,90,1000,"105°C",1.3,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1,0.1,105.6,2000,0,"B2",-55,105,"→16TQC33MB2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC22MYFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  33","≤ 2","16TQC33MYFD","7.3x4.3(D)",1.9,null,2,16,33,70,1400,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,52.8,3000,0,"D2",-55,105,"→20TQC33MD2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC33MYFD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  33","≤ 2","16TQC33MYFB","3.5x2.8(B)",1.9,null,2,16,33,90,1000,"105°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",1,0.1,158.4,2000,0,"B2",-55,105,"→16TQC33MB2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC33MYFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  33","≤ 2","16TQC33MB2","3.5x2.8(B)",1.9,null,2,16,33,90,1000,"105°C",1.3,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1,0.1,158.4,2000,0,"B2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC33MB2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 16","≤  33","≤ 2","16TDC33MYFB","3.5x2.8(B)",1.9,null,2,16,33,90,1000,"105°C",1.3,"-55 to 125","125°C 1000H(12.8V)","125°C 1000H(12.8V)",2,"100kHz","10MHz",1,0.1,158.4,2000,0,"B2",-55,125,"→16TDC33MB2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TDC33MYFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 16","≤  33","≤ 2","16TDC33MB2","3.5x2.8(B)",1.9,null,2,16,33,90,1000,"105°C",1.3,"-55 to 125","125°C 1000H(12.8V)","125°C 1000H(12.8V)",2,"100kHz","10MHz",1,0.1,158.4,2000,0,"B2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TDC33MB2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  47","≤ 1.5","16TQC47MYFT","7.3x4.3(D)",1.4,null,1.5,16,47,55,1500,"105°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.5,0.1,75.2,3000,0,"D15",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC47MYFT","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  47","≤ 2","16TQC47MYFD","7.3x4.3(D)",1.9,null,2,16,47,55,1450,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.45,0.1,75.2,3000,0,"D2",-55,105,"→16TQC47MD2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC47MYFD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  47","≤ 2","16TQC47MBD","7.3x4.3(D)",1.9,null,2,16,47,70,1250,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.25,0.1,75.2,3000,0,"D2",-55,105,"→16TQC47MBD2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC47MBD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  47","≤ 2","16TQC47MD2","7.3x4.3(D)",1.9,null,2,16,47,55,1450,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.45,0.1,75.2,3000,0,"D2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC47MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 16","≤  47","≤ 2","16TDC47MD2","7.3x4.3(D)",1.9,null,2,16,47,55,1450,"105°C",2,"-55 to 125","125°C 1000H(12.8V)","-",2,"100kHz","10MHz",1.45,0.1,75.2,3000,0,"D2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TDC47MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  47","≤ 2","16TQC47MBD2","7.3x4.3(D)",1.9,null,2,16,47,70,1250,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.25,0.1,75.2,3000,0,"D2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC47MBD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 16","≤  47","≤ 2","16TDC47MBD2","7.3x4.3(D)",1.9,null,2,16,47,70,1250,"105°C",2,"-55 to 125","125°C 1000H(12.8V)","-",2,"100kHz","10MHz",1.25,0.1,75.2,3000,0,"D2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TDC47MBD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  47","≤ 2","16TQC47MYFB","3.5x2.8(B)",1.9,null,2,16,47,90,1000,"105°C",1.3,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1,0.1,75.2,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC47MYFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  68","≤ 2","16TQC68MYF","7.3x4.3(D)",1.9,null,2,16,68,50,1500,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.5,0.1,108.8,3000,0,"D2",-55,105,"→16TQC68MD2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC68MYF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤  68","≤ 2","16TQC68MD2","7.3x4.3(D)",1.9,null,2,16,68,50,1500,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.5,0.1,108.8,3000,0,"D2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC68MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 16","≤  68","≤ 2","16TDC68MD2","7.3x4.3(D)",1.9,null,2,16,68,50,1500,"105°C",2,"-55 to 125","125°C 1000H(12.8V)","-",2,"100kHz","10MHz",1.5,0.1,108.8,3000,0,"D2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TDC68MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤ 100","≤ 2","16TQC100MYF","7.3x4.3(D)",1.9,null,2,16,100,50,1800,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.8,0.1,160,3000,0,"D2",-55,105,"→16TQC100MD2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC100MYF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤ 100","≤ 2","16TQC100MD2","7.3x4.3(D)",1.9,null,2,16,100,50,1800,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.8,0.1,160,3000,0,"D2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC100MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 16","≤ 100","≤ 2","16TDC100MD2","7.3x4.3(D)",1.9,null,2,16,100,50,1800,"105°C",2,"-55 to 125","125°C 1000H(12.8V)","-",2,"100kHz","10MHz",1.8,0.1,160,3000,0,"D2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TDC100MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤ 100","≤ 2","16TDC100MYF","7.3x4.3(D)",1.9,null,2,16,100,50,1800,"105°C",2,"-55 to 105","125°C 1000H(12.8V)","125°C 1000H(12.8V)",2,"100kHz","10MHz",1.8,0.1,160,3000,0,"D2",-55,105,"→16TDC100MD2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TDC100MYF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤ 150","≤ 3","16TQC150MYF","7.3x4.3(D)",2.8,null,3,16,150,50,1800,"105°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.8,0.1,240,2500,0,"D3L",-55,105,"→16TQC150MD3",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC150MYF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤ 150","≤ 3","16TQC150MD3","7.3x4.3(D)",2.8,null,3,16,150,50,1800,"105°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.8,0.1,240,2500,0,"D3L",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC150MD3","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 16","≤ 150","≤ 3","16TDC150MYF","7.3x4.3(D)",2.8,null,3,16,150,50,1800,"105°C",2.2999999999999998,"-55 to 125","125°C 1000H(12.8V)","125°C 1000H(12.8V)",2,"100kHz","10MHz",1.8,0.1,240,2500,0,"D3L",-55,125,"→16TDC150MD3",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TDC150MYF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 16","≤ 150","≤ 3","16TDC150MD3","7.3x4.3(D)",2.8,null,3,16,150,50,1800,"105°C",2.2999999999999998,"-55 to 125","125°C 1000H(12.8V)","125°C 1000H(12.8V)",2,"100kHz","10MHz",1.8,0.1,240,2500,0,"D3L",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TDC150MD3","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤ 150","≤ 2","1CTQC15173F1","7.3x4.3(D)",1.9,null,2,16,150,70,1500,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.5,0.15,240,3000,0,"D2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/1CTQC15173F1","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 16","≤ 220","≤ 3","16TQC220MD3","7.3x4.3(D)",2.8,null,3,16,220,50,1750,"105°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.75,0.1,352,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TQC220MD3","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 16","≤ 220","≤ 3","16TDC220MD3","7.3x4.3(D)",2.8,null,3,16,220,50,1800,"105°C",2.2999999999999998,"-55 to 125","125°C 1000H(12.8V)","125°C 1000H(12.8V)",2,"100kHz","10MHz",1.8,0.1,240,2500,0,"D3L",-55,125,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/16TDC220MD3","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤  22","≤ 2","20TQC22MYFB","3.5x2.8(B)",1.9,null,2,20,22,90,1000,"105°C",1.3,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1,0.1,132,2000,0,"B2",-55,105,"→20TQC22MB2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC22MYFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤  22","≤ 2","20TQC22MB2","3.5x2.8(B)",1.9,null,2,20,22,90,1000,"105°C",1.3,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1,0.1,132,2000,0,"B2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC22MB2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤  22","≤ 2","20TQC22MQD","7.3x4.3(D)",1.9,null,2,20,22,90,1200,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.2,0.1,44,3000,0,"D2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC22MQD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 20","≤  22","≤ 2","20TDC22MYFB","3.5x2.8(B)",1.9,null,2,20,22,90,1000,"105°C",1.3,"-55 to 125","125°C 1000H(16V)","125°C 1000H(16V)",2,"100kHz","10MHz",1,0.1,132,2000,0,"B2",-55,125,"→20TDC22MB2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TDC22MYFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 20","≤  22","≤ 2","20TDC22MB2","3.5x2.8(B)",1.9,null,2,20,22,90,1000,"105°C",1.3,"-55 to 125","125°C 1000H(16V)","125°C 1000H(16V)",2,"100kHz","10MHz",1,0.1,132,2000,0,"B2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TDC22MB2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤  33","≤ 2","20TQC33MYFD","7.3x4.3(D)",1.9,null,2,20,33,60,1400,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,66,3000,0,"D2",-55,105,"→20TQC33MD2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC33MYFD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤  33","≤ 2","20TQC33MD2","7.3x4.3(D)",1.9,null,2,20,33,60,1400,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,66,3000,0,"D2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC33MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 20","≤  33","≤ 2","20TDC33MD2","7.3x4.3(D)",1.9,null,2,20,33,60,1400,"105°C",2,"-55 to 125","125°C 1000H(16V)","-",2,"100kHz","10MHz",1.4,0.1,66,3000,0,"D2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TDC33MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤  33","≤ 2","20TQC33MYFB","3.5x2.8(B)",1.9,null,2,20,33,100,900,"105°C",1.3,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",0.9,0.1,198,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC33MYFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤  47","≤ 1.5","20TQC47MYFT","7.3x4.3(D)",1.4,null,1.5,20,47,55,1500,"105°C",1.8,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.5,0.1,94,3000,0,"D15",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC47MYFT","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤  47","≤ 2","20TQC47MYF","7.3x4.3(D)",1.9,null,2,20,47,55,1450,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.45,0.1,94,3000,0,"D2",-55,105,"→20TQC47MD2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC47MYF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤  47","≤ 2","20TQC47MD2","7.3x4.3(D)",1.9,null,2,20,47,55,1450,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.45,0.1,94,3000,0,"D2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC47MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 20","≤  47","≤ 2","20TDC47MD2","7.3x4.3(D)",1.9,null,2,20,47,55,1450,"105°C",2,"-55 to 125","125°C 1000H(16V)","-",2,"100kHz","10MHz",1.45,0.1,94,3000,0,"D2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TDC47MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤ 100","≤ 3","20TQC100MYF","7.3x4.3(D)",2.8,null,3,20,100,55,1700,"105°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.7,0.1,200,2500,0,"D3L",-55,105,"→20TQC100MD3",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC100MYF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤ 100","≤ 3","20TQC100MD3","7.3x4.3(D)",2.8,null,3,20,100,55,1700,"105°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.7,0.1,200,2500,0,"D3L",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC100MD3","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 20","≤ 100","≤ 3","20TDC100MYF","7.3x4.3(D)",2.8,null,3,20,100,55,1700,"105°C",2.2999999999999998,"-55 to 125","125°C 1000H(16V)","125°C 1000H(16V)",2,"100kHz","10MHz",1.7,0.1,200,2500,0,"D3L",-55,125,"→20TDC100MD3",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TDC100MYF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 20","≤ 100","≤ 3","20TDC100MD3","7.3x4.3(D)",2.8,null,3,20,100,55,1700,"105°C",2.2999999999999998,"-55 to 125","125°C 1000H(16V)","125°C 1000H(16V)",2,"100kHz","10MHz",1.7,0.1,200,2500,0,"D3L",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TDC100MD3","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 20","≤ 100","≤ 2","20TQC100MD2","7.3x4.3(D)",1.9,null,2,20,100,100,1250,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.25,0.1,200,3000,0,"D2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/20TQC100MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  10","≤ 2","25TQC10MEB","3.5x2.8(B)",1.9,null,2,25,10,100,900,"105°C",1.3,"-55 to 105","105°C 1000H","-",2,"100kHz","10MHz",0.9,0.08,25,2000,0,"B2",-55,105,"→25TQC15MB",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC10MEB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  15","≤ 2","25TQC15MYFD","7.3x4.3(D)",1.9,null,2,25,15,90,1000,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1,0.1,38,3000,0,"D2",-55,105,"→25TQC15MD2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC15MYFD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  15","≤ 2","25TQC15MD2","7.3x4.3(D)",1.9,null,2,25,15,90,1000,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1,0.1,37.5,3000,0,"D2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC15MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 25","≤  15","≤ 2","25TDC15MD2","7.3x4.3(D)",1.9,null,2,25,15,90,1000,"105°C",2,"-55 to 125","125°C 1000H(20V)","-",2,"100kHz","10MHz",1,0.1,37.5,3000,0,"D2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TDC15MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  15","≤ 2","25TQC15MYFB","3.5x2.8(B)",1.9,null,2,25,15,100,900,"105°C",1.3,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",0.9,0.1,112.5,2000,0,"B2",-55,105,"→25TQC15MB",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC15MYFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  15","≤ 2","25TQC15MB","3.5x2.8(B)",1.9,null,2,25,15,100,900,"105°C",1.3,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",0.9,0.1,112.5,2000,0,"B2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC15MB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 25","≤  15","≤ 2","25TDC15MYFB","3.5x2.8(B)",1.9,null,2,25,15,100,900,"105°C",1.3,"-55 to 125","125°C 1000H(20V)","125°C 1000H(20V)",2,"100kHz","10MHz",0.9,0.1,112.5,2000,0,"B2",-55,125,"→25TDC15MB",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TDC15MYFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 25","≤  15","≤ 2","25TDC15MB","3.5x2.8(B)",1.9,null,2,25,15,100,900,"105°C",1.3,"-55 to 125","125°C 1000H(20V)","125°C 1000H(20V)",2,"100kHz","10MHz",0.9,0.1,112.5,2000,0,"B2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TDC15MB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  22","≤ 2","25TQC22MYFD","7.3x4.3(D)",1.9,null,2,25,22,60,1400,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,55,3000,0,"D2",-55,105,"→25TQC22MD2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC22MYFD","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  22","≤ 2","25TQC22MD2","7.3x4.3(D)",1.9,null,2,25,22,60,1400,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,55,3000,0,"D2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC22MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 25","≤  22","≤ 2","25TDC22MD2","7.3x4.3(D)",1.9,null,2,25,22,60,1400,"105°C",2,"-55 to 125","125°C 1000H(20V)","-",2,"100kHz","10MHz",1.4,0.1,55,3000,0,"D2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TDC22MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  22","≤ 2","25TQC22MYFB","3.5x2.8(B)",1.9,null,2,25,22,100,1100,"105°C",1.3,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.1000000000000001,0.1,55,2000,0,"B2",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC22MYFB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  33","≤ 2","25TQC33MYF","7.3x4.3(D)",1.9,null,2,25,33,60,1400,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,82.5,3000,0,"D2",-55,105,"→25TQC33MD2",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC33MYF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  33","≤ 2","25TQC33MD2","7.3x4.3(D)",1.9,null,2,25,33,60,1400,"105°C",2,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,82.5,3000,0,"D2",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC33MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg","100kHz"]
[null,null,"後付けで、CV順じゃない（今回だけ）",null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 25","≤  33","≤ 2","25TDC33MD2","7.3x4.3(D)",1.9,null,2,25,33,60,1400,"105°C",2,"-55 to 125","125°C 1000H(20V)","-",2,"100kHz","10MHz",1.4,0.1,82.5,3000,0,"D2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TDC33MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg"]
[null,null,"後付けで、CV順じゃない（今回だけ）",null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  68","≤ 3","25TQC68MYF","7.3x4.3(D)",2.8,null,3,25,68,70,1400,"105°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,170,2500,0,"D3L",-55,105,"→25TQC68MD3",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC68MYF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg"]
[null,null,"後付けで、CV順じゃない（今回だけ）",null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤  68","≤ 3","25TQC68MD3","7.3x4.3(D)",2.8,null,3,25,68,70,1400,"105°C",2.2999999999999998,"-55 to 105","105°C 2000H","-",2,"100kHz","10MHz",1.4,0.1,170,2500,0,"D3L",-55,105,"Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC68MD3","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg"]
[null,null,"後付けで、CV順じゃない（今回だけ）",null,"Open","NRND","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 25","≤  68","≤ 3","25TDC68MYF","7.3x4.3(D)",2.8,null,3,25,68,70,1400,"105°C",2.2999999999999998,"-55 to 125","125°C 1000H(20V)","125°C 1000H(20V)",2,"100kHz","10MHz",1.4,0.1,170,2500,0,"D3L",-55,125,"→25TDC68MD3",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TDC68MYF","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg"]
[null,null,"後付けで、CV順じゃない（今回だけ）",null,"Open","Std","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TQC","No","≤ 25","≤ 100","≤ 3","25TQC100MD3","7.3x4.3(D)",2.8,null,3,25,100,60,1600,"105°C",2.2999999999999998,"-55 to 105","105°C 2000H",0,2,"100kHz","10MHz",1.6,0.1,250,2500,0,"D3L",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/25TQC100MD3","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg"]
[null,null,"後付けで、CV順じゃない（今回だけ）",null,"Open","New","Panasonic","Japan","SMD","Mold","Polymer Ta","POSCAP","TDC","No","≤ 35","≤  15","≤ 2","35TDC15MD2","7.3x4.3(D)",1.9,null,2,35,15,150,900,"105°C",2,"-55 to 125","125°C 1000H(28V)","-",2,"100kHz","10MHz",0.9,0.1,52.5,3000,0,"D2",-55,125,"High Rel. / Reflow upgrade",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/POSCAP/models/35TDC15MD2","https://industrial.panasonic.com/content/data/CP/pictures/lineup-TQC.jpg"]
[null,null,"後付けで、CV順じゃない（今回だけ）",null,"Open","NRND","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPB","No","≤  2.5","≤ 120","≤ 5","2R5SVPB120M","dia. 6.3",4.9000000000000004,null,5,2.5,120,40,1670,"105°C",2.4,"-55 to 105","105°C 1000H","-",2,"100kHz","40MHz",1.67,0.12,120,1300,0,"C5",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/2R5SVPB120M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPE","No","≤  2.5","≤ 390","≤ 6","2R5SVPE390MX","dia. 5",5.9,null,6,2.5,390,10,3860,"105°C",2.1,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",3.86,0.12,700,1500,0,"B6",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/2R5SVPE390MX","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVT","No","≤  2.5","≤ 680","≤ 6.5","2R5SVT680MX","dia. 6.3",6.4,null,6.5,2.5,680,16,3500,"105°C",2.5,"-55 to 125","125°C 2000H","-",2,"100kHz","40MHz",3.5,0.12,850,1000,0,"C65",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/2R5SVT680MX","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPC","No","≤  2.5","≤1500","≤12","2R5SVPC1500M","dia. 8",11.9,null,12,2.5,1500,10,5150,"105°C",4.4000000000000004,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",5.15,0.15,750,400,0,"E12",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/2R5SVPC1500M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVT","No","≤  2.5","≤1500","≤12","2R5SVT1500M","dia. 8",11.9,null,12,2.5,1500,10,5150,"105°C",4.4000000000000004,"-55 to 125","125°C 2000H","-",2,"100kHz","40MHz",5.15,0.12,750,400,0,"E12",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/2R5SVT1500M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPA","No","≤  4","≤  68","≤ 6","4SVPA68MAA","dia. 5",5.9,null,6,4,68,30,1970,"105°C",2.1,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",1.97,0.12,300,1500,0,"B6",-55,105,"→4SVP68M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/4SVPA68MAA","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVQP","No","≤  4","≤ 150","≤ 6","4SVQP150M","dia. 6.3",5.9,null,6,4,150,40,1810,"105°C",2.7,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",1.81,0.12,300,1000,0,"C6",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/4SVQP150M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVT","No","≤  4","≤ 560","≤ 7","4SVT560M","dia. 8",6.9,null,7,4,560,22,3220,"105°C",4.3,"-55 to 125","125°C 2000H","-",2,"100kHz","40MHz",3.22,0.12,500,1000,0,"E7",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/4SVT560M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVT","No","≤  4","≤1500","≤12","4SVT1500M","dia. 8",11.9,null,12,4,1500,12,4700,"105°C",4.4000000000000004,"-55 to 125","125°C 2000H","-",2,"100kHz","40MHz",4.7,0.12,1200,400,0,"E12",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/4SVT1500M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPC","No","≤  6.3","≤ 100","≤ 6","6SVPC100MY","dia. 5",5.9,null,6,6.3,100,25,2150,"105°C",2.1,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",2.15,0.12,300,1500,0,"B6",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/6SVPC100MY","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPC","No","≤  6.3","≤ 220","≤ 6","6SVPC220MV","dia. 6.3",5.9,null,6,6.3,220,15,3160,"105°C",2.7,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",3.16,0.12,300,1000,0,"C6",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/6SVPC220MV","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPT","No","≤  6.3","≤ 330","≤ 6.5","6SVPT330M","dia. 6.3",6.4,null,6.5,6.3,330,15,3390,"105°C",2.5,"-55 to 105","105°C20000H","-",2,"100kHz","40MHz",3.39,0.12,415,1000,0,"C65",-55,105,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/6SVPT330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPS","No","≤  6.3","≤ 470","≤ 8","6SVPS470M","dia.10",7.9,null,8,6.3,470,20,4130,"105°C",5.2,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",4.13,0.12,592,500,0,"F8",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/6SVPS470M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVP","No","≤  6.3","≤ 820","≤13","6SVP820M","dia.10",12.6,null,12.7,6.3,820,12,5440,"105°C",5,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",5.44,0.15,775,400,0,"F12",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/6SVP820M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPS","No","≤ 10","≤  15","≤ 5.5","10SVPS15M","dia. 4",5.4,null,5.5,10,15,200,740,"105°C",2,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",0.74,0.1,75,2000,0,"A5",-55,105,"→16SVP15M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/10SVPS15M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPC","No","≤ 10","≤  68","≤ 6","10SVPC68MV","dia. 5",5.9,null,6,10,68,23,2540,"105°C",2.1,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",2.54,0.12,300,1500,0,"B6",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/10SVPC68MV","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPA","No","≤ 10","≤ 150","≤ 7","10SVPA150MAA","dia. 8",6.9,null,7,10,150,30,2760,"105°C",4.3,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",2.76,0.12,500,1000,0,"E7",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/10SVPA150MAA","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPS","No","≤ 10","≤ 330","≤ 8","10SVPS330M","dia.10",7.9,null,8,10,330,24,3770,"105°C",5.2,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",3.77,0.12,660,500,0,"F8",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/10SVPS330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPS","No","≤ 16","≤  39","≤ 6","16SVPS39M","dia. 6.3",5.9,null,6,16,39,24,2460,"105°C",2.7,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",2.46,0.12,300,1000,0,"C6",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SVPS39M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPC","No","≤ 16","≤  68","≤ 6","16SVPC68MV","dia. 6.3",5.9,null,6,16,68,25,2440,"105°C",2.7,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",2.44,0.12,300,1000,0,"C6",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SVPC68MV","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPF","No","≤ 16","≤  82","≤ 6","16SVPF82M","dia. 5",5.9,null,6,16,82,27,3000,"105°C",2.1,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",3,0.12,262,1500,0,"B6",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SVPF82M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPT","No","≤ 16","≤ 100","≤ 6.5","16SVPT100M","dia. 6.3",6.4,null,6.5,16,100,24,2490,"105°C",2.5,"-55 to 105","105°C20000H","-",2,"100kHz","40MHz",2.4900000000000002,0.12,300,1000,0,"C65",-55,105,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SVPT100M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVP","No","≤ 16","≤ 180","≤12","16SVP180M","dia. 8",11.9,null,12,16,180,20,3640,"105°C",4.4000000000000004,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",3.64,0.15,576,400,0,"E12",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SVP180M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPF","No","≤ 16","≤ 270","≤ 7","16SVPF270M","dia. 8",6.9,null,7,16,270,22,3300,"105°C",4.3,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",3.3,0.12,864,1000,0,"E7",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SVPF270M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPE","No","≤ 16","≤ 470","≤13","16SVPE470M","dia.10",12.6,null,12.7,16,470,10,6100,"105°C",5,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",6.1,0.12,1504,400,0,"F12",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SVPE470M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPG","No","≤ 16","≤ 680","≤12","16SVPG680M","dia. 8",11.9,null,12,16,680,8,6500,"105°C",4.4000000000000004,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",6.5,0.12,2176,400,0,"E12",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SVPG680M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPK","No","≤ 16","≤1200","≤13","16SVPK1200M","dia.10",12.6,null,12.7,16,1200,12,5400,"105°C",5,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",5.4,0.12,3840,400,0,"F12",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SVPK1200M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVP","No","≤ 20","≤  22","≤ 6","20SVP22M","dia. 6.3",5.9,null,6,20,22,60,1450,"105°C",2.7,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",1.45,0.1,88,1000,0,"C6",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/20SVP22M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPF","No","≤ 20","≤  56","≤ 6","20SVPF56MX","dia. 5",5.9,null,6,20,56,30,2800,"105°C",2.1,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",2.8,0.12,224,1500,0,"B6",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/20SVPF56MX","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVP","No","≤ 20","≤  68","≤ 8","20SVP68M","dia.10",7.9,null,8,20,68,40,2400,"105°C",5.2,"-55 to 105","105°C 2000H","-",2,"100kHz","40MHz",2.4,0.12,272,500,0,"F8",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/20SVP68M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPG","No","≤ 20","≤ 180","≤10","20SVPG180M","dia. 6.3",9.9,null,10,20,180,11,4700,"105°C",2.6,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",4.7,0.12,720,500,0,"C10",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/20SVPG180M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPT","No","≤ 20","≤ 390","≤12","20SVPT390M","dia. 8",11.9,null,12,20,390,14,4950,"105°C",4.4000000000000004,"-55 to 105","105°C20000H","-",2,"100kHz","40MHz",4.95,0.12,1560,400,0,"E12",-55,105,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/20SVPT390M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPG","No","≤ 20","≤ 680","≤13","20SVPG680M","dia.10",12.6,null,12.7,20,680,9,6200,"105°C",5,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",6.2,0.12,2720,400,0,"F12",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/20SVPG680M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVF","No","≤ 25","≤  47","≤ 6","25SVF47M","dia. 6.3",5.9,null,6,25,47,30,2800,"105°C",2.7,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",2.8,0.12,235,1000,0,"C6",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/25SVF47M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPF","No","≤ 25","≤ 100","≤ 7","25SVPF100M","dia. 8",6.9,null,7,25,100,24,3200,"105°C",4.3,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",3.2,0.12,500,1000,0,"E7",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/25SVPF100M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPT","No","≤ 25","≤ 180","≤12","25SVPT180M","dia. 8",11.9,null,12,25,180,16,4650,"105°C",4.4000000000000004,"-55 to 105","105°C20000H","-",2,"100kHz","40MHz",4.6500000000000004,0.12,900,400,0,"E12",-55,105,"High Rel.",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/25SVPT180M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVT","No","≤ 25","≤ 180","≤12","25SVT180M","dia. 8",11.9,null,12,25,180,16,4650,"105°C",4.4000000000000004,"-55 to 125","125°C 2000H","-",2,"100kHz","40MHz",4.6500000000000004,0.12,900,400,0,"E12",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/25SVT180M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPD","No","≤ 35","≤  18","≤ 8","35SVPD18M","dia.10",7.9,null,8,35,18,60,1800,"105°C",5.2,"-55 to 125","125°C 2000H","-",2,"100kHz","40MHz",1.8,0.1,126,500,0,"F8",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/35SVPD18M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPK","No","≤ 35","≤  47","≤ 6","35SVPK47M","dia. 6.3",5.9,null,6,35,47,27,2950,"105°C",2.7,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",2.95,0.12,329,1000,0,"C6",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/35SVPK47M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVPK","No","≤ 35","≤ 180","≤12","35SVPK180M","dia. 8",11.9,null,12,35,180,20,4000,"105°C",4.4000000000000004,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",4,0.12,1260,400,0,"E12",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/35SVPK180M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVT","No","≤ 50","≤  18","≤ 7","50SVT18M","dia. 8",6.9,null,7,50,18,35,2700,"105°C",4.3,"-55 to 125","125°C 2000H","-",2,"100kHz","40MHz",2.7,0.12,180,1000,0,"E7",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/50SVT18M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SVF","No","≤ 50","≤  68","≤13","50SVF68M","dia.10",12.6,null,12.7,50,68,20,4300,"105°C",5,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",4.3,0.12,680,400,0,"F12",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/50SVF68M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SXV","No","≤ 63","≤ 100","≤13","63SXV100M","dia.10",12.6,null,12.7,63,100,25,3280,"105°C",5,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",3.28,0.12,315,400,0,"F12",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/63SXV100M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SXV","No","≤ 80","≤  27","≤ 8","80SXV27MX","dia.10",7.9,null,8,80,27,55,2080,"105°C",4.7,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",2.08,0.12,108,500,0,"F8",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/80SXV27MX","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SXV","No","≤100","≤  15","≤12","100SXV15M","dia. 8",11.9,null,12,100,15,40,2350,"105°C",4.4000000000000004,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",2.35,0.12,75,400,0,"E12",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/100SXV15M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Polymer Al","OS-CON","SXV","No","≤100","≤  22","≤13","100SXV22M","dia.10",12.6,null,12.7,100,22,30,3000,"105°C",5,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",3,0.12,110,400,0,"F12",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/100SXV22M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SVPG.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEPC","No","≤  2.5","≤ 470","≤ 9","2SEPC470MZ","dia. 5",9,null,9,2.5,470,7,4180,"105°C",1.4,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",4.18,0.1,500,500,0,"B9",-55,105,"→2R5SVPC560M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/2SEPC470MZ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEPC","No","≤  2.5","≤ 820","≤ 9","2SEPC820MX","dia. 8",9,null,9,2.5,820,7,6100,"105°C",2.7,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",6.1,0.1,500,200,0,"E9",-55,105,"→2R5SVPC820M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/2SEPC820MX","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEP","No","≤  4","≤ 220","≤ 7","4SEP220M","dia. 8",7,null,7,4,220,35,2560,"105°C",2.8,"-55 to 105","105°C 3000H","-",2,"100kHz","40MHz",2.56,0.12,440,200,0,"E7",-55,105,"→4SVP220M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/4SEP220M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEQP","No","≤  4","≤ 680","≤ 8","4SEQP680M","dia.10",8,null,8,4,680,25,3700,"105°C",4.7,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",3.7,0.12,544,200,0,"F8",-55,125,"→4SVP680M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/4SEQP680M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEP","No","≤  6.3","≤ 330","≤ 8","6SEP330M","dia.10",8,null,8,6.3,330,25,3700,"105°C",4.7,"-55 to 105","105°C 3000H","-",2,"100kHz","40MHz",3.7,0.12,416,200,0,"F8",-55,105,"→6SVP330M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/6SEP330M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEPC","No","≤  6.3","≤ 680","≤13","6SEPC680M","dia.10",13,null,13,6.3,680,7,6640,"105°C",5.8,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",6.64,0.1,857,200,0,"F13",-55,105,"→20SVPK680M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/6SEPC680M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEQP","No","≤  6.3","≤ 820","≤13","6SEQP820M","dia.10",13,null,13,6.3,820,12,5440,"105°C",5.8,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",5.44,0.15,775,200,0,"F13",-55,125,"→6SVP820M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/6SEQP820M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEQP","No","≤ 10","≤ 270","≤ 8","10SEQP270M","dia.10",8,null,8,10,270,25,3700,"105°C",4.7,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",3.7,0.12,540,200,0,"F8",-55,125,"→10SVP270M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/10SEQP270M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEPC","No","≤ 16","≤ 100","≤ 9","16SEPC100MW","dia. 6.3",9,null,9,16,100,10,4680,"105°C",2,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",4.68,0.1,500,500,0,"C9",-55,105,"→16SVPC100M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SEPC100MW","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEPF","No","≤ 16","≤ 180","≤ 6","16SEPF180M","dia. 6.3",6,null,6,16,180,22,3300,"105°C",2.5,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",3.3,0.12,576,500,0,"C6",-55,105,"→16SVPF180M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SEPF180M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEF","No","≤ 16","≤ 270","≤ 7","16SEF270M","dia. 8",7,null,7,16,270,22,3300,"105°C",2.8,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",3.3,0.12,864,200,0,"E7",-55,125,"→16SVF270M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SEF270M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEF","No","≤ 16","≤1000","≤13","16SEF1000M","dia.10",13,null,13,16,1000,12,5400,"105°C",5.8,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",5.4,0.12,3200,200,0,"F13",-55,125,"→16SVF1000M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/16SEF1000M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEPF","No","≤ 20","≤ 120","≤ 6","20SEPF120M","dia. 6.3",6,null,6,20,120,25,3200,"105°C",2.5,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",3.2,0.12,480,500,0,"C6",-55,105,"→20SVF120M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/20SEPF120M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEF","No","≤ 20","≤ 390","≤12","20SEF390M","dia. 8",12,null,12,20,390,14,4950,"105°C",4.0999999999999996,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",4.95,0.12,1560,200,0,"E12",-55,125,"→20SVF390M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/20SEF390M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEPF","No","≤ 25","≤ 180","≤12","25SEPF180M","dia. 8",12,null,12,25,180,16,4650,"105°C",4.0999999999999996,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",4.6500000000000004,0.12,900,200,0,"E12",-55,105,"→25SVPF180M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/25SEPF180M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEQP","No","≤ 35","≤  18","≤12","32SEQP18M","dia. 8",12,null,12,32,18,50,2500,"105°C",4.0999999999999996,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",2.5,0.12,115,200,0,"E12",-55,125,"→35SVPD18M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/32SEQP18M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEF","No","≤ 35","≤  68","≤ 7","32SEF68M","dia. 8",7,null,7,32,68,25,3200,"105°C",2.8,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",3.2,0.1,435,200,0,"E7",-55,125,"→35SVPK82M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/32SEF68M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SEPF","No","≤ 35","≤ 120","≤13","35SEPF120M","dia.10",13,null,13,35,120,18,4400,"105°C",5.8,"-55 to 105","105°C 5000H","-",2,"100kHz","40MHz",4.4000000000000004,0.12,840,200,0,"F13",-55,105,"→35SVPF120M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/35SEPF120M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SXE","No","≤ 63","≤  18","≤ 7","63SXE18M","dia. 8",7,null,7,63,18,60,1100,"105°C",2.8,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",1.1000000000000001,0.12,56,200,0,"E7",-55,125,"→63SXV18M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/63SXE18M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SXE","No","≤ 80","≤  27","≤12","80SXE27M","dia. 8",12,null,12,80,27,35,2490,"105°C",4.0999999999999996,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",2.4900000000000002,0.12,108,200,0,"E12",-55,125,"→80SXV27M",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/80SXE27M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic","Japan","THD","Can","Polymer Al","OS-CON","SXE","No","≤100","≤  18","≤12","100SXE18MX","dia. 8",12,null,12,100,18,40,2350,"105°C",4.0999999999999996,"-55 to 125","125°C 1000H","-",2,"100kHz","40MHz",2.35,0.12,90,200,0,"E12",-55,125,"→100SXV18MX",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/OS-CON/models/100SXE18MX","https://industrial.panasonic.com/content/data/CP/pictures/lineup-SEPF.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 25","≤  47","≤ 6.5","EEHZA1E470P","dia. 6.3",5.8,null,6.1,25,47,50,1300,"105°C",2.6,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",1.3,0.14000000000000001,11.75,1000,0,"D",-55,105,"EEHZA1E470V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZA1E470P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZK","Yes","≤ 25","≤  47","≤ 6.5","EEHZK1E470R","dia. 5",5.8,null,6.1,25,47,80,850,"125°C",2.2999999999999998,"-55 to 125","125°C 4000H","-",2,"100kHz","10MHz",0.66,0.14000000000000001,11.75,1000,0,"C",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZK1E470R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 25","≤ 100","≤ 8","EEHZA1E101XP","dia. 6.3",7.7,null,8,25,100,30,2000,"105°C",2.8,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",2,0.14000000000000001,25,900,0,"D8",-55,105,"EEHZA1E101XV (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZA1E101XP","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","New","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZV","Yes","≤ 25","≤ 220","≤10.5","EEHZV1E221P","dia. 8",10.199999999999999,null,10.5,25,220,16,3900,"125°C",3.4,"-55 to 135","125°C 4000H / 135°C 4000H","-",2,"100kHz","10MHz",3.9,0.14000000000000001,55,500,0,"F",-55,135,"EEHZV1E221V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZV1E221P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 25","≤ 330","≤10.5","EEHZA1E331P","dia.10",10.199999999999999,null,10.5,25,330,20,2500,"105°C",4,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",2.5,0.14000000000000001,82.5,500,0,"G",-55,105,"EEHZA1E331V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZA1E331P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZK","Yes","≤ 25","≤ 470","≤10.5","EEHZK1E471P","dia.10",10.199999999999999,null,10.5,25,470,20,2800,"125°C",4,"-55 to 125","125°C 4000H","-",2,"100kHz","10MHz",2.8,0.14000000000000001,117.5,500,0,"G",-55,125,"EEHZK1E471V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZK1E471P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZUU","Yes","≤ 25","≤1000","≤17","EEHZU1E102UP","dia.10",16.5,null,16.8,25,1000,8,6100,"125°C",5.21,"-55 to 135","135°C 4000H","-",2,"100kHz","10MHz",6.1,0.14000000000000001,250,250,0,"G16",-55,135,"EEHZU1E102UV (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZU1E102UP","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 35","≤  33","≤ 6.5","EEHZA1V330P","dia. 6.3",5.8,null,6.1,35,33,60,1300,"105°C",2.6,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",1.3,0.12,11.55,1000,0,"D",-55,105,"EEHZA1V330V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZA1V330P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 35","≤ 100","≤10.5","EEHZA1V101P","dia. 8",10.199999999999999,null,10.5,35,100,27,2300,"105°C",3.4,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",2.2999999999999998,0.12,35,500,0,"F",-55,105,"EEHZA1V101V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZA1V101P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 35","≤ 150","≤10.5","EEHZA1V151P","dia. 8",10.199999999999999,null,10.5,35,150,27,2300,"105°C",3.4,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",2.2999999999999998,0.12,52.5,500,0,"F",-55,105,"EEHZA1V151V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZA1V151P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZKU","Yes","≤ 35","≤ 220","≤10.5","EEHZK1V221UP","dia. 8",10.199999999999999,null,10.5,35,220,27,2000,"125°C",3.4,"-55 to 125","125°C 4000H","-",2,"100kHz","10MHz",2,0.12,77,500,0,"F",-55,125,"EEHZK1V221UV (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZK1V221UP","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 35","≤ 270","≤10.5","EEHZA1V271P","dia.10",10.199999999999999,null,10.5,35,270,20,2500,"105°C",4,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",2.5,0.12,94.5,500,0,"G",-55,105,"EEHZA1V271V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZA1V271P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZKU","Yes","≤ 35","≤ 390","≤10.5","EEHZK1V391UP","dia.10",10.199999999999999,null,10.5,35,390,20,2800,"125°C",4,"-55 to 125","125°C 4000H","-",2,"100kHz","10MHz",2.8,0.12,136.5,500,0,"G",-55,125,"EEHZK1V391UV (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZK1V391UP","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 50","≤  10","≤ 6.5","EEHZA1H100R","dia. 5",5.8,null,6.1,50,10,120,750,"105°C",2.2999999999999998,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",0.75,0.1,5,1000,0,"C",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZA1H100R","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 50","≤  68","≤10.5","EEHZA1H680P","dia. 8",10.199999999999999,null,10.5,50,68,30,1800,"105°C",3.4,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",1.8,0.1,34,500,0,"F",-55,105,"EEHZA1H680V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZA1H680P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZF","Yes","≤ 50","≤ 100","≤10.5","EEHZF1H101P","dia.10",10.199999999999999,null,10.5,50,100,28,900,"150°C",4,"-55 to 150","150°C 1000H","-",2,"100kHz","10MHz",0.9,0.1,50,500,0,"G",-55,150,"EEHZF1H101V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZF1H101P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZU","Yes","≤ 50","≤ 220","≤17","EEHZU1H221P","dia.10",16.5,null,16.8,50,220,10,5200,"125°C",5.2,"-55 to 135","125°C 4000H / 135°C 4000H","-",2,"100kHz","10MHz",5.2,0.1,110,250,0,"G16",-55,135,"EEHZU1H221V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZU1H221P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 63","≤  33","≤10.5","EEHZA1J330P","dia. 8",10.199999999999999,null,10.5,63,33,40,1700,"105°C",3.4,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",1.7,0.08,20.7,500,0,"F",-55,105,"EEHZA1J330V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZA1J330P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZC","Yes","≤ 63","≤  33","≤10.5","EEHZC1J330P","dia. 8",10.199999999999999,null,10.5,63,33,40,1100,"125°C",3.4,"-55 to 125","125°C 4000H","-",2,"100kHz","10MHz",1.1000000000000001,0.08,20.7,500,0,"F",-55,125,"EEHZC1J330V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZC1J330P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZT","Yes","≤ 63","≤  56","≤10.5","EEHZT1J560P","dia.10",10.199999999999999,null,10.5,63,56,25,2800,"125°C",4,"-55 to 125","125°C 4000H / 135°C 4000H","-",2,"100kHz","10MHz",2.8,0.08,35.28,500,0,"G",-55,125,"EEHZT1J560V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZT1J560P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 63","≤  82","≤10.5","EEHZA1J820P","dia.10",10.199999999999999,null,10.5,63,82,30,1800,"105°C",4,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",1.8,0.08,51.66,500,0,"G",-55,105,"EEHZA1J820V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZA1J820P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZU","Yes","≤ 63","≤ 150","≤17","EEHZU1J151P","dia.10",16.5,null,16.8,63,150,10,5200,"125°C",5.2,"-55 to 135","125°C 4000H / 135°C 4000H","-",2,"100kHz","10MHz",5.2,0.08,94.5,250,0,"G16",-55,135,"EEHZU1J151V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZU1J151P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","SMD","Can","Hybrid Al","Hybrid","ZC","Yes","≤ 80","≤  47","≤10.5","EEHZC1K470P","dia.10",10.199999999999999,null,10.5,80,47,36,1360,"125°C",4,"-55 to 125","125°C 4000H","-",2,"100kHz","10MHz",1.36,0.08,37.6,500,0,"G",-55,125,"EEHZC1K470V (anti-vib.)",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHZC1K470P","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZK.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","THD","Can","Hybrid Al","Hybrid","ZE","Yes","≤ 25","≤ 220","≤10.5","EEHAZE1E221B","dia. 8",9.5,null,10.5,25,220,27,1600,"135°C",3.4,"-55 to 145","135°C 4000H / 145°C 2000H","-",2,"100kHz","10MHz",1.6,0.14000000000000001,55,1000,0,"F",-55,145,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHAZE1E221B","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZF-A.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","THD","Can","Hybrid Al","Hybrid","ZSU","Yes","≤ 25","≤ 680","≤13","EEHAZSE681UB","dia.10",11.7,null,12.7,25,680,14,3500,"125°C",4.88,"-55 to 125","125°C 4000H / 135°C 4000H","-",2,"100kHz","10MHz",3.5,0.14000000000000001,170,500,0,"G12",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHAZSE681UB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZSU-A.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","THD","Can","Hybrid Al","Hybrid","ZE","Yes","≤ 35","≤ 150","≤10.5","EEHAZE1V151B","dia. 8",9.5,null,10.5,35,150,27,1600,"135°C",3.4,"-55 to 145","135°C 4000H / 145°C 2000H","-",2,"100kHz","10MHz",1.6,0.12,52.5,1000,0,"F",-55,145,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHAZE1V151B","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZF-A.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","THD","Can","Hybrid Al","Hybrid","ZE","Yes","≤ 35","≤ 270","≤10.5","EEHAZE1V271B","dia.10",9.5,null,10.5,35,270,20,2000,"135°C",4,"-55 to 145","135°C 4000H / 145°C 2000H","-",2,"100kHz","10MHz",2,0.12,94.5,500,0,"G",-55,145,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHAZE1V271B","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZF-A.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","THD","Can","Hybrid Al","Hybrid","ZKU","Yes","≤ 35","≤ 390","≤10.5","EEHAZKV391UB","dia.10",9.5,null,10.5,35,390,20,2800,"125°C",4,"-55 to 125","125°C 4000H","-",2,"100kHz","10MHz",2.8,0.12,136.5,500,0,"G",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHAZKV391UB","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZF-A.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","THD","Can","Hybrid Al","Hybrid","ZC","Yes","≤ 50","≤  68","≤10.5","EEHAZC1H680B","dia. 8",9.5,null,10.5,50,68,30,1250,"125°C",3.4,"-55 to 125","125°C 4000H","-",2,"100kHz","10MHz",1.25,0.1,34,1000,0,"F",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHAZC1H680B","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZF-A.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","THD","Can","Hybrid Al","Hybrid","ZC","Yes","≤ 50","≤ 120","≤10.5","EEHAZC1H121B","dia.10",9.5,null,10.5,50,120,28,1600,"125°C",4,"-55 to 125","125°C 4000H","-",2,"100kHz","10MHz",1.6,0.1,60,500,0,"G",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHAZC1H121B","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZF-A.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","THD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 63","≤  47","≤10.5","EEHAZA1J470B","dia. 8",9.5,null,10.5,63,47,40,1700,"105°C",3.4,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",1.7,0.08,29.61,1000,0,"F",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHAZA1J470B","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZF-A.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","THD","Can","Hybrid Al","Hybrid","ZC","Yes","≤ 63","≤  68","≤10.5","EEHAZC1J680B","dia.10",9.5,null,10.5,63,68,30,1400,"125°C",4,"-55 to 125","125°C 4000H","-",2,"100kHz","10MHz",1.4,0.08,42.84,500,0,"G",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHAZC1J680B","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZF-A.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic","Japan","THD","Can","Hybrid Al","Hybrid","ZA","Yes","≤ 80","≤  22","≤10.5","EEHAZA1K220B","dia. 8",9.5,null,10.5,80,22,45,1550,"105°C",3.4,"-55 to 105","105°C10000H","-",2,"100kHz","10MHz",1.55,0.08,17.600000000000001,1000,0,"F",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/hybrid-aluminum/models/EEHAZA1K220B","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZF-A.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB","Yes",null,null,null,"EEEHB0G151P","dia. 6.3",5.8,null,6.1,4,150,"N/A",82,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,8.2000000000000003E-2,0.5,6,1000,null,"D",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHB0G151P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE0GA101SR","dia. 5",5.4,null,5.5,4,100,"N/A",61," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,6.0999999999999999E-2,0.35,4,1000,null,"C",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE0GA101SR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (Medium size)","Yes",null,null,null,"EEEFK0J682AM","dia.16",16.5,null,17,6.3,6800,35,1800,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.8,0.36,428.4,125,null,"J16",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK0J682AM","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK0J152GP","dia.10",10.199999999999999,null,10.5,6.3,1500,80,850,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,0.85,0.26,94.5,500,null,"G",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK0J152GP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC (LF reflow)","Yes",null,null,null,"EEEFC0J152AP","dia.10",10.199999999999999,null,10.5,6.3,1500,150,670,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.67,0.26,94.5,500,null,"G",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC0J152AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC","Yes",null,null,null,"EEEFC0J102P","dia.10",10.199999999999999,null,10.5,6.3,1000,150,670,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.67,0.26,63,500,null,"G",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC0J102P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE0JA102UP","dia. 8",10.199999999999999,null,10.5,6.3,1000,"N/A",500," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.5,0.35,63,500,null,"F",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE0JA102UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK0J471P","dia. 8",10.199999999999999,null,10.5,6.3,470,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.26,29.6,500,null,"F",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK0J471P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA0J471UP","dia. 8",10.199999999999999,null,10.5,6.3,470,"N/A",300,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.3,0.35,29.6,500,null,"F",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA0J471UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC (LF reflow)","Yes",null,null,null,"EEEFC0J331AP","dia. 8",10.199999999999999,null,10.5,6.3,330,300,450,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.45,0.26,20.7,500,null,"F",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC0J331AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK0J331XP","dia. 6.3",7.7,null,8,6.3,330,340,280,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.28000000000000003,0.26,20.7,900,null,"D8",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK0J331XP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA (LF reflow)","Yes",null,null,null,"EEEHA0J331AP","dia. 8",10.199999999999999,null,10.5,6.3,330,"N/A",230,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.23,0.35,20.7,500,null,"F",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA0J331AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN0J271UP","dia. 6.3",5.8,null,6.1,6.3,270,360,240,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.24,0.26,17,1000,null,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN0J271UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB","Yes",null,null,null,"EEEHB0J221AP","dia. 8",10.199999999999999,null,10.5,6.3,220,"N/A",150,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,0.15,0.35,13.8,500,null,"F",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHB0J221AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FH","Yes",null,null,null,"EEEFH0J101XL","dia. 6.3",7.7,null,8,6.3,100,450,300,"105°C",null,"-55 to 105","105°C 7000H",null,2,"100kHz",null,0.3,0.32,6.3,900,null,"D8",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFH0J101XL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE0JA101WR","dia. 5",5.4,null,5.5,6.3,100,"N/A",47," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,4.7E-2,0.35,6.3,1000,null,"C",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE0JA101WR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HC","Yes",null,null,null,"EEEHC0J101P","dia. 6.3",5.8,null,6.1,6.3,100,"N/A",71,"105°C",null,"-40 to 105","105°C 3000H",null,2,"100kHz",null,7.0999999999999994E-2,0.3,6.3,1000,null,"D",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHC0J101P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC (LF reflow)","Yes",null,null,null,"EEEFC0J680AP","dia. 6.3",5.4,null,5.5,6.3,68,1000,140,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.14000000000000001,0.26,4.2,1000,null,"D",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC0J680AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK0J470UR","dia. 4",5.8,null,6.1,6.3,47,1350,90,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.09,0.26,3,2000,null,"B",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK0J470UR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB (L: 5.5㎜)","Yes",null,null,null,"EEEHB0J470SR","dia. 5",5.4,null,5.5,6.3,47,"N/A",46,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,4.5999999999999999E-2,0.3,3,1000,null,"C",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHB0J470SR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE0JA330WR","dia. 4",5.4,null,5.5,6.3,33,"N/A",22," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,2.1999999999999999E-2,0.35,3,2000,null,"B",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE0JA330WR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC (LF reflow)","Yes",null,null,null,"EEEFC0J220AR","dia. 4",5.4,null,5.5,6.3,22,3000,60,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.06,0.26,3,2000,null,"B",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC0J220AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB","Yes",null,null,null,"EEEHB0J220AR","dia. 4",5.8,null,6.1,6.3,22,"N/A",26,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,2.5999999999999999E-2,0.3,3,2000,null,"B",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHB0J220AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (Medium size)","Yes",null,null,null,"EEVFK1A472M","dia.16",16.5,null,17,10,4700,35,1800,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.8,0.25,470,125,null,"J16",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEVFK1A472M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (Medium size)","Yes",null,null,null,"EEEFK1A222AQ","dia.12.5",13.5,null,14,10,2200,60,1100,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.1000000000000001,0.21,220,200,null,"H13",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1A222AQ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1A152UP","dia.10",10.199999999999999,null,10.5,10,1500,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.19,150,500,null,"G",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1A152UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP","Yes",null,null,null,"EEEFPA122UAP","dia.10",10.199999999999999,null,10.5,10,1200,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.19,120,500,null,"G",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPA122UAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1A102P","dia.10",10.199999999999999,null,10.5,10,1000,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.19,100,500,null,"G",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1A102P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1A102P","dia.10",10.199999999999999,null,10.5,10,1000,"N/A",400,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.4,0.26,100,500,null,"G",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1A102P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FH","Yes",null,null,null,"EEEFH1A561L","dia. 8",10.199999999999999,null,10.5,10,560,200,600,"105°C",null,"-55 to 105","105°C10000H",null,2,"100kHz",null,0.6,0.3,56,500,null,"F",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFH1A561L","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT","Yes",null,null,null,"EEEFTA471XAP","dia. 6.3",7.7,null,8,10,470,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.19,47,900,null,"D8",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFTA471XAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE1AA471P","dia.10",10.199999999999999,null,10.5,10,470,"N/A",400," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.4,0.26,47,500,null,"G",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1AA471P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TC","Yes",null,null,null,"EEETC1A331P","dia.10",10.199999999999999,null,10.5,10,330,150,750,"125°C",null,"-40 to 125","125°C 3000H",null,2,"100kHz",null,0.75,0.3,33,500,null,"G",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETC1A331P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (LF reflow)","Yes",null,null,null,"EEEFK1A331AP","dia. 8",10.199999999999999,null,10.5,10,330,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.19,33,500,null,"F",-55,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1A331AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TK","Yes",null,null,null,"EEETK1A331UP","dia. 8",10.199999999999999,null,10.5,10,330,300,197,"125°C",null,"-40 to 125","125°C 3000H",null,2,"100kHz",null,0.19700000000000001,0.3,33,500,null,"F",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETK1A331UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TC","Yes",null,null,null,"EEETC1A221P","dia. 8",10.199999999999999,null,10.5,10,220,200,410,"125°C",null,"-40 to 125","125°C 3000H",null,2,"100kHz",null,0.41,0.3,22,500,null,"F",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETC1A221P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS","Yes",null,null,null,"EEEFK1A221SP","dia. 6.3",5.8,null,6.1,10,220,360,240,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.24,0.19,22,1000,null,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1A221SP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA (LF reflow)","Yes",null,null,null,"EEEHAA221XAP","dia. 6.3",7.7,null,8,10,220,"N/A",105,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.105,0.22,22,900,null,"D8",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHAA221XAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HC","Yes",null,null,null,"EEEHC1A221P","dia. 8",10.199999999999999,null,10.5,10,220,"N/A",160,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,0.16,0.26,22,500,null,"F",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHC1A221P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC (LF reflow)","Yes",null,null,null,"EEEFC1A101P","dia. 8",6.2,null,6.5,10,100,400,230,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.23,0.19,10,1000,null,"E",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1A101P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA (LF reflow)","Yes",null,null,null,"EEEHAA101WAP","dia. 6.3",5.4,null,5.5,10,100,"N/A",71,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,7.0999999999999994E-2,0.3,10,1000,null,"D",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHAA101WAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT","Yes",null,null,null,"EEEFT1A680AR","dia. 4",5.8,null,6.1,10,68,850,160,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.16,0.19,6.8,2000,null,"B",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1A680AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1A560UR","dia. 4",5.8,null,6.1,10,56,1350,90,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.09,0.19,5.6,2000,null,"B",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1A560UR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP","Yes",null,null,null,"EEEFPA330UAR","dia. 4",5.8,null,6.1,10,33,850,160,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.16,0.19,3.3,2000,null,"B",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPA330UAR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE1AA330WR","dia. 4",5.4,null,5.5,10,33,"N/A",29," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,2.9000000000000001E-2,0.3,3.3,2000,null,"B",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1AA330WR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB (L: 5.5㎜)","Yes",null,null,null,"EEEHB1A330SR","dia. 5",5.4,null,5.5,10,33,"N/A",43,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,4.2999999999999997E-2,0.22,3.3,1000,null,"C",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHB1A330SR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1A220WR","dia. 4",5.4,null,5.5,10,22,"N/A",28,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,2.8000000000000001E-2,0.3,3,2000,null,"B",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1A220WR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS (Medium size)","Yes",null,null,null,"EEEFK1C432SM","dia.16",16.5,null,17,16,4300,35,1800,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.8,0.22,688,125,null,"J16",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1C432SM","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS (Medium size)","Yes",null,null,null,"EEEFK1C182SQ","dia.12.5",13.5,null,14,16,1800,60,1100,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.1000000000000001,0.16,288,200,null,"H13",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1C182SQ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (Medium size)","Yes",null,null,null,"EEEFK1C152AQ","dia.12.5",13.5,null,14,16,1500,60,1100,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.1000000000000001,0.16,240,200,null,"H13",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1C152AQ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT","Yes",null,null,null,"EEEFT1C821UP","dia. 8",10.199999999999999,null,10.5,16,820,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,1.1599999999999999,131.19999999999999,500,null,"F",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1C821UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT","Yes",null,null,null,"EEEFT1C681GP","dia. 8",10.199999999999999,null,10.5,16,680,80,850,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,0.85,0.16,108.8,500,null,"F",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1C681GP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA (LF reflow)","Yes",null,null,null,"EEEHAC681UAP","dia.10",10.199999999999999,null,10.5,16,680,"N/A",380,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.38,0.26,108.8,500,null,"G",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHAC681UAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TP","Yes",null,null,null,"EEETP1C471AP","dia.10",10.199999999999999,null,10.5,16,470,150,500,"125°C",null,"-40 to 125","125°C 3000H",null,2,"100kHz",null,0.5,0.23,75.2,500,null,"G",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETP1C471AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HD","Yes",null,null,null,"EEEHD1C471AP","dia.10",10.199999999999999,null,10.5,16,470,800,340,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,0.34,0.2,75.2,500,null,"G",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHD1C471AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TCU","Yes",null,null,null,"EEETC1C391UP","dia. 8",10.199999999999999,null,10.5,16,390,200,410,"125°C",null,"-40 to 125","125°C 3000H",null,2,"100kHz",null,0.41,0.23,62.4,500,null,"F",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETC1C391UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (LF reflow)","Yes",null,null,null,"EEEFK1C331AP","dia. 8",10.199999999999999,null,10.5,16,330,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.16,52.8,500,null,"F",-55,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1C331AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TG","Yes",null,null,null,"EEETG1C331UP","dia.10",10.199999999999999,null,10.5,16,330,300,270,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.27,0.23,52.8,500,null,"G",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETG1C331UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE1CA331UP","dia. 8",10.199999999999999,null,10.5,16,330,"N/A",320," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.32,0.2,52.8,500,null,"F",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1CA331UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFNC271XUP","dia. 6.3",7.7,null,8,16,270,340,280,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.28000000000000003,0.16,43.2,900,null,"D8",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFNC271XUP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FH","Yes",null,null,null,"EEEFH1C221L","dia. 8",10.199999999999999,null,10.5,16,220,200,600,"105°C",null,"-55 to 105","105°C10000H",null,2,"100kHz",null,0.6,0.23,35.200000000000003,500,null,"F",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFH1C221L","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE1CA221UP","dia. 8",6.2,null,6.5,16,220,"-",200," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.2,0.2,35.200000000000003,1000,null,"E",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1CA221UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1C221UP","dia. 8",10.199999999999999,null,10.5,16,220,"N/A",150,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.15,0.2,35.200000000000003,500,null,"F",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1C221UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB","Yes",null,null,null,"EEEHB1C221P","dia.10",10.199999999999999,null,10.5,16,220,"N/A",210,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,0.21,0.2,35.200000000000003,500,null,"G",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHB1C221P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC (LF reflow)","Yes",null,null,null,"EEEFC1C101AP","dia. 8",6.2,null,6.5,16,100,400,230,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.23,0.16,16,1000,null,"E",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1C101AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC","Yes",null,null,null,"EEEFC1C101P","dia. 8",6.2,null,6.5,16,100,400,230,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.23,0.16,16,1000,null,"E",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1C101P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1C101WP","dia. 6.3",5.4,null,5.5,16,100,"N/A",70,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,7.0000000000000007E-2,0.26,16,1000,null,"D",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1C101WP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP","Yes",null,null,null,"EEEFP1C680AP","dia. 6.3",5.8,null,6.1,16,68,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.16,10.8,1000,null,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1C680AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK1C470P","dia. 6.3",5.8,null,6.1,16,47,360,240,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.24,0.16,7.5,1000,null,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1C470P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT","Yes",null,null,null,"EEEFT1C470AR","dia. 4",5.8,null,6.1,16,47,850,160,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.16,0.16,7.5,2000,null,"B",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1C470AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB","Yes",null,null,null,"EEEHBC470UAR","dia. 5",5.8,null,6.1,16,47,"N/A",39,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,3.9E-2,0.26,7.5,1000,null,"C",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHBC470UAR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA (LF reflow)","Yes",null,null,null,"EEEHAC330WAR","dia. 5",5.4,null,5.5,16,33,"N/A",35,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,3.5000000000000003E-2,0.26,5.2,1000,null,"C",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHAC330WAR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1C220R","dia. 4",5.8,null,6.1,16,22,1350,90,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.09,0.16,3.5,2000,null,"B",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1C220R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S (Bi-polar)","Yes",null,null,null,"EEE1CA220NP","dia. 6.3",5.4,null,5.5,16,22,"N/A",39," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,3.9E-2,0.32,3.5,1000,null,"D",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1CA220NP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Bipolar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1C220WR","dia. 4",5.4,null,5.5,16,22,"N/A",28,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,2.8000000000000001E-2,0.26,3.5,2000,null,"B",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1C220WR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK1C100R","dia. 4",5.8,null,6.1,16,10,1350,90,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.09,0.16,3,2000,null,"B",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1C100R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA (LF reflow)","Yes",null,null,null,"EEEHA1C100AR","dia. 4",5.4,null,5.5,16,10,"N/A",28,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,2.8000000000000001E-2,0.16,3,2000,null,"B",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1C100AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (Medium size)","Yes",null,null,null,"EEEFK1E332AM","dia.18",16.5,null,17,25,3300,33,2060,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.06,0.18,825,125,null,"K16",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1E332AM","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HD (Medium size)","Yes",null,null,null,"EEEHD1E222AM","dia.16",16.5,null,17,25,2200,"N/A",1200,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.2,0.18,550,125,null,"J16",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHD1E222AM","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS (Medium size)","Yes",null,null,null,"EEEFK1E122SQ","dia.12.5",13.5,null,14,25,1200,60,1100,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.1000000000000001,0.14000000000000001,300,200,null,"H13",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1E122SQ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS","Yes",null,null,null,"EEEFK1E681SP","dia.10",10.199999999999999,null,10.5,25,680,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.14000000000000001,170,500,null,"G",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1E681SP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1E681UP","dia.10",10.199999999999999,null,10.5,25,680,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.14000000000000001,170,500,null,"G",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1E681UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC (LF reflow)","Yes",null,null,null,"EEEFC1E471AP","dia.10",10.199999999999999,null,10.5,25,470,150,670,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.67,0.14000000000000001,117.5,500,null,"G",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1E471AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S (LF reflow)","Yes",null,null,null,"EEE1EA471UAP","dia.10",10.199999999999999,null,10.5,25,470,"N/A",380," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,0.38,0.25,117.5,500,null,"G",-40,85,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1EA471UAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TK (Medium size)","Yes",null,null,null,"EEETK1E331AQ","dia.12.5",13.5,null,14,25,330,120,800,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.8,0.18,82.5,200,null,"H13",-40,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETK1E331AQ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FH","Yes",null,null,null,"EEEFH1E331L","dia.10",10.199999999999999,null,10.5,25,330,150,850,"105°C",null,"-55 to 105","105°C10000H",null,2,"100kHz",null,0.85,0.18,82.5,500,null,"G",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFH1E331L","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA (LF reflow)","Yes",null,null,null,"EEEHAE331UAP","dia. 8",10.199999999999999,null,10.5,25,330,"N/A",180,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.18,0.2,82.5,500,null,"F",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHAE331UAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC","Yes",null,null,null,"EEEFC1E221P","dia.10",10.199999999999999,null,10.5,25,220,150,670,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.67,0.14000000000000001,55,500,null,"G",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1E221P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TCU","Yes",null,null,null,"EEETC1E221UP","dia. 8",10.199999999999999,null,10.5,25,220,200,410,"125°C",null,"-40 to 125","125°C 3000H",null,2,"100kHz",null,0.41,0.18,55,500,null,"F",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETC1E221UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE1EA221P","dia.10",10.199999999999999,null,10.5,25,220,"N/A",310," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.31,0.16,55,500,null,"G",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1EA221P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1E221UP","dia. 8",10.199999999999999,null,10.5,25,220,"N/A",160,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.16,0.16,55,500,null,"F",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1E221UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK1E151P","dia. 8",10.199999999999999,null,10.5,25,150,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.14000000000000001,37.5,500,null,"F",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1E151P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC (LF reflow)","Yes",null,null,null,"EEEFC1E101AP","dia. 8",10.199999999999999,null,10.5,25,100,300,450,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.45,0.14000000000000001,25,500,null,"F",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1E101AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FH","Yes",null,null,null,"EEEFH1E101XL","dia. 6.3",7.7,null,8,25,100,450,300,"105°C",null,"-55 to 105","105°C 7000H",null,2,"100kHz",null,0.3,0.18,25,900,null,"D8",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFH1E101XL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE1EA101P","dia. 8",10.199999999999999,null,10.5,25,100,"N/A",180," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.18,0.16,25,500,null,"F",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1EA101P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1E101XP","dia. 6.3",7.7,null,8,25,100,"N/A",91,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,9.0999999999999998E-2,0.14000000000000001,25,900,null,"D8",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1E101XP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1E560UR","dia. 5",5.8,null,6.1,25,56,700,160,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.16,0.14000000000000001,14,1000,null,"C",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1E560UR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP","Yes",null,null,null,"EEEFP1E470AP","dia. 6.3",5.8,null,6.1,25,47,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.14000000000000001,11.7,1000,null,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1E470AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA (LF reflow)","Yes",null,null,null,"EEEHA1E470AP","dia. 8",6.2,null,6.5,25,47,"N/A",91,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,9.0999999999999998E-2,0.16,11.7,1000,null,"E",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1E470AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HC","Yes",null,null,null,"EEEHC1E470XP","dia. 6.3",7.7,null,8,25,47,"N/A",65,"105°C",null,"-40 to 105","105°C 3000H",null,2,"100kHz",null,6.5000000000000002E-2,0.16,11.7,900,null,"D8",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHC1E470XP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT","Yes",null,null,null,"EEEFT1E330AR","dia. 4",5.8,null,6.1,25,33,850,160,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.16,0.14000000000000001,8.1999999999999993,2000,null,"B",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1E330AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S (LF reflow)","Yes",null,null,null,"EEE1EA330AP","dia. 6.3",5.4,null,5.5,25,33,"N/A",65," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,6.5000000000000002E-2,0.14000000000000001,8.1999999999999993,1000,null,"D",-40,85,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1EA330AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP","Yes",null,null,null,"EEEFP1E220AR","dia. 5",5.8,null,6.1,25,22,360,240,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.24,0.14000000000000001,5.5,1000,null,"C",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1E220AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S (LF reflow)","Yes",null,null,null,"EEE1EA220AP","dia. 6.3",5.4,null,5.5,25,22,"N/A",55," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,5.5E-2,0.14000000000000001,5.5,1000,null,"D",-40,85,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1EA220AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP","Yes",null,null,null,"EEEFP1E100AR","dia. 4",5.8,null,6.1,25,10,850,160,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.16,0.14000000000000001,3,2000,null,"B",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1E100AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1E100R","dia. 4",5.8,null,6.1,25,10,1350,90,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.09,0.14000000000000001,3,2000,null,"B",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1E100R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA (LF reflow)","Yes",null,null,null,"EEEHA1E100AR","dia. 5",5.4,null,5.5,25,10,"N/A",28,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,2.8000000000000001E-2,0.14000000000000001,3,1000,null,"C",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1E100AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB","Yes",null,null,null,"EEEHB1E6R8R","dia. 4",5.8,null,6.1,25,6.8,"N/A",25,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,2.5000000000000001E-2,0.14000000000000001,3,2000,null,"B",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHB1E6R8R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S (Bi-polar)","Yes",null,null,null,"EEE1EA3R3NR","dia. 4",5.4,null,5.5,25,3.3,"N/A",12," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,1.2E-2,0.28000000000000003,3,2000,null,"B",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1EA3R3NR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Bipolar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS (Medium size)","Yes",null,null,null,"EEEFK1V162SM","dia.16",16.5,null,17,35,1600,35,1800,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.8,0.14000000000000001,560,125,null,"J16",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1V162SM","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS (Medium size)","Yes",null,null,null,"EEEFK1V751SQ","dia.12.5",13.5,null,14,35,750,60,1100,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.1000000000000001,0.12,262.5,200,null,"H13",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1V751SQ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TG (Medium size)","Yes",null,null,null,"EEVTG1V681M","dia.18",16.5,null,17,35,680,75,1300,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,1.3,0.16,238,125,null,"K16",-40,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEVTG1V681M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TG (Medium size)","Yes",null,null,null,"EEVTG1V471UQ","dia.12.5",13.5,null,14,35,470,120,800,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.8,0.16,164.5,200,null,"H13",-40,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEVTG1V471UQ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TK (Medium size)","Yes",null,null,null,"EEETKV471UAQ","dia.12.5",13.5,null,14,35,470,120,800,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.8,0.16,164.5,200,null,"H13",-40,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETKV471UAQ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC (LF reflow)","Yes",null,null,null,"EEEFC1V331AP","dia.10",10.199999999999999,null,10.5,35,330,150,670,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.67,0.12,115.5,500,null,"G",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1V331AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S (LF reflow)","Yes",null,null,null,"EEE1VA331UAP","dia.10",10.199999999999999,null,10.5,35,330,"N/A",350," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,0.35,0.3,115.5,500,null,"G",-40,85,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1VA331UAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TP","Yes",null,null,null,"EEETP1V221AP","dia.10",10.199999999999999,null,10.5,35,220,150,500,"125°C",null,"-40 to 125","125°C 3000H",null,2,"100kHz",null,0.5,0.16,77,500,null,"G",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETP1V221AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK1V221GP","dia. 8",10.199999999999999,null,10.5,35,220,160,600,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,0.6,0.12,77,500,null,"F",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1V221GP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HC","Yes",null,null,null,"EEEHC1V221P","dia.10",10.199999999999999,null,10.5,35,220,"N/A",220,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,0.22,0.14000000000000001,77,500,null,"G",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHC1V221P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS","Yes",null,null,null,"EEEFKV121XSP","dia. 6.3",7.7,null,8,35,120,340,280,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.28000000000000003,0.12,42,900,null,"D8",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFKV121XSP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK1V101P","dia. 8",10.199999999999999,null,10.5,35,100,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.12,35,500,null,"F",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1V101P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TC","Yes",null,null,null,"EEETC1V101P","dia. 8",10.199999999999999,null,10.5,35,100,200,410,"125°C",null,"-40 to 125","125°C 3000H",null,2,"100kHz",null,0.41,0.16,35,500,null,"F",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETC1V101P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TG","Yes",null,null,null,"EEETG1V101UP","dia. 8",10.199999999999999,null,10.5,35,100,500,197,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.19700000000000001,0.16,35,500,null,"F",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETG1V101UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA (LF reflow)","Yes",null,null,null,"EEEHAV101UAP","dia. 8",10.199999999999999,null,10.5,35,100,"N/A",120,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.12,0.14000000000000001,35,500,null,"F",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHAV101UAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (LF reflow)","Yes",null,null,null,"EEEFKV680XAP","dia. 6.3",7.7,null,8,35,68,340,280,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.28000000000000003,0.12,23.8,900,null,"D8",-55,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFKV680XAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TK","Yes",null,null,null,"EEETK1V470P","dia. 8",10.199999999999999,null,10.5,35,47,300,197,"125°C",null,"-40 to 125","125°C 3000H",null,2,"100kHz",null,0.19700000000000001,0.16,16.399999999999999,500,null,"F",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETK1V470P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TC","Yes",null,null,null,"EEETC1V470XP","dia. 6.3",7.7,null,8,35,47,450,300,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.3,0.16,16.399999999999999,900,null,"D8",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETC1V470XP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HD","Yes",null,null,null,"EEEHD1V470AP","dia. 8",10.199999999999999,null,10.5,35,47,1500,79,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,7.9000000000000001E-2,0.14000000000000001,16.399999999999999,500,null,"F",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHD1V470AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1V390UR","dia. 5",5.8,null,6.1,35,39,700,160,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.16,0.12,13.6,1000,null,"C",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1V390UR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP","Yes",null,null,null,"EEEFP1V330AP","dia. 6.3",5.8,null,6.1,35,33,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.12,11.5,1000,null,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1V330AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE1VA330WP","dia. 6.3",5.4,null,5.5,35,33,"N/A",60," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,0.06,0.16,11.5,1000,null,"D",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1VA330WP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB","Yes",null,null,null,"EEEHB1V330AP","dia. 8",6.2,null,6.5,35,33,"N/A",84,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,8.4000000000000005E-2,0.14000000000000001,11.5,1000,null,"E",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHB1V330AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC (LF reflow)","Yes",null,null,null,"EEEFC1V220AP","dia. 6.3",5.4,null,5.5,35,22,1000,140,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.14000000000000001,0.12,7.7,1000,null,"D",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1V220AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE1VA220WR","dia. 5",5.4,null,5.5,35,22,"N/A",36," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,3.5999999999999997E-2,0.16,7.7,1000,null,"C",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1VA220WR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK1V100R","dia. 5",5.8,null,6.1,35,10,700,160,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.16,0.12,3.5,1000,null,"C",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1V100R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S (LF reflow)","Yes",null,null,null,"EEE1VA100AR","dia. 5",5.4,null,5.5,35,10,"N/A",30," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.03,0.12,3.5,1000,null,"C",-40,85,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1VA100AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1V100WR","dia. 4",5.4,null,5.5,35,10,"N/A",22,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,2.1999999999999999E-2,0.16,3.5,2000,null,"B",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1V100WR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HC","Yes",null,null,null,"EEEHC1V100R","dia. 5",5.8,null,6.1,35,10,"N/A",28,"105°C",null,"-40 to 105","105°C 3000H",null,2,"100kHz",null,2.8000000000000001E-2,0.14000000000000001,3.5,1000,null,"C",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHC1V100R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S (LF reflow)","Yes",null,null,null,"EEE1VA4R7AR","dia. 4",5.4,null,5.5,35,4.7,"N/A",22," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,2.1999999999999999E-2,0.12,3,2000,null,"B",-40,85,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1VA4R7AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC (LF reflow)","Yes",null,null,null,"EEEFC1V2R2AR","dia. 4",5.4,null,5.5,35,2.2000000000000002,3000,60,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.06,0.12,3,2000,null,"B",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1V2R2AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TP (Medium size)","Yes",null,null,null,"EEETP1H751M","dia.16",16.5,null,17,50,750,80,2000,"125°C",null,"-55 to 125","125°C 3000H",null,2,"100kHz",null,2,0.14000000000000001,375,125,null,"J16",-55,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETP1H751M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (Medium size)","Yes",null,null,null,"EEEFK1H561AM","dia.16",16.5,null,17,50,560,73,1610,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.61,0.12,280,125,null,"J16",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1H561AM","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT","Yes",null,null,null,"EEEFT1H331AP","dia.10",10.199999999999999,null,10.5,50,330,120,900,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.9,0.1,165,500,null,"G",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1H331AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TK (Medium size)","Yes",null,null,null,"EEETK1H331AQ","dia.12.5",13.5,null,14,50,330,230,600,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.6,0.14000000000000001,165,200,null,"H13",-40,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETK1H331AQ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1H221P","dia.10",10.199999999999999,null,10.5,50,220,"N/A",150,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.15,0.12,110,500,null,"G",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1H221P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB","Yes",null,null,null,"EEEHBH221UAP","dia.10",10.199999999999999,null,10.5,50,220,"N/A",270,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,0.27,0.18,110,500,null,"G",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHBH221UAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FH","Yes",null,null,null,"EEEFH1H101L","dia.10",10.199999999999999,null,10.5,50,100,500,670,"105°C",null,"-55 to 105","105°C 7000H",null,2,"100kHz",null,0.67,0.14000000000000001,50,500,null,"G",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFH1H101L","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA (LF reflow)","Yes",null,null,null,"EEEHAH101UAP","dia. 8",10.199999999999999,null,10.5,50,100,"N/A",110,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.11,0.18,50,500,null,"F",-40,105,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHAH101UAP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC","Yes",null,null,null,"EEEFC1H470P","dia.10",10.199999999999999,null,10.5,50,47,300,500,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.5,0.12,23.5,500,null,"G",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1H470P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,"202/7/8 Automotive - Yes",null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1H470XP","dia. 6.3",7.7,null,8,50,47,680,195,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.19500000000000001,0.1,23.5,900,null,"D8",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1H470XP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1H470UP","dia. 8",10.199999999999999,null,10.5,50,47,"N/A",95,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,9.5000000000000001E-2,0.12,23.5,500,null,"F",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1H470UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC","Yes",null,null,null,"EEEFC1H330P","dia. 8",10.199999999999999,null,10.5,50,33,600,300,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.3,0.12,16.5,500,null,"F",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1H330P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE1HA330XP","dia. 6.3",7.7,null,8,50,33,"N/A",85," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,8.5000000000000006E-2,0.12,16.5,900,null,"D8",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1HA330XP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE1HA330UP","dia. 8",6.2,null,6.5,50,33,"N/A",65," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,6.5000000000000002E-2,0.12,16.5,1000,null,"E",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1HA330UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB","Yes",null,null,null,"EEEHB1H330P","dia. 8",10.199999999999999,null,10.5,50,33,"N/A",91,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,9.0999999999999998E-2,0.12,16.5,500,null,"F",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHB1H330P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S (LF reflow)","Yes",null,null,null,"EEE1HA220AP","dia. 8",6.2,null,6.5,50,22,"N/A",120," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.12,0.12,11,1000,null,"E",-40,85,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1HA220AP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK1H100P","dia. 6.3",5.8,null,6.1,50,10,880,165,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.16500000000000001,0.1,5,1000,null,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1H100P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S (LF reflow)","Yes",null,null,null,"EEE1HA100WAR","dia. 5",5.4,null,5.5,50,10,"N/A",27," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,2.7E-2,0.14000000000000001,5,1000,null,"C",-40,85,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1HA100WAR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HC","Yes",null,null,null,"EEEHC1H100P","dia. 6.3",5.8,null,6.1,50,10,"N/A",35,"105°C",null,"-40 to 105","105°C 3000H",null,2,"100kHz",null,3.5000000000000003E-2,0.12,5,1000,null,"D",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHC1H100P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK","Yes",null,null,null,"EEEFK1H4R7R","dia. 4",5.8,null,6.1,50,4.7,2900,60,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.06,0.1,3,2000,null,"B",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1H4R7R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FC","Yes",null,null,null,"EEEFC1H3R3R","dia. 4",5.4,null,5.5,50,3.3,5000,30,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.03,0.12,3,2000,null,"B",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFC1H3R3R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HD","Yes",null,null,null,"EEEHD1H3R3R","dia. 4",5.8,null,6.1,50,3.3,12000,16,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,1.6E-2,0.12,3,2000,null,"B",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHD1H3R3R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S (LF reflow)","Yes",null,null,null,"EEE1HA2R2AR","dia. 4",5.4,null,5.5,50,2.2000000000000002,"N/A",16," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,1.6E-2,0.12,3,2000,null,"B",-40,85,"Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1HA2R2AR","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HB","Yes",null,null,null,"EEEHB1H2R2R","dia. 4",5.8,null,6.1,50,2.2000000000000002,"N/A",16,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,1.6E-2,0.12,3,2000,null,"B",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHB1H2R2R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1H1R0R","dia. 4",5.4,null,5.5,50,1,"N/A",10,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.01,0.12,3,2000,null,"B",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1H1R0R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HC","Yes",null,null,null,"EEEHC1H1R0R","dia. 4",5.8,null,6.1,50,1,"N/A",10,"105°C",null,"-40 to 105","105°C 3000H",null,2,"100kHz",null,0.01,0.12,3,2000,null,"B",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHC1H1R0R","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TG (Medium size)","Yes",null,null,null,"EEVTG1J221Q","dia.12.5",13.5,null,14,63,220,260,350,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.35,0.12,138.6,200,null,"H13",-40,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEVTG1J221Q","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1J101P","dia.10",10.199999999999999,null,10.5,63,100,350,400,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.4,0.08,63,500,null,"G",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1J101P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","S","Yes",null,null,null,"EEE1JA470P","dia.10",10.199999999999999,null,10.5,63,47,"N/A",45," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,4.4999999999999998E-2,0.18,29.6,500,null,"G",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEE1JA470P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA1J470UP","dia. 8",10.199999999999999,null,10.5,63,47,"N/A",45,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,4.4999999999999998E-2,0.18,29.6,500,null,"F",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA1J470UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TG","Yes",null,null,null,"EEETG1J220P","dia. 8",10.199999999999999,null,10.5,63,22,1000,100,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.1,0.12,13.8,500,null,"F",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETG1J220P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1J100P","dia. 6.3",5.8,null,6.1,63,10,1500,80,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.08,0.08,6.3,1000,null,"D",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1J100P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TP (Medium size)","Yes",null,null,null,"EEETP1K511M","dia.18",16.5,null,17,80,510,95,2000,"125°C",null,"-55 to 125","125°C 3000H",null,2,"100kHz",null,2,0.12,408,125,null,"K16",-55,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETP1K511M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TK (Medium size)","Yes",null,null,null,"EEETK1K331AM","dia.18",16.5,null,17,80,330,280,400,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.4,0.12,264,125,null,"K16",-40,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETK1K331AM","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TG (Medium size)","Yes",null,null,null,"EEVTG1K101M","dia.16",16.5,null,17,80,100,300,350,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.35,0.12,80,125,null,"J16",-40,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEVTG1K101M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TG (Medium size)","Yes",null,null,null,"EEVTG1K101UQ","dia.12.5",13.5,null,14,80,100,420,250,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.25,0.12,80,200,null,"H13",-40,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEVTG1K101UQ","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN","Yes",null,null,null,"EEEFN1K330P","dia. 8",10.199999999999999,null,10.5,80,33,1300,130,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.13,0.08,26.4,500,null,"F",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1K330P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TG","Yes",null,null,null,"EEETG1K220P","dia.10",10.199999999999999,null,10.5,80,22,1000,90,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.09,0.12,17.600000000000001,500,null,"G",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETG1K220P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TK (Medium size)","Yes",null,null,null,"EEETK2A331AM","dia.18",16.5,null,17,100,330,280,400,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.4,0.1,330,125,null,"K16",-40,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEETK2A331AM","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (Medium size)","Yes",null,null,null,"EEVFK2A151M","dia.16",16.5,null,17,100,150,170,793,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,0.79300000000000004,7.0000000000000007E-2,150,125,null,"J16",-55,105,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEVFK2A151M","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","TG (Medium size)","Yes",null,null,null,"EEVTG2A470Q","dia.12.5",13.5,null,14,100,47,420,250,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.25,0.1,47,200,null,"H13",-40,125,"Medium Size",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEVTG2A470Q","https://industrial.panasonic.com/content/data/CP/pictures/lineup-ZU.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA2A330P","dia.10",10.199999999999999,null,10.5,100,33,"N/A",65,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,6.5000000000000002E-2,0.18,33,500,null,"G",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA2A330P","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA2A220UP","dia. 8",10.199999999999999,null,10.5,100,22,"N/A",55,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,5.5E-2,0.18,22,500,null,"F",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA2A220UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","HA","Yes",null,null,null,"EEEHA2A4R7UP","dia. 8",6.2,null,6.5,100,4.7,"N/A",30,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.03,0.18,4.7,1000,null,"E",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEHA2A4R7UP","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KA-A","No",null,null,null,"ECEA0GKA331Q","dia. 8",7,null,8,4,330,"N/A",110," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,0.11,0.35,13.2,"N/A",null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA0GKA331Q","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KA-A","No",null,null,null,"ECEA0GKA221","dia. 6.3",7,null,8,4,220,"N/A",82," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,8.2000000000000003E-2,0.35,8.8000000000000007,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA0GKA221","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA0JM223","dia.18",35.5,null,37.5,6.3,22000,"N/A",1900," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,1.9,0.7,1386,50,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA0JM223","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA0JHG103","dia.16",25,null,27,6.3,10000,"N/A",1650,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.65,0.46,630,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA0JHG103","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK0J822S","dia.18",20,null,22,6.3,8200,25,2640,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.64,0.36,516.6,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK0J822S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC0J682","dia.16",25,null,27,6.3,6800,22,2555,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.5550000000000002,0.32,428.4,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC0J682","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC0J562L","dia.12.5",35,null,37,6.3,5600,22,2510,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.5099999999999998,0.3,352.8,100,null,"N/A",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC0J562L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC0J472","dia.12.5",30,null,32,6.3,4700,25,2310,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.31,0.28000000000000003,296.10000000000002,100,null,"N/A",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC0J472","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC0J392","dia.12.5",25,null,27,6.3,3900,30,1945,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.9450000000000001,0.26,245.7,200,null,"N/A",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC0J392","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FM-A","No",null,null,null,"EEUFM0J332","dia.12.5",20,null,22,6.3,3300,18,2600,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,2.6,0.26,207.9,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFM0J332","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA0JHG332","dia.10",20,null,22,6.3,3300,"N/A",840,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.84,0.32,207.9,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA0JHG332","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK0J222L","dia.10",25,null,27,6.3,2200,33,1680,"105°C",null,"-55 to 105","105°C 4000H",null,2,"100kHz",null,1.68,0.24,138.6,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK0J222L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS0J182L","dia. 8",20,null,22,6.3,1800,30,1560,"105°C",null,"-40 to 105","105°C 9000H",null,2,"100kHz",null,1.56,0.22,113.4,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS0J182L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC0J152S","dia.12.5",15,null,16,6.3,1500,65,1205,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.2050000000000001,0.22,94.5,200,null,"N/A",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC0J152S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK0J102","dia.10",12.5,null,14,6.3,1000,63,900,"105°C",null,"-55 to 105","105°C 4000H",null,2,"100kHz",null,0.9,0.22,63,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK0J102","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK0J681","dia. 8",11.5,null,13,6.3,680,90,630,"105°C",null,"-55 to 105","105°C 3000H",null,2,"100kHz",null,0.63,0.22,42.8,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK0J681","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR0J331","dia. 6.3",11.2,null,12.7,6.3,330,130,455,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,0.45500000000000002,0.22,20.7,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR0J331","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC0J331S","dia. 6.3",11.2,null,12.2,6.3,330,350,290,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,0.28999999999999998,0.22,20.7,200,null,"N/A",-55,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC0J331S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS0J221","dia. 5",11,null,12.5,6.3,220,300,280,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,0.28000000000000003,0.22,13.8,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS0J221","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KA-A","No",null,null,null,"ECEA0JKA101","dia. 5",7,null,8,6.3,100,"N/A",71," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,7.0999999999999994E-2,0.24,6.3,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA0JKA101","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KS-A (Bi-polar)","No",null,null,null,"ECEA0JSN330","dia. 6.3",5,null,6,6.3,33,"N/A",38," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,3.7999999999999999E-2,0.24,10.3,200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA0JSN330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1A123","dia.18",40,null,42,10,12000,14,3735,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,3.7349999999999999,0.16,1200,50,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1A123","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK1A682L","dia.12.5",40,null,42,10,6800,14,3010,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,3.01,0.28999999999999998,680,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK1A682L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA1AM682","dia.16",25,null,27,10,6800,"N/A",1400," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,1.4,0.34,680,100,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1AM682","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FM-A","No",null,null,null,"EEUFM1A472L","dia.12.5",35,null,37,10,4700,12,3750,"105°C",null,"-40 to 105","105°C 7000H",null,2,"100kHz",null,3.75,0.23,470,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFM1A472L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1A472L","dia.12.5",30,null,32,10,4700,13,3630,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,3.63,0.25,470,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1A472L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK1A472S","dia.16",20,null,22,10,4700,26,2330,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.33,0.25,470,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK1A472S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK1A392S","dia.18",15,null,16.5,10,3900,36,2060,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.06,0.23,390,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK1A392S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA1AHG332","dia.12.5",20,null,22,10,3300,"N/A",1000,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1,0.28000000000000003,330,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1AHG332","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FM-A","No",null,null,null,"EEUFM1A222","dia.12.5",20,null,22,10,2200,18,2600,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,2.6,0.21,220,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFM1A222","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","HD-A","No",null,null,null,"EEUHD1A222","dia.10",16,null,17.5,10,2200,"N/A",760,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.76,0.26,220,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUHD1A222","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1A182S","dia.16",15,null,16.5,10,1800,43,1690,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.69,0.19,180,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1A182S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1A122","dia.10",20,null,22,10,1200,52,1220,"105°C",null,"-55 to 105","105°C 3000H",null,2,"100kHz",null,1.22,0.19,120,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1A122","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1A122S","dia.12.5",15,null,16,10,1200,65,1205,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.2050000000000001,0.19,120,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1A122S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","TA-A","Yes",null,null,null,"EEUTA1A102S","dia.12.5",15,null,16,10,1000,70,1085,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,1.085,0.2,100,200,null,"N/A",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUTA1A102S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FM-A","No",null,null,null,"EEUFM1A681","dia.10",12.5,null,14,10,680,38,1290,"105°C",null,"-40 to 105","105°C 4000H",null,2,"100kHz",null,1.29,0.19,68,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFM1A681","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","TA-A","Yes",null,null,null,"EEUTA1A471","dia.10",12.5,null,13.5,10,470,100,680,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.68,0.2,47,200,null,"N/A",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUTA1A471","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","TA-A","Yes",null,null,null,"EEUTA1A331","dia. 8",11.5,null,12.5,10,330,130,500,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,0.5,0.2,33,200,null,"N/A",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUTA1A331","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","SU-A (Bi-polar)","No",null,null,null,"ECEA1AN221U","dia. 8",11.5,null,12.5,10,220,"N/A",200," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.2,0.25,"N/A",200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1AN221U","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1A151","dia. 6.3",11.2,null,12.2,10,150,350,290,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,0.28999999999999998,0.19,15,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1A151","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEAFC1A820","dia. 6.3",7,null,8,10,82,450,200,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,0.2,0.19,8.1999999999999993,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEAFC1A820","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1A820","dia. 5",11,null,12,10,82,800,175,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,0.17499999999999999,0.19,8.1999999999999993,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1A820","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","GA-A","No",null,null,null,"EEAGA1A330","dia. 5",7,null,8,10,33,"N/A",50,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,0.05,0.22,3.3,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEAGA1A330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KS-A (Bi-polar)","No",null,null,null,"ECEA1ASN100","dia. 4",5,null,6,10,10,"N/A",25," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,2.5000000000000001E-2,0.2,10,200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1ASN100","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA1CHG682","dia.16",31.5,null,33.5,16,6800,"N/A",1780,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.78,0.3,1088,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1CHG682","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1C472L","dia.12.5",35,null,37,16,4700,12,3750,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,3.75,0.22,752,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1C472L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA1CM472","dia.16",25,null,27,16,4700,"N/A",1360," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,1.36,0.26,752,100,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1CM472","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS1C362L","dia.12.5",30,null,32,16,3600,13,3630,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,3.63,0.16,576,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS1C362L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA1CHG332","dia.12.5",25,null,27,16,3300,"N/A",1170,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.17,0.24,528,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1CHG332","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","HD-A","No",null,null,null,"EEUHD1C332","dia.12.5",20,null,22,16,3300,"N/A",1170,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.17,0.24,528,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUHD1C332","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK1C272S","dia.18",15,null,16.5,16,2700,36,2060,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.06,0.18,432,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK1C272S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","TA-A","Yes",null,null,null,"EEUTA1C222S","dia.18",20,null,22,16,2200,31,2250,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,2.25,0.18,352,100,null,"N/A",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUTA1C222S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1C182S","dia.18",15,null,16.5,16,1800,38,2000,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2,0.16,288,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1C182S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS1C122L","dia. 8",20,null,22,16,1200,30,1560,"105°C",null,"-40 to 105","105°C 9000H",null,2,"100kHz",null,1.56,0.16,192,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS1C122L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK1C102","dia.10",16,null,17.5,16,1000,49,1240,"105°C",null,"-55 to 105","105°C 4000H",null,2,"100kHz",null,1.24,0.16,160,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK1C102","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1C821","dia.10",20,null,22,16,820,52,1220,"105°C",null,"-55 to 105","105°C 3000H",null,2,"100kHz",null,1.22,0.16,131.19999999999999,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1C821","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1C681","dia.10",16,null,17,16,680,68,1050,"105°C",null,"-55 to 105","105°C 3000H",null,2,"100kHz",null,1.05,0.16,108.8,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1C681","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1C471L","dia. 8",15,null,16.5,16,470,85,730,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.73,0.16,75.2,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1C471L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA1CM471","dia. 8",11.5,null,12.5,16,470,"N/A",440," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.44,0.2,75.2,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1CM471","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","SU-A (Bi-polar)","No",null,null,null,"ECEA1CN331U","dia.10",16,null,17,16,330,"N/A",330," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.33,0.2,"N/A",200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1CN331U","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FM-A","No",null,null,null,"EEUFM1C121","dia. 6.3",11.2,null,12.7,16,120,130,455,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,0.45500000000000002,0.16,19.2,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFM1C121","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA1CM101","dia. 5",11,null,12,16,100,"N/A",180," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.18,0.2,16,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1CM101","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","GA-A","No",null,null,null,"EEAGA1C470","dia. 6.3",7,null,8,16,47,"N/A",77,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,7.6999999999999999E-2,0.18,7.5,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEAGA1C470","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","SU-A (Bi-polar)","No",null,null,null,"ECEA1CN330U","dia. 5",11,null,12,16,33,"N/A",80," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.08,0.2,"N/A",200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1CN330U","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KA-A (Bi-polar)","No",null,null,null,"ECEA1CKN220","dia. 6.3",7,null,8,16,22,"N/A",39," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,3.9E-2,0.16,17.600000000000001,200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1CKN220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KS-A","No",null,null,null,"ECEA1CKS220","dia. 5",5,null,6,16,22,"N/A",39," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,3.9E-2,0.16,3.5,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1CKS220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KA-A (Bi-polar)","No",null,null,null,"ECEA1CKN100","dia. 5",7,null,8,16,10,"N/A",25," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,2.5000000000000001E-2,0.16,10,200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1CKN100","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","HD-A","No",null,null,null,"EEUHD1E562","dia.16",25,null,27,25,5600,"N/A",1750,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.75,0.24,1400,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUHD1E562","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1E392L","dia.16",35.5,null,37.5,25,3900,16,3150,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,3.15,0.18,975,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1E392L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","TP-A","Yes",null,null,null,"EEUTP1E332","dia.16",31.5,null,33.5,25,3300,18,2710,"135°C",null,"-40 to 135","135°C 2000H",null,2,"100kHz",null,2.71,0.18,825,100,null,"N/A",-40,135,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUTP1E332","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1E272S","dia.16",20,null,22,25,2700,17,3300,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,3.3,0.16,675,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1E272S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK1E222L","dia.12.5",30,null,32,25,2200,18,2720,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.72,0.16,550,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK1E222L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","HD-A","No",null,null,null,"EEUHD1E222","dia.12.5",20,null,22,25,2200,"N/A",1090,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.0900000000000001,0.18,550,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUHD1E222","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FM-A","No",null,null,null,"EEUFM1E182S","dia.16",20,null,22,25,1800,17,3300,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,3.3,0.16,450,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFM1E182S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1E182","dia.16",20,null,22,25,1800,29,2205,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.2050000000000001,0.14000000000000001,450,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1E182","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK1E152S","dia.16",15,null,16.5,25,1500,38,1800,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.8,0.14000000000000001,375,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK1E152S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1E102L","dia.10",25,null,27,25,1000,18,2470,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,2.4700000000000002,0.14000000000000001,250,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1E102L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1E102S","dia.16",15,null,16.5,25,1000,43,1690,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.69,0.14000000000000001,250,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1E102S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1E821S","dia.12.5",20,null,22,25,820,38,1655,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.655,0.14000000000000001,205,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1E821S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1E561L","dia. 8",20,null,22,25,560,30,1560,"105°C",null,"-40 to 105","105°C 9000H",null,2,"100kHz",null,1.56,0.14000000000000001,140,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1E561L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1E471","dia.10",12.5,null,14,25,470,43,1290,"105°C",null,"-40 to 105","105°C 6000H",null,2,"100kHz",null,1.29,0.14000000000000001,117.5,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1E471","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","TA-A","Yes",null,null,null,"EEUTA1E471","dia.10",20,null,22,25,470,57,1100,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,1.1000000000000001,0.14000000000000001,117.5,200,null,"N/A",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUTA1E471","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","HD-A","No",null,null,null,"EEUHD1E471","dia.10",12.5,null,14,25,470,"N/A",380,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.38,0.16,117.5,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUHD1E471","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1E331","dia.10",12.5,null,13.5,25,330,90,755,"105°C",null,"-55 to 105","105°C 3000H",null,2,"100kHz",null,0.755,0.14000000000000001,82.5,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1E331","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FM-A","No",null,null,null,"EEUFM1E221","dia. 8",11.5,null,13,25,220,56,950,"105°C",null,"-40 to 105","105°C 3000H",null,2,"100kHz",null,0.95,0.14000000000000001,55,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFM1E221","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1E181","dia. 8",11.5,null,12.5,25,180,117,555,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.55500000000000005,0.14000000000000001,45,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1E181","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EB-A","No",null,null,null,"EEUEB1E101S","dia. 6.3",11.2,null,12.2,25,100,"N/A",95,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,9.5000000000000001E-2,0.22,25,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEB1E101S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1E470","dia. 5",11,null,12,25,47,800,175,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,0.17499999999999999,0.14000000000000001,11.7,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1E470","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","GA-A","No",null,null,null,"EEAGA1E330","dia. 6.3",7,null,8,25,33,"N/A",75,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,7.4999999999999997E-2,0.16,8.1999999999999993,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEAGA1E330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","GA-A (Bi-polar)","No",null,null,null,"ECA1EEN220","dia. 6.3",11.2,null,12.2,25,22,"N/A",60,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.06,0.15,19.5,200,null,"N/A",-40,105,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1EEN220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KS-A","No",null,null,null,"ECEA1EKS220","dia. 6.3",5,null,6,25,22,"N/A",55," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,5.5E-2,0.14000000000000001,5.5,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1EKS220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KS-A (Bi-polar)","No",null,null,null,"ECEA1ESN100","dia. 6.3",5,null,6,25,10,"N/A",28," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,2.8000000000000001E-2,0.2,12.5,200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1ESN100","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA1VHG472","dia.18",35.5,null,37.5,35,4700,"N/A",1910,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.91,0.2,1645,50,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1VHG472","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","TP-A","Yes",null,null,null,"EEUTP1V272","dia.18",31.5,null,33.5,35,2700,16,2900,"135°C",null,"-40 to 135","135°C 2000H",null,2,"100kHz",null,2.9,0.14000000000000001,945,50,null,"N/A",-40,135,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUTP1V272","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","TA-A","Yes",null,null,null,"EEUTA1V222","dia.18",35.5,null,37.5,35,2200,25,2790,"125°C",null,"-40 to 125","125°C 2000H",null,2,"100kHz",null,2.79,0.14000000000000001,770,50,null,"N/A",-40,125,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUTA1V222","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FK-A","Yes",null,null,null,"EEUFK1V182L","dia.12.5",35,null,37,35,1800,16,2940,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.94,0.12,630,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFK1V182L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1V152L","dia.12.5",30,null,32,35,1500,13,3630,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,3.63,0.12,525,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1V152L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS1V152","dia.12.5",25,null,27,35,1500,15,3190,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,3.19,0.12,525,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS1V152","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FM-A","No",null,null,null,"EEUFM1V122L","dia.12.5",30,null,32,35,1200,13,3630,"105°C",null,"-40 to 105","105°C 7000H",null,2,"100kHz",null,3.63,0.12,420,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFM1V122L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1V102","dia.12.5",25,null,27,35,1000,30,1945,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.9450000000000001,0.12,350,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1V102","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EB-A","No",null,null,null,"EEUEB1V102","dia.12.5",25,null,27,35,1000,"N/A",586,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,0.58599999999999997,0.18,350,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEB1V102","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FP-A","Yes",null,null,null,"EEUFP1V751","dia.10",20,null,22,35,750,52,3000,"105°C",null,"-55 to 105","105°C 4000H",null,2,"100kHz",null,3,0.12,262.5,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFP1V751","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1V681","dia.12.5",20,null,22,35,680,38,1655,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.655,0.12,238,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1V681","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1V471","dia.10",16,null,17.5,35,470,28,1790,"105°C",null,"-40 to 105","105°C 8000H",null,2,"100kHz",null,1.79,0.12,164.5,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1V471","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA1VM471","dia.10",16,null,17,35,470,"N/A",550," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.55000000000000004,0.14000000000000001,164.5,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1VM471","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1V391S","dia.12.5",15,null,16,35,390,65,1205,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.2050000000000001,0.12,136.5,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1V391S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1V331U","dia.10",12.5,null,14,35,330,43,1330,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,1.33,0.12,115.5,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1V331U","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","SU-A (Bi-polar)","No",null,null,null,"ECEA1VN331U","dia.12.5",20,null,22,35,330,"N/A",450," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.45,0.15,"N/A",200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1VN331U","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","TP-A","Yes",null,null,null,"EEUTP1V271","dia.10",16,null,17.5,35,270,130,945,"135°C",null,"-40 to 135","135°C 2000H",null,2,"100kHz",null,0.94499999999999995,0.12,94.5,200,null,"N/A",-40,135,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUTP1V271","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA1VM221","dia. 8",11.5,null,12.5,35,220,"N/A",350," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.35,0.14000000000000001,77,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1VM221","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1V101","dia. 8",11.5,null,13,35,100,56,950,"105°C",null,"-40 to 105","105°C 6000H",null,2,"100kHz",null,0.95,0.12,35,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1V101","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FM-A","No",null,null,null,"EEUFM1V680","dia. 6.3",11.2,null,12.7,35,68,130,455,"105°C",null,"-40 to 105","105°C 2000H",null,2,"100kHz",null,0.45500000000000002,0.12,23.8,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFM1V680","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA1VHG470","dia. 5",11,null,12,35,47,"N/A",90,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,0.09,0.14000000000000001,16.399999999999999,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1VHG470","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KA-A","No",null,null,null,"ECEA1VKA470Q","dia. 8",7,null,8,35,47,"N/A",85," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,8.5000000000000006E-2,0.12,16.399999999999999,"N/A",null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1VKA470Q","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KA-A","No",null,null,null,"ECEA1VKA330","dia. 6.3",7,null,8,35,33,"N/A",65," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,6.5000000000000002E-2,0.12,11.5,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1VKA330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KA-A","No",null,null,null,"ECEA1VKA100","dia. 5",7,null,8,35,10,"N/A",30," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,0.03,0.12,3.5,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1VKA100","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KA-A (Bi-polar)","No",null,null,null,"ECEA1VKN4R7","dia. 5",7,null,8,35,4.7,"N/A",22," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,2.1999999999999999E-2,0.14000000000000001,10,200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1VKN4R7","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1H222","dia.18",35.5,null,37.5,50,2200,23,3100,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,3.1,0.12,1100,50,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1H222","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1H152L","dia.16",35.5,null,37.5,50,1500,25,2790,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.79,0.1,750,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1H152L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA1HM102","dia.12.5",25,null,27,50,1000,"N/A",1050," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,1.05,0.12,500,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1HM102","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1H681L","dia.12.5",30,null,32,50,680,16,3160,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,3.16,0.1,340,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1H681L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1H561","dia.12.5",25,null,27,50,560,50,1832,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.8320000000000001,0.1,280,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1H561","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1H471","dia.12.5",20,null,22,50,470,22,2260,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,2.2599999999999998,0.1,235,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1H471","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA1HM471","dia.10",20,null,22,50,470,"N/A",650," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.65,0.12,235,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1HM471","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS1H331","dia.10",20,null,22,50,330,23,1890,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,1.89,0.1,165,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS1H331","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1H271","dia.10",25,null,27,50,270,82,1200,"105°C",null,"-55 to 105","105°C 3000H",null,2,"100kHz",null,1.2,0.1,135,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1H271","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","HD-A","No",null,null,null,"EEUHD1H221","dia.10",12.5,null,14,50,220,"N/A",300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.12,110,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUHD1H221","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS1H151L","dia. 8",15,null,16.5,50,150,45,1140,"105°C",null,"-40 to 105","105°C 8000H",null,2,"100kHz",null,1.1399999999999999,0.1,75,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS1H151L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1H121","dia.10",12.5,null,13.5,50,120,162,615,"105°C",null,"-55 to 105","105°C 3000H",null,2,"100kHz",null,0.61499999999999999,0.1,60,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1H121","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA1HHG101","dia. 8",11.5,null,12.5,50,100,"N/A",180,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,0.18,0.12,50,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1HHG101","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1H560","dia. 6.3",11.2,null,12.7,50,56,140,405,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,0.40500000000000003,0.1,28,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1H560","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","HD-A","No",null,null,null,"EEUHD1H330","dia. 5",11,null,12.5,50,33,"N/A",90,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,0.09,0.12,16.5,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUHD1H330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KA-A","No",null,null,null,"ECEA1HKA330","dia. 8",7,null,8,50,33,"N/A",75," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,7.4999999999999997E-2,0.1,16.5,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1HKA330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","HD-A","No",null,null,null,"EEUHD1H220","dia. 5",11,null,12.5,50,22,"N/A",65,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,6.5000000000000002E-2,0.12,11,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUHD1H220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KS-A","No",null,null,null,"ECEA1HKS220","dia. 8",5,null,6,50,22,"N/A",60," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,0.06,0.1,11,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1HKS220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","GA-A (Bi-polar)","No",null,null,null,"ECA1HEN100","dia. 6.3",11.2,null,12.2,50,10,"N/A",50,"105°C",null,"-40 to 105","105°C 1000H",null,2,"100kHz",null,0.05,0.15,18,200,null,"N/A",-40,105,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1HEN100","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA1HHG4R7","dia. 5",11,null,12,50,4.7,"N/A",26,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,2.5999999999999999E-2,0.12,3,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1HHG4R7","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","KA-A (Bi-polar)","No",null,null,null,"ECEA1HKN4R7","dia. 6.3",7,null,8,50,4.7,"N/A",23," 85°C",null,"-40 to  85"," 85°C 1000H",null,2,"100kHz",null,2.3E-2,0.12,11.7,200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1HKN4R7","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA1HHG3R3","dia. 5",11,null,12,50,3.3,"N/A",22,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,2.1999999999999999E-2,0.12,3,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1HHG3R3","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1H2R2","dia. 5",11,null,12,50,2.2000000000000002,1800,45,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,4.4999999999999998E-2,0.1,3,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1H2R2","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","SU-A (Bi-polar)","No",null,null,null,"ECEA1HN2R2U","dia. 5",11,null,12,50,2.2000000000000002,"N/A",18," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,1.7999999999999999E-2,0.15,"N/A",200,null,"N/A",-40,85,"Bipolar",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECEA1HN2R2U","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Bipolar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS1J102","dia.16",25,null,27,63,1000,24,2988,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,2.988,0.09,630,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS1J102","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1J821S","dia.18",25,null,27,63,820,43,2585,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,2.585,0.08,516.6,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1J821S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1J561S","dia.16",20,null,22,63,560,29,2153,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,2.153,0.09,352.8,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1J561S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS1J391","dia.12.5",20,null,22,63,390,33,1582,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,1.5820000000000001,0.09,245.7,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS1J391","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1J391","dia.12.5",25,null,27,63,390,70,1720,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.72,0.08,245.7,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1J391","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA1JHG331","dia.10",20,null,22,63,330,"N/A",510,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.51,0.1,207.9,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1JHG331","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA1JHG221","dia.10",16,null,17,63,220,"N/A",335,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.33500000000000002,0.1,138.6,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1JHG221","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1J181S","dia.12.5",15,null,16,63,180,150,1020,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.02,0.08,113.4,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1J181S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1J101L","dia. 8",15,null,16.5,63,100,68,741,"105°C",null,"-40 to 105","105°C 8000H",null,2,"100kHz",null,0.74099999999999999,0.09,63,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1J101L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA1JM101","dia. 8",11.5,null,12.5,63,100,"N/A",270," 85°C",null,"-40 to  85"," 85°C 2000H",null,2,"100kHz",null,0.27,0.11,63,200,null,"N/A",-40,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA1JM101","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC1J330","dia. 6.3",11.2,null,12.2,63,33,1000,240,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,0.24,0.08,20.7,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC1J330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FR-A","No",null,null,null,"EEUFR1J180","dia. 5",11,null,12.5,63,18,510,175,"105°C",null,"-40 to 105","105°C 5000H",null,2,"100kHz",null,0.17499999999999999,0.09,11.3,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFR1J180","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS1K681","dia.16",25,null,27,80,680,25,2500,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,2.5,0.08,544,100,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS1K681","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS1K391","dia.12.5",25,null,27,80,390,34,1800,"105°C",null,"-40 to 105","105°C10000H",null,2,"100kHz",null,1.8,0.08,312,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS1K391","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS1K560","dia. 8",11.5,null,13,80,56,160,490,"105°C",null,"-40 to 105","105°C 6000H",null,2,"100kHz",null,0.49,0.08,44.8,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS1K560","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA2AHG471","dia.16",25,null,27,100,470,"N/A",715,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.71499999999999997,0.08,470,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2AHG471","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC2A271L","dia.12.5",40,null,42,100,270,72,1130,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,1.1299999999999999,7.0000000000000007E-2,270,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC2A271L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC2A181","dia.16",20,null,22,100,180,110,995,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,0.995,7.0000000000000007E-2,180,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC2A181","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC2A101","dia.12.5",20,null,22,100,100,180,671,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,0.67100000000000004,7.0000000000000007E-2,100,100,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC2A101","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FS-A","No",null,null,null,"EEUFS2A390","dia. 8",15,null,16.5,100,39,112,590,"105°C",null,"-40 to 105","105°C 8000H",null,2,"100kHz",null,0.59,0.08,39,200,null,"N/A",-40,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFS2A390","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","FC-A","Yes",null,null,null,"EEUFC2A390L","dia. 8",20,null,22,100,39,330,455,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.45500000000000002,7.0000000000000007E-2,39,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUFC2A390L","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA2AHG220","dia. 6.3",11.2,null,12.2,100,22,"N/A",93,"105°C",null,"-55 to 105","105°C 1000H",null,2,"100kHz",null,9.2999999999999999E-2,0.08,22,200,null,"N/A",-55,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2AHG220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EE-A","No",null,null,null,"EEUEE2C331","dia.18",31.5,null,33.5,160,330,"N/A",2600,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,2.6,0.15,3178,50,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEE2C331","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EE-A","No",null,null,null,"EEUEE2C221","dia.16",31.5,null,33.5,160,220,"N/A",2280,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,2.2799999999999998,0.15,2122,100,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEE2C221","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EB-A","No",null,null,null,"EEUEB2C101S","dia.18",20,null,22,160,100,"N/A",1060,"105°C",null,"-25 to 105","105°C 5000H",null,2,"100kHz",null,1.06,0.15,160,100,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEB2C101S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EB-A","No",null,null,null,"EEUEB2C680","dia.12.5",25,null,27,160,68,"N/A",750,"105°C",null,"-25 to 105","105°C 5000H",null,2,"100kHz",null,0.75,0.15,108.8,200,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEB2C680","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA2CHG220","dia.10",20,null,22,160,22,"N/A",130,"105°C",null,"-25 to 105","105°C 2000H",null,2,"100kHz",null,0.13,0.15,221.2,200,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2CHG220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA2CM2R2","dia. 6.3",11.2,null,12.2,160,2.2000000000000002,"N/A",53," 85°C",null,"-25 to  85"," 85°C 2000H",null,2,"100kHz",null,5.2999999999999999E-2,0.16,31.1,200,null,"N/A",-25,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2CM2R2","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EB-A","No",null,null,null,"EEUEB2D151","dia.16",31.5,null,33.5,200,150,"N/A",1280,"105°C",null,"-25 to 105","105°C 5000H",null,2,"100kHz",null,1.28,0.15,300,100,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEB2D151","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EB-A","No",null,null,null,"EEUEB2D101S","dia.18",20,null,22,200,100,"N/A",1060,"105°C",null,"-25 to 105","105°C 5000H",null,2,"100kHz",null,1.06,0.15,200,100,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEB2D101S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EE-A","No",null,null,null,"EEUEE2D680S","dia.16",20,null,22,200,68,"N/A",1330,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.33,0.15,826,100,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEE2D680S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA2DHG330","dia.12.5",20,null,22,200,33,"N/A",190,"105°C",null,"-25 to 105","105°C 2000H",null,2,"100kHz",null,0.19,0.15,406,200,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2DHG330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA2DHG2R2","dia. 6.3",11.2,null,12.2,200,2.2000000000000002,"N/A",25,"105°C",null,"-25 to 105","105°C 2000H",null,2,"100kHz",null,2.5000000000000001E-2,0.15,36.4,200,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2DHG2R2","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA2EM101","dia.16",31.5,null,33.5,250,100,"N/A",530," 85°C",null,"-25 to  85"," 85°C 2000H",null,2,"100kHz",null,0.53,0.18,1510,100,null,"N/A",-25,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2EM101","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EB-A","No",null,null,null,"EEUEB2E680","dia.16",25,null,27,250,68,"N/A",990,"105°C",null,"-25 to 105","105°C 5000H",null,2,"100kHz",null,0.99,0.15,170,100,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEB2E680","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA2EM220","dia.10",20,null,22,250,22,"N/A",180," 85°C",null,"-25 to  85"," 85°C 2000H",null,2,"100kHz",null,0.18,0.18,340,200,null,"N/A",-25,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2EM220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA2EHG100","dia.10",16,null,17,250,10,"N/A",88,"105°C",null,"-25 to 105","105°C 2000H",null,2,"100kHz",null,8.7999999999999995E-2,0.15,160,200,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2EHG100","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EB-A","No",null,null,null,"EEUEB2V680","dia.16",31.5,null,33.5,350,68,"N/A",780,"105°C",null,"-25 to 105","105°C 5000H",null,2,"100kHz",null,0.78,0.2,238,100,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEB2V680","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EE-A","No",null,null,null,"EEUEE2V470S","dia.18",20,null,22,350,47,"N/A",1070,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.07,0.2,997,100,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEE2V470S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EE-A","No",null,null,null,"EEUEE2V220","dia.12.5",20,null,22,350,22,"N/A",660,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.66,0.2,472,200,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEE2V220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA2VHG3R3","dia.10",12.5,null,13.5,350,3.3,"N/A",38,"105°C",null,"-25 to 105","105°C 2000H",null,2,"100kHz",null,3.7999999999999999E-2,0.2,79.3,200,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2VHG3R3","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EE-A","No",null,null,null,"EEUEE2G820","dia.18",31.5,null,33.5,400,82,"N/A",1645,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.645,0.24,1978,50,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEE2G820","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EB-A","No",null,null,null,"EEUEB2G220","dia.12.5",25,null,27,400,22,"N/A",410,"105°C",null,"-25 to 105","105°C 5000H",null,2,"100kHz",null,0.41,0.24,88,200,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEB2G220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","NHG-A","Yes",null,null,null,"ECA2GHG100","dia.10",20,null,22,400,10,"N/A",80,"105°C",null,"-25 to 105","105°C 2000H",null,2,"100kHz",null,0.08,0.24,250,200,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2GHG100","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA2GM2R2","dia. 8",11.5,null,12.5,400,2.2000000000000002,"N/A",50," 85°C",null,"-25 to  85"," 85°C 2000H",null,2,"100kHz",null,0.05,0.2,62.8,200,null,"N/A",-25,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2GM2R2","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EE-A","No",null,null,null,"EEUEE2W470","dia.16",31.5,null,33.5,450,47,"N/A",1200,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.2,0.24,1279,100,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEE2W470","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","EB-A","No",null,null,null,"EEUEB2W220S","dia.18",20,null,22,450,22,"N/A",560,"105°C",null,"-25 to 105","105°C 5000H",null,2,"100kHz",null,0.56000000000000005,0.24,99,100,null,"N/A",-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUEB2W220S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz","Polar"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","M-A","No",null,null,null,"ECA2WM4R7","dia.10",20,null,22,450,4.7,"N/A",79," 85°C",null,"-25 to  85"," 85°C 2000H",null,2,"100kHz",null,7.9000000000000001E-2,0.2,136.9,200,null,"N/A",-25,85,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/ECA2WM4R7","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","120Hz","Polar"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS (HF)","Yes",null,null,null,"EEEFK1A221SL","dia. 6.3",5.8,null,6.1,10,220,680,240,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.24,0.19,22,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1A221SL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS (HF)","Yes",null,null,null,"EEEFK1C102SL","dia.10",10.199999999999999,null,10.5,16,1000,360,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.16,160,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1C102SL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS (HF)","Yes",null,null,null,"EEEFKE181XSL","dia. 6.3",7.7,null,8,25,180,880,280,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.28000000000000003,0.14000000000000001,45,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFKE181XSL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS (HF)","Yes",null,null,null,"EEEFK1J121SL","dia.10",10.199999999999999,null,10.5,63,120,350,400,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.4,0.08,75.599999999999994,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1J121SL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FKS (HF)","Yes",null,null,null,"EEEFK1K470SL","dia. 8",10.199999999999999,null,10.5,80,47,1300,130,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.13,0.08,37.6,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1K470SL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (HF)","Yes",null,null,null,"EEEFK1H221L","dia.10",10.199999999999999,null,10.5,50,220,180,670,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.67,0.1,110,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1H221L","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (HF)","Yes",null,null,null,"EEEFK1J101L","dia.10",10.199999999999999,null,10.5,63,100,350,400,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.4,0.08,63,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1J101L","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (HF)","Yes",null,null,null,"EEEFK0J471GL","dia. 8",10.199999999999999,null,10.5,6.3,470,160,600,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,0.6,0.26,29.61,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK0J471GL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (HF)","Yes",null,null,null,"EEEFK1C681GL","dia.10",10.199999999999999,null,10.5,16,680,80,850,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,0.85,0.16,108.8,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1C681GL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (HF)","Yes",null,null,null,"EEEFK1V151GL","dia. 8",10.199999999999999,null,10.5,35,150,160,600,"105°C",null,"-55 to 105","105°C 5000H",null,2,"100kHz",null,0.6,0.12,52.5,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1V151GL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (HF, LF reflow)","Yes",null,null,null,"EEEFK1A151AL","dia. 6.3",5.8,null,6.1,10,150,360,240,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.24,0.19,15,1000,null,"D",-55,105,"Halogen-free, Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1A151AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (HF, LF reflow)","Yes",null,null,null,"EEEFK1C101AL","dia. 6.3",5.8,null,6.1,16,100,360,240,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.24,0.16,16,1000,null,"D",-55,105,"Halogen-free, Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1C101AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (HF, LF reflow)","Yes",null,null,null,"EEEFKC221XAL","dia. 6.3",7.7,null,8,16,220,340,280,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.28000000000000003,0.16,35.200000000000003,900,null,"D8",-55,105,"Halogen-free, Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFKC221XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (HF, LF reflow)","Yes",null,null,null,"EEEFK1E101AL","dia. 8",6.2,null,6.5,25,100,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.14000000000000001,25,1000,null,"E",-55,105,"Halogen-free, Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1E101AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FK (HF, LF reflow)","Yes",null,null,null,"EEEFK1V101AL","dia. 8",10.199999999999999,null,10.5,35,100,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.12,35,500,null,"F",-55,105,"Halogen-free, Lead-free Reflow",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFK1V101AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN (HF)","Yes",null,null,null,"EEEFN0J182UL","dia.10",10.199999999999999,null,10.5,6.3,1800,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.26,113.4,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN0J182UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN (HF)","Yes",null,null,null,"EEEFN1A122UL","dia.10",10.199999999999999,null,10.5,10,1200,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.19,120,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1A122UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN (HF)","Yes",null,null,null,"EEEFN1C102UL","dia.10",10.199999999999999,null,10.5,16,1000,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.16,160,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1C102UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN (HF)","Yes",null,null,null,"EEEFNE151XUL","dia. 6.3",7.7,null,8,25,150,340,280,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.28000000000000003,0.14000000000000001,37.5,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFNE151XUL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN (HF)","Yes",null,null,null,"EEEFN1V331UL","dia. 8",10.199999999999999,null,10.5,35,330,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.12,115.5,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1V331UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN (HF)","Yes",null,null,null,"EEEFN1V471UL","dia.10",10.199999999999999,null,10.5,35,470,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.12,164.5,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1V471UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN (HF)","Yes",null,null,null,"EEEFN1J100L","dia. 6.3",5.8,null,6.1,63,10,1500,80,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.08,0.08,6.3,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1J100L","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN (HF)","Yes",null,null,null,"EEEFN1K100XL","dia. 6.3",7.7,null,8,80,10,2400,60,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.06,0.08,8,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN1K100XL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FN (HF)","Yes",null,null,null,"EEEFN2A470UL","dia.10",10.199999999999999,null,10.5,100,47,700,200,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.2,7.0000000000000007E-2,47,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFN2A470UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1A471AL","dia. 8",10.199999999999999,null,10.5,10,470,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.19,47,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1A471AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1A681AL","dia. 8",10.199999999999999,null,10.5,10,680,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.19,68,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1A681AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1A102AL","dia.10",10.199999999999999,null,10.5,10,1000,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.19,100,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1A102AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFPA122UAL","dia.10",10.199999999999999,null,10.5,10,1200,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.19,120,500,null,"(G)",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPA122UAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1C470AL","dia. 6.3",5.8,null,6.1,16,47,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.16,7.52,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1C470AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1C680AL","dia. 6.3",5.8,null,6.1,16,68,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.16,10.88,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1C680AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1C101AL","dia. 6.3",5.8,null,6.1,16,100,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.16,16,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1C101AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFPC101XAL","dia. 6.3",7.7,null,8,16,100,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.16,16,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPC101XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFPC151XAL","dia. 6.3",7.7,null,8,16,150,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.16,24,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPC151XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFPC221XAL","dia. 6.3",7.7,null,8,16,220,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.16,35.200000000000003,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPC221XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1C221AL","dia. 8",6.2,null,6.5,16,220,180,500,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.5,0.16,35.200000000000003,1000,null,"E",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1C221AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1C331AL","dia. 8",10.199999999999999,null,10.5,16,330,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.16,52.8,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1C331AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1C471AL","dia. 8",10.199999999999999,null,10.5,16,470,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.16,75.2,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1C471AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1C681AL","dia.10",10.199999999999999,null,10.5,16,680,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.16,108.8,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1C681AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFPC821UAL","dia.10",10.199999999999999,null,10.5,16,820,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.16,131.19999999999999,500,null,"(G)",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPC821UAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1E330AL","dia. 6.3",5.8,null,6.1,25,33,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.14000000000000001,8.25,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1E330AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1E470AL","dia. 6.3",5.8,null,6.1,25,47,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.14000000000000001,11.75,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1E470AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1E680AL","dia. 6.3",5.8,null,6.1,25,68,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.14000000000000001,17,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1E680AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFPE101XAL","dia. 6.3",7.7,null,8,25,100,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.14000000000000001,25,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPE101XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1E101AL","dia. 8",6.2,null,6.5,25,100,180,500,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.5,0.14000000000000001,25,1000,null,"E",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1E101AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1E151AL","dia. 8",10.199999999999999,null,10.5,25,150,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.14000000000000001,37.5,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1E151AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1E221AL","dia. 8",10.199999999999999,null,10.5,25,220,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.14000000000000001,55,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1E221AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1E331AL","dia. 8",10.199999999999999,null,10.5,25,330,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.14000000000000001,82.5,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1E331AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1E471AL","dia.10",10.199999999999999,null,10.5,25,470,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.14000000000000001,117.5,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1E471AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFPE561UAL","dia.10",10.199999999999999,null,10.5,25,560,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.14000000000000001,140,500,null,"(G)",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPE561UAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1V330AL","dia. 6.3",5.8,null,6.1,35,33,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.12,11.55,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1V330AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1V470AL","dia. 6.3",5.8,null,6.1,35,47,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.12,16.45,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1V470AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFPV680XAL","dia. 6.3",7.7,null,8,35,68,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.12,23.8,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPV680XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFPV101XAL","dia. 6.3",7.7,null,8,35,100,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.12,35,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPV101XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1V101AL","dia. 8",10.199999999999999,null,10.5,35,100,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.12,35,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1V101AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1V151AL","dia. 8",10.199999999999999,null,10.5,35,150,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.12,52.5,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1V151AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1V221AL","dia. 8",10.199999999999999,null,10.5,35,220,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.12,77,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1V221AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1V331AL","dia.10",10.199999999999999,null,10.5,35,330,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.12,115.5,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1V331AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFPV391UAL","dia.10",10.199999999999999,null,10.5,35,390,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.12,136.5,500,null,"(G)",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFPV391UAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1H101AL","dia. 8",10.199999999999999,null,10.5,50,100,180,670,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.67,0.1,50,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1H101AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FP (HF)","Yes",null,null,null,"EEEFP1H221AL","dia.10",10.199999999999999,null,10.5,50,220,120,900,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.9,0.1,110,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFP1H221AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT0J331AL","dia. 6.3",5.8,null,6.1,6.3,330,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.26,20.79,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT0J331AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFTJ471XAL","dia. 6.3",7.7,null,8,6.3,470,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.26,29.61,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFTJ471XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFTJ681XAL","dia. 6.3",7.7,null,8,6.3,680,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.26,42.84,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFTJ681XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT0J152AL","dia. 8",10.199999999999999,null,10.5,6.3,1500,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.26,94.5,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT0J152AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT0J222AL","dia.10",10.199999999999999,null,10.5,6.3,2200,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.28000000000000003,138.6,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT0J222AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1A221AL","dia. 6.3",5.8,null,6.1,10,220,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.19,22,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1A221AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFTA331XAL","dia. 6.3",7.7,null,8,10,330,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.19,33,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFTA331XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFTA471XAL","dia. 6.3",7.7,null,8,10,470,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.19,47,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFTA471XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1A102AL","dia. 8",10.199999999999999,null,10.5,10,1000,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.19,100,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1A102AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1A152AL","dia.10",10.199999999999999,null,10.5,10,1500,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.19,150,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1A152AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1C151AL","dia. 6.3",5.8,null,6.1,16,150,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.16,24,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1C151AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1C221AL","dia. 6.3",5.8,null,6.1,16,220,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.16,35.200000000000003,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1C221AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFTC331XAL","dia. 6.3",7.7,null,8,16,330,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.16,52.8,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFTC331XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1C681AL","dia. 8",10.199999999999999,null,10.5,16,680,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.16,108.8,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1C681AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1C821UL","dia. 8",10.199999999999999,null,10.5,16,820,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.16,131.19999999999999,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1C821UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1C102AL","dia.10",10.199999999999999,null,10.5,16,1000,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.16,160,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1C102AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1C122UL","dia.10",10.199999999999999,null,10.5,16,1200,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.16,192,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1C122UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1E101AL","dia. 6.3",5.8,null,6.1,25,100,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.14000000000000001,25,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1E101AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFTE151XAL","dia. 6.3",7.7,null,8,25,150,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.14000000000000001,37.5,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFTE151XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFTE221XAL","dia. 6.3",7.7,null,8,25,220,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.14000000000000001,55,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFTE221XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1E471AL","dia. 8",10.199999999999999,null,10.5,25,470,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.14000000000000001,117.5,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1E471AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1E561UL","dia. 8",10.199999999999999,null,10.5,25,560,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.14000000000000001,140,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1E561UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1E821AL","dia.10",10.199999999999999,null,10.5,25,820,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.14000000000000001,205,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1E821AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1E102UL","dia.10",10.199999999999999,null,10.5,25,1000,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.14000000000000001,250,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1E102UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1V680AL","dia. 6.3",5.8,null,6.1,35,68,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.12,23.8,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1V680AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1V101AL","dia. 6.3",5.8,null,6.1,35,100,260,300,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.3,0.12,35,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1V101AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFTV151XAL","dia. 6.3",7.7,null,8,35,150,160,600,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.6,0.12,52.5,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFTV151XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1V331AL","dia. 8",10.199999999999999,null,10.5,35,330,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.12,115.5,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1V331AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1V391UL","dia. 8",10.199999999999999,null,10.5,35,390,80,850,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.85,0.12,136.5,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1V391UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1V561AL","dia.10",10.199999999999999,null,10.5,35,560,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.12,196,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1V561AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1V681UL","dia.10",10.199999999999999,null,10.5,35,680,60,1190,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,1.19,0.12,238,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1V681UL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1H470AL","dia. 6.3",5.8,null,6.1,50,47,680,195,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.19500000000000001,0.1,23.5,1000,null,"D",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1H470AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFTH101XAL","dia. 6.3",7.7,null,8,50,100,340,350,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.35,0.1,50,900,null,"D8",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFTH101XAL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1H221AL","dia. 8",10.199999999999999,null,10.5,50,220,80,670,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.67,0.1,110,500,null,"F",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1H221AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"SMD","Can","Liquid Al","E-Cap","FT (HF)","Yes",null,null,null,"EEEFT1H331AL","dia.10",10.199999999999999,null,10.5,50,330,120,900,"105°C",null,"-55 to 105","105°C 2000H",null,2,"100kHz",null,0.9,0.1,165,500,null,"G",-55,105,"Halogen-free",null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-smd/models/EEEFT1H331AL","https://sigma.octopart.com/502833/image/Panasonic-EEEFK1H220P.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C220","dia.10",20,null,22,160,22,"N/A",500,"105°C",null,"-25 to 105","105°C 8000H",null,2,"100kHz",null,0.5,0.15,35.200000000000003,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C330","dia.10",20,null,22,160,33,"N/A",580,"105°C",null,"-25 to 105","105°C 8000H",null,2,"100kHz",null,0.57999999999999996,0.15,52.8,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C470","dia.10",20,null,22,160,47,"N/A",750,"105°C",null,"-25 to 105","105°C 8000H",null,2,"100kHz",null,0.75,0.15,75.2,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C470","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C680","dia.12.5",20,null,22,160,68,"N/A",950,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.95,0.15,108.8,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C680","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C820","dia.12.5",25,null,27,160,82,"N/A",1060,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.06,0.15,131.19999999999999,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C820","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C101","dia.12.5",25,null,27,160,100,"N/A",1170,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.17,0.15,160,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C101","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C101S","dia.16",20,null,22,160,100,"N/A",1280,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.28,0.15,160,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C101S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C151","dia.16",25,null,27,160,150,"N/A",1400,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.4,0.15,240,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C151","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C151S","dia.18",20,null,22,160,150,"N/A",1400,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.4,0.15,240,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C151S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C221","dia.16",31.5,null,33.5,160,220,"N/A",1700,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.7,0.15,352,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C221","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C221S","dia.18",25,null,27,160,220,"N/A",1500,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.5,0.15,352,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C221S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2C331","dia.18",31.5,null,33.5,160,330,"N/A",2000,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,2,0.15,528,50,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2C331","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2D220","dia.10",20,null,22,200,22,"N/A",600,"105°C",null,"-25 to 105","105°C 8000H",null,2,"100kHz",null,0.6,0.15,44,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2D220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2D330","dia.10",20,null,22,200,33,"N/A",650,"105°C",null,"-25 to 105","105°C 8000H",null,2,"100kHz",null,0.65,0.15,66,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2D330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2D470","dia.12.5",20,null,22,200,47,"N/A",790,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.79,0.15,94,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2D470","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2D680","dia.12.5",25,null,27,200,68,"N/A",950,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.95,0.15,136,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2D680","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2D680S","dia.16",20,null,22,200,68,"N/A",1000,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1,0.15,136,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2D680S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2D820S","dia.16",20,null,22,200,82,"N/A",1100,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.1000000000000001,0.15,164,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2D820S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2D101","dia.16",25,null,27,200,100,"N/A",1300,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.3,0.15,200,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2D101","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2D101S","dia.18",20,null,22,200,100,"N/A",1280,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.28,0.15,200,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2D101S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2D151","dia.16",25,null,27,200,150,"N/A",1400,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.4,0.15,300,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2D151","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2D221","dia.18",31.5,null,33.5,200,220,"N/A",2000,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,2,0.15,440,50,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2D221","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2D331","dia.18",40,null,42,200,330,"N/A",2400,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,2.4,0.15,660,50,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2D331","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2E220","dia.10",20,null,22,250,22,"N/A",560,"105°C",null,"-25 to 105","105°C 8000H",null,2,"100kHz",null,0.56000000000000005,0.15,55,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2E220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2E330","dia.12.5",20,null,22,250,33,"N/A",710,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.71,0.15,82.5,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2E330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2E470","dia.12.5",25,null,27,250,47,"N/A",920,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.92,0.15,117.5,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2E470","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2E470S","dia.16",20,null,22,250,47,"N/A",990,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.99,0.15,117.5,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2E470S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2E680S","dia.16",20,null,22,250,68,"N/A",1000,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1,0.15,170,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2E680S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2E820","dia.16",25,null,27,250,82,"N/A",1200,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.2,0.15,205,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2E820","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2E820S","dia.18",20,null,22,250,82,"N/A",1200,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.2,0.15,205,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2E820S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2E101","dia.16",31.5,null,33.5,250,100,"N/A",1500,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.5,0.15,250,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2E101","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2E101S","dia.18",25,null,27,250,100,"N/A",1500,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.5,0.15,250,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2E101S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2E151","dia.18",31.5,null,33.5,250,150,"N/A",1800,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.8,0.15,375,50,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2E151","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2E221","dia.18",40,null,42,250,220,"N/A",2100,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,2.1,0.15,550,50,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2E221","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2V100","dia.10",20,null,22,350,10,"N/A",350,"105°C",null,"-25 to 105","105°C 8000H",null,2,"100kHz",null,0.35,0.2,35,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2V100","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2V220","dia.12.5",20,null,22,350,22,"N/A",480,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.48,0.2,77,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2V220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2V330S","dia.16",20,null,22,350,33,"N/A",640,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.64,0.2,115.5,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2V330S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2V470","dia.16",25,null,27,350,47,"N/A",800,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.8,0.2,164.5,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2V470","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2V470S","dia.18",20,null,22,350,47,"N/A",800,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.8,0.2,164.5,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2V470S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2V680","dia.16",31.5,null,33.5,350,68,"N/A",1100,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.1000000000000001,0.2,238,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2V680","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2V680S","dia.18",25,null,27,350,68,"N/A",1000,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1,0.2,238,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2V680S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2V820S","dia.18",25,null,27,350,82,"N/A",1100,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.1000000000000001,0.2,287,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2V820S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","NRND","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2V101","dia.18",31.5,null,33.5,350,100,"N/A",1200,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,1.2,0.2,350,50,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2V101","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2G100","dia.10",20,null,22,400,10,"N/A",300,"105°C",null,"-25 to 105","105°C 8000H",null,2,"100kHz",null,0.3,0.24,40,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2G100","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2G150","dia.12.5",20,null,22,400,15,"N/A",410,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.41,0.24,60,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2G150","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2G220","dia.12.5",25,null,27,400,22,"N/A",500,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.5,0.24,88,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2G220","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2G220S","dia.16",20,null,22,400,22,"N/A",600,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.6,0.24,88,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2G220S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2G330S","dia.16",20,null,22,400,33,"N/A",730,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.73,0.24,132,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2G330S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2G470","dia.16",25,null,27,400,47,"N/A",840,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.84,0.24,188,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2G470","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2G470S","dia.18",20,null,22,400,47,"N/A",840,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.84,0.24,188,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2G470S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2W100","dia.12.5",20,null,22,450,10,"N/A",350,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.35,0.24,45,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2W100","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2W150","dia.12.5",25,null,27,450,15,"N/A",560,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.56000000000000005,0.24,67.5,200,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2W150","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2W220S","dia.16",20,null,22,450,22,"N/A",680,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.68,0.24,99,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2W220S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
[null,null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2W330","dia.16",31.5,null,33.5,450,33,"N/A",850,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.85,0.24,148.5,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2W330","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]
["E-cap End",null,null,null,"Open","Std","Panasonic",null,"THD","Can","Liquid Al","E-Cap","ED-A","No",null,null,null,"EEUED2W330S","dia.18",25,null,27,450,33,"N/A",850,"105°C",null,"-25 to 105","105°C10000H",null,2,"100kHz",null,0.85,0.24,148.5,100,null,null,-25,105,null,null,null,null,null,null,null,"https://industrial.panasonic.com/ww/products/pt/aluminum-cap-lead/models/EEUED2W330S","https://sigma.octopart.com/21429079/image/Panasonic-ECA1JM101B.jpg","100kHz"]

{"sheet":"Cross PN","index":4,"n_rows":743,"n_cols":56,"rows_kept":743,"cut":false,"hidden":true,"merged":[[0,0,0,4],[9,42,10,42],[7,42,8,42]]}
["Panasonic Capacitor \ncross reference tool"]
[]
[null,"Comparative Finder",null,null,null,null,null,null,null,null,null,"List",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"For function"]
[null,"Type","# of T","Area","Max H","Volt.","Cap.","ESR","Ripple","Max T",null,"#","Status","Part Number","Spec Summary (Type, V uF, ESR, Ripple, Size, Endurance)","Product \n(Series)","Maker",null,"Type","# of Terminal","LxW (mm)","H (mm)","Volt (V)","Cap (uF)","ESR (mΩ)","Ir (Arms)","Tupper(°C)","Endurance",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,">100KHz?","f ESR","Type List","Area List","Area Lock","Height Lock","Pakcage","Product List","Maker Lock","Automotive?"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"\nIFERROR(IF(N5=\"\",\"\",IF(AND(B5=S5,C5=T5,D5=U5,E5=V5,F5=W5,G5=X5,H5=Y5,I5=Z5,J5=AA5),\"←\",\"\")),\"\")","v":""},{"$f":"\nIF(N5=\"\",\"\",\"0.\")","v":""},{"$f":"\nIF(N5=0,\"\",INDEX('All Data'!$F:$F,MATCH(N5,'All Data'!$R:$R,0)))","v":""},null,{"$f":"IF(N5=0,\"\",\nCONCATENATE(S5,\", \",W5,\"V \",X5,\"uF, \",Y5,\"mΩ\",AU5,\", \",Z5,\"A\",\", \",U5,\" x \",V5,\" mm\",IF(T5=3,\"(3-T)\",\"\"),\", \",IF(N5=\"\",\"\",AB5)))","v":""},{"$f":"IF(N5=\"\",\"\",\nINDEX('All Data'!$L:$L,MATCH(N5,'All Data'!$R:$R,0))&\" (\"&INDEX('All Data'!$M:$M,MATCH(N5,'All Data'!$R:$R,0))&\")\")","v":""},{"$f":"IF(N5=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N5,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(N5=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N5,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(N5=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N5,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(N5=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N5,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(N5=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N5,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(N5=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N5,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(N5=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N5,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(N5=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N5,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(N5=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N5,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(N5=\"\",\"\",IF(INDEX('All Data'!$AI:$AI,MATCH(N5,'All Data'!$R:$R,0))=\"-\",0,INDEX('All Data'!$AI:$AI,MATCH(N5,'All Data'!$R:$R,0))))","v":""},{"$f":"\nIF(N5=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N5,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIF(N5=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N5,'All Data'!$R:$R,0)))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(COUNTIF(AV5,\"500kHz\"),\"@500kHz\",IF(COUNTIF(AV5,\"300kHz\"),\"@300kHz\",\"\"))","v":""},{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N5,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}},null,null,"yes","yes"]
[null,"Type","# of T","Area (mm)","Max H (mm)","Volt. (V)","Cap. (uF)","ESR (mΩ)","Ir (Arms)","Max T(°C)",null,"#","Status","Part Number","Type, Voltage Cap., ESR, Ripple, Size","Product (Series)","Maker","Car","T","#2","A","H","V","C","R","I","Tu","E",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SMD","3.5x2.8(B)","no","no","Mold","SP-Cap","Panasonic","yes"]
[null,{"$f":"\nS7","v":""},"","","","","","","","",{"$f":"\nIF(L7=\"\",\"\",\"→\")","v":""},{"$f":"\nIF(B7=\"\",\"\",CONCATENATE(ROW()-6,\". \"))","v":""},{"$f":"\nIF(B7=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N7,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!#REF!","v":{"$error":"#REF!"}},{"$f":"IF(M7=\"\",\"\",\nCONCATENATE(S7,\", \",W7,\"V \",X7,\"uF, \",Y7,\"mΩ\",AU7,\", \",Z7,\"A\",\", \",U7,\" x \",V7,\" mm\",IF(T7=3,\"(3-T)\",\"\"),\", \",IF(N7=\"\",\"\",AB7)))","v":""},{"$f":"\nIF(M7=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N7,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N7,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M7=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N7,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N7=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N7,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N7=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N7,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N7=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N7,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N7=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N7,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N7=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N7,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N7=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N7,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N7=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N7,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N7=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N7,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N7=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N7,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N7=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N7,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N7=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N7,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,"Lock",null,null,null,null,null,null,{"$f":"IF(COUNTIF(AV7,\"500kHz\"),\"@500kHz\",IF(COUNTIF(AV7,\"300kHz\"),\"@300kHz\",\"\"))","v":""},{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N7,'All Data'!$R:$R,0))","v":{"$error":"#REF!"}},"THD","7.3x4.3(D)",null,null,"Can","POSCAP","KEMET","no"]
[null,"","","","","","","","","",{"$f":"\nIF(L8=\"\",\"\",\"→\")","v":""},"",{"$f":"\nIF(B8=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N8,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!#REF!","v":{"$error":"#REF!"}},"",{"$f":"\nIF(M8=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N8,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N8,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M8=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N8,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N8=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N8,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N8=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N8,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N8=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N8,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N8=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N8,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N8=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N8,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N8=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N8,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N8=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N8,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N8=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N8,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N8=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N8,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N8=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N8,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N8=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N8,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,"Range",null,null,null,null,null,"=Area",null,"Product",null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N8,'All Data'!$R:$R,0))","v":{"$error":"#REF!"}},null,"dia. 4",null,null,null,"OS-CON","NEC"]
[null,"","","","","","","","","","","",{"$f":"\nIF(B9=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N9,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!#REF!","v":{"$error":"#REF!"}},"",{"$f":"\nIF(M9=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N9,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N9,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M9=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N9,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N9=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N9,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N9=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N9,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N9=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N9,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N9=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N9,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N9=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N9,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N9=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N9,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N9=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N9,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N9=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N9,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N9=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N9,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N9=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N9,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N9=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N9,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,"Volt.","Cap.","ESR","Max T",null,"≤Height","Package",null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N9,'All Data'!$R:$R,0))","v":{"$error":"#REF!"}},null,"dia. 5",null,null,null,"Hybrid","AVX"]
[null,"","","","","","","","","","","",{"$f":"\nIF(B10=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N10,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ31","v":0},"",{"$f":"\nIF(M10=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N10,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N10,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M10=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N10,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N10=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N10,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N10=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N10,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N10=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N10,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N10=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N10,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N10=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N10,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N10=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N10,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N10=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N10,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N10=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N10,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N10=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N10,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N10=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N10,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N10=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N10,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,"Upper",5,5,5,2,null,"yes",null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N10,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}},null,"dia. 6.3",null,null,null,"E-Cap","Murata"]
[null,"","","","","","","","","","","",{"$f":"\nIF(B11=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N11,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ32","v":0},"",{"$f":"\nIF(M11=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N11,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N11,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M11=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N11,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N11=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N11,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N11=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N11,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N11=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N11,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N11=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N11,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N11=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N11,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N11=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N11,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N11=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N11,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N11=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N11,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N11=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N11,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N11=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N11,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N11=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N11,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,"Lower",1,0.1,"no limit",0.5,null,"no",null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N11,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}},null,"dia. 8",null,null,null,null,"Rohm"]
[null,"","","","","","","","","","","",{"$f":"\nIF(B12=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N12,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!#REF!","v":{"$error":"#REF!"}},"",{"$f":"\nIF(M12=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N12,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N12,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M12=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N12,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N12=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N12,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N12=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N12,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N12=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N12,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N12=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N12,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N12=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N12,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N12=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N12,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N12=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N12,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N12=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N12,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N12=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N12,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N12=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N12,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N12=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N12,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N12,'All Data'!$R:$R,0))","v":{"$error":"#REF!"}},null,"dia.10",null,null,null,null,"Nippon Chemi-con"]
[null,"","","","","","","","","","","",{"$f":"\nIF(B13=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N13,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ33","v":0},"",{"$f":"\nIF(M13=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N13,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N13,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M13=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N13,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N13=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N13,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N13=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N13,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N13=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N13,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N13=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N13,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N13=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N13,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N13=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N13,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N13=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N13,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N13=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N13,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N13=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N13,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N13=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N13,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N13=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N13,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,"Quick Set",null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N13,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}},null,"dia.12.5",null,null,null,null,"nichicon"]
[null,"","","","","","","","","","","",{"$f":"\nIF(B14=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N14,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ34","v":0},"",{"$f":"\nIF(M14=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N14,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N14,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M14=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N14,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N14=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N14,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N14=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N14,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N14=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N14,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N14=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N14,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N14=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N14,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N14=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N14,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N14=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N14,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N14=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N14,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N14=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N14,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N14=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N14,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N14=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N14,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,"Search For",null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N14,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}},null,"dia.16",null,null,null,null,"Rubycon"]
[null,"","","","","","","","","","","",{"$f":"\nIF(B15=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N15,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!#REF!","v":{"$error":"#REF!"}},"",{"$f":"\nIF(M15=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N15,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N15,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M15=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N15,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N15=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N15,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N15=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N15,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N15=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N15,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N15=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N15,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N15=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N15,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N15=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N15,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N15=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N15,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N15=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N15,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N15=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N15,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N15=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N15,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N15=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N15,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N15,'All Data'!$R:$R,0))","v":{"$error":"#REF!"}},null,"dia.18",null,null,null,null,"SUNCON"]
[null,"","","","","","","","","","","",{"$f":"\nIF(B16=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N16,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ35","v":0},"",{"$f":"\nIF(M16=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N16,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N16,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M16=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N16,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N16=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N16,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N16=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N16,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N16=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N16,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N16=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N16,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N16=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N16,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N16=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N16,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N16=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N16,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N16=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N16,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N16=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N16,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N16=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N16,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N16=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N16,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,"Range Preset",null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N16,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}},null,null,null,null,null,null,"Matsuo"]
[null,"","","","","","","","","","","",{"$f":"\nIF(B17=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N17,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ36","v":0},"",{"$f":"\nIF(M17=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N17,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N17,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M17=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N17,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N17=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N17,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N17=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N17,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N17=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N17,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N17=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N17,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N17=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N17,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N17=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N17,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N17=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N17,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N17=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N17,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N17=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N17,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N17=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N17,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N17=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N17,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N17,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}},null,null,null,null,null,null,"Samsung"]
[null,"","","","","","","","","","","",{"$f":"\nIF(B18=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N18,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ37","v":0},"",{"$f":"\nIF(M18=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N18,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N18,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M18=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N18,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N18=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N18,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N18=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N18,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N18=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N18,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N18=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N18,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N18=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N18,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N18=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N18,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N18=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N18,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N18=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N18,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N18=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N18,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N18=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N18,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N18=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N18,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N18,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}}]
[null,"","","","","","","","","","","",{"$f":"\nIF(B19=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N19,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ38","v":0},"",{"$f":"\nIF(M19=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N19,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N19,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M19=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N19,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N19=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N19,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N19=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N19,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N19=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N19,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N19=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N19,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N19=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N19,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N19=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N19,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N19=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N19,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N19=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N19,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N19=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N19,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N19=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N19,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N19=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N19,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N19,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}}]
[null,"","","","","","","","","","","",{"$f":"\nIF(B20=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N20,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ39","v":0},"",{"$f":"\nIF(M20=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N20,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N20,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M20=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N20,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N20=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N20,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N20=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N20,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N20=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N20,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N20=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N20,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N20=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N20,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N20=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N20,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N20=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N20,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N20=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N20,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N20=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N20,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N20=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N20,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N20=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N20,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N20,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}}]
[null,"","","","","","","","","","","",{"$f":"\nIF(B21=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N21,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ40","v":0},"",{"$f":"\nIF(M21=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N21,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N21,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M21=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N21,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N21=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N21,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N21=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N21,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N21=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N21,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N21=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N21,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N21=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N21,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N21=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N21,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N21=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N21,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N21=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N21,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N21=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N21,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N21=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N21,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N21=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N21,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N21,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}}]
[null,"","","","","","","","","","","",{"$f":"\nIF(B22=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N22,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ41","v":0},"",{"$f":"\nIF(M22=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N22,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N22,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M22=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N22,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N22=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N22,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N22=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N22,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N22=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N22,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N22=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N22,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N22=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N22,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N22=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N22,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N22=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N22,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N22=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N22,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N22=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N22,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N22=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N22,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N22=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N22,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N22,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}}]
[null,"","","","","","","","","","","",{"$f":"\nIF(B23=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N23,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ42","v":0},"",{"$f":"\nIF(M23=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N23,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N23,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M23=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N23,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N23=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N23,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N23=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N23,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N23=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N23,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N23=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N23,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N23=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N23,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N23=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N23,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N23=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N23,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N23=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N23,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N23=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N23,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N23=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N23,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N23=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N23,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N23,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}}]
[null,"","","","","","","","","","","",{"$f":"\nIF(B24=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N24,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ43","v":0},"",{"$f":"\nIF(M24=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N24,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N24,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M24=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N24,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N24=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N24,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N24=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N24,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N24=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N24,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N24=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N24,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N24=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N24,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N24=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N24,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N24=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N24,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N24=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N24,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N24=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N24,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N24=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N24,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N24=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N24,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N24,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}}]
[null,"","","","","","","","","","","",{"$f":"\nIF(B25=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N25,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ44","v":0},"",{"$f":"\nIF(M25=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N25,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N25,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M25=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N25,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N25=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N25,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N25=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N25,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N25=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N25,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N25=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N25,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N25=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N25,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N25=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N25,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N25=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N25,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N25=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N25,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N25=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N25,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N25=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N25,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N25=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N25,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N25,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}}]
[null,"","","","","","","","","","","",{"$f":"\nIF(B26=\"\",\"\",INDEX('All Data'!$F:$F,MATCH(N26,'All Data'!$R:$R,0)))","v":""},{"$f":"\n'All Data'!CJ45","v":0},"",{"$f":"\nIF(M26=\"\",\"\",CONCATENATE(INDEX('All Data'!$L:$L,MATCH(N26,'All Data'!$R:$R,0)),\" (\",INDEX('All Data'!$M:$M,MATCH(N26,'All Data'!$R:$R,0)),\")\"))","v":""},{"$f":"IF(M26=\"\",\"\",INDEX('All Data'!$G:$G,MATCH(N26,'All Data'!$R:$R,0)))","v":""},{"$f":"\nIFERROR(IF(N26=\"\",\"\",INDEX('All Data'!$N:$N,MATCH(N26,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N26=\"\",\"\",INDEX('All Data'!$I:$I,MATCH(N26,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N26=\"\",\"\",INDEX('All Data'!$AF:$AF,MATCH(N26,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N26=\"\",\"\",INDEX('All Data'!$S:$S,MATCH(N26,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N26=\"\",\"\",INDEX('All Data'!$V:$V,MATCH(N26,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N26=\"\",\"\",INDEX('All Data'!$W:$W,MATCH(N26,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N26=\"\",\"\",INDEX('All Data'!$X:$X,MATCH(N26,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N26=\"\",\"\",INDEX('All Data'!$Y:$Y,MATCH(N26,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N26=\"\",\"\",INDEX('All Data'!$AI:$AI,MATCH(N26,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N26=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N26,'All Data'!$R:$R,0))),\"\")","v":""},{"$f":"\nIFERROR(IF(N26=\"\",\"\",INDEX('All Data'!$AD:$AD,MATCH(N26,'All Data'!$R:$R,0))),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"INDEX('All Data'!$AG:$AG,MATCH(N26,'All Data'!$R:$R,0))","v":{"$error":"#N/A"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N39=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N39,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N40=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N40,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N41=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N41,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N42=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N42,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N43=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N43,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N44=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N44,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N45=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N45,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N46=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N46,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"=INDEX('All Data'!$M:$M,MATCH($O$7,'All Data'!$P:$P,1),MATCH($P$7,'All Data'!$Q:$Q,0),MATCH($Q$7,'All Data'!$R:$R,0))",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N47=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N47,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"=INDEX('All Data'!M:M,SUMPRODUCT(('All Data'!P:P='Auto PN'!$O$7)*('All Data'!Q:Q='Auto PN'!$P$7)*('All Data'!N:N='Auto PN'!$S$7)*('All Data'!O:O='Auto PN'!$Q$7)*ROW('All Data'!M:M)))",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N48=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N48,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N49=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N49,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N50=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N50,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N51=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N51,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N52=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N52,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N53=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N53,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N54=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N54,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N55=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N55,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N56=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N56,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N57=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N57,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N58=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N58,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N59=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N59,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N60=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N60,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N61=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N61,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N62=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N62,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N63=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N63,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N64=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N64,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N65=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N65,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N66=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N66,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N67=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N67,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N68=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N68,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N69=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N69,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N70=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N70,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N71=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N71,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N72=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N72,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N73=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N73,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N74=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N74,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N75=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N75,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N76=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N76,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N77=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N77,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N78=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N78,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N79=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N79,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N80=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N80,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N81=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N81,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N82=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N82,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N83=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N83,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N84=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N84,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N85=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N85,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N86=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N86,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N87=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N87,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N88=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N88,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N89=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N89,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N90=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N90,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N91=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N91,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N92=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N92,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N93=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N93,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N94=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N94,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N95=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N95,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N96=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N96,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N97=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N97,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N98=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N98,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N99=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N99,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N100=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N100,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N101=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N101,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N102=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N102,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N103=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N103,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N104=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N104,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N105=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N105,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N106=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N106,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N107=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N107,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N108=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N108,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N109=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N109,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N110=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N110,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N111=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N111,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N112=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N112,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N113=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N113,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N114=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N114,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N115=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N115,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N116=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N116,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N117=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N117,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N118=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N118,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N119=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N119,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N120=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N120,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N121=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N121,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N122=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N122,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N123=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N123,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N124=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N124,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N125=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N125,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N126=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N126,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N127=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N127,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N128=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N128,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N129=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N129,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N130=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N130,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N131=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N131,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N132=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N132,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N133=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N133,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N134=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N134,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N135=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N135,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N136=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N136,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N137=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N137,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N138=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N138,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N139=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N139,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N140=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N140,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N141=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N141,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N142=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N142,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N143=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N143,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N144=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N144,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N145=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N145,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N146=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N146,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N147=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N147,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N148=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N148,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N149=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N149,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N150=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N150,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N151=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N151,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N152=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N152,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N153=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N153,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N154=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N154,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N155=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N155,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N156=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N156,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N157=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N157,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N158=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N158,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N159=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N159,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N160=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N160,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N161=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N161,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N162=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N162,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N163=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N163,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N164=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N164,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N165=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N165,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N166=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N166,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N167=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N167,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N168=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N168,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N169=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N169,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N170=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N170,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N171=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N171,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N172=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N172,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N173=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N173,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N174=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N174,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N175=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N175,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N176=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N176,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N177=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N177,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N178=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N178,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N179=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N179,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N180=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N180,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N181=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N181,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N182=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N182,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N183=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N183,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N184=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N184,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N185=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N185,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N186=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N186,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N187=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N187,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N188=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N188,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N189=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N189,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N190=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N190,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N191=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N191,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N192=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N192,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N193=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N193,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N194=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N194,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N195=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N195,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N196=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N196,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N197=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N197,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N198=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N198,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N199=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N199,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N200=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N200,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N201=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N201,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N202=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N202,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N203=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N203,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N204=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N204,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N205=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N205,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N206=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N206,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N207=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N207,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N208=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N208,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N209=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N209,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N210=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N210,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N211=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N211,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N212=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N212,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N213=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N213,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N214=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N214,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N215=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N215,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N216=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N216,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N217=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N217,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N218=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N218,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N219=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N219,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N220=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N220,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N221=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N221,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N222=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N222,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N223=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N223,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N224=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N224,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N225=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N225,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N226=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N226,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N227=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N227,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N228=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N228,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N229=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N229,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N230=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N230,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N231=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N231,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N232=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N232,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N233=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N233,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N234=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N234,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N235=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N235,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N236=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N236,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N237=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N237,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N238=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N238,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N239=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N239,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N240=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N240,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N241=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N241,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N242=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N242,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N243=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N243,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N244=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N244,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N245=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N245,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N246=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N246,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N247=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N247,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N248=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N248,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N249=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N249,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N250=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N250,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N251=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N251,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N252=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N252,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N253=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N253,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N254=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N254,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N255=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N255,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N256=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N256,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N257=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N257,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N258=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N258,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N259=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N259,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N260=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N260,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N261=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N261,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N262=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N262,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N263=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N263,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N264=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N264,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N265=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N265,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N266=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N266,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N267=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N267,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N268=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N268,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N269=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N269,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N270=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N270,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N271=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N271,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N272=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N272,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N273=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N273,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N274=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N274,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N275=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N275,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N276=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N276,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N277=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N277,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N278=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N278,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N279=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N279,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N280=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N280,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N281=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N281,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N282=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N282,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N283=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N283,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N284=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N284,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N285=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N285,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N286=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N286,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N287=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N287,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N288=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N288,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N289=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N289,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N290=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N290,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N291=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N291,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N292=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N292,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N293=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N293,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N294=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N294,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N295=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N295,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N296=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N296,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N297=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N297,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N298=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N298,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N299=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N299,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N300=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N300,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N301=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N301,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N302=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N302,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N303=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N303,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N304=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N304,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N305=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N305,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N306=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N306,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N307=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N307,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N308=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N308,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N309=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N309,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N310=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N310,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N311=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N311,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N312=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N312,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N313=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N313,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N314=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N314,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N315=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N315,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N316=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N316,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N317=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N317,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N318=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N318,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N319=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N319,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N320=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N320,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N321=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N321,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N322=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N322,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N323=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N323,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N324=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N324,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N325=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N325,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N326=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N326,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N327=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N327,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N328=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N328,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N329=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N329,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N330=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N330,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N331=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N331,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N332=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N332,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N333=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N333,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N334=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N334,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N335=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N335,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N336=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N336,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N337=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N337,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N338=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N338,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N339=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N339,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N340=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N340,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N341=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N341,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N342=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N342,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N343=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N343,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N344=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N344,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N345=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N345,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N346=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N346,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N347=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N347,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N348=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N348,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N349=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N349,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N350=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N350,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N351=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N351,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N352=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N352,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N353=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N353,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N354=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N354,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N355=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N355,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N356=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N356,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N357=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N357,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N358=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N358,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N359=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N359,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N360=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N360,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N361=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N361,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N362=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N362,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N363=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N363,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N364=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N364,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N365=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N365,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N366=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N366,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N367=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N367,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N368=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N368,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N369=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N369,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N370=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N370,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N371=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N371,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N372=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N372,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N373=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N373,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N374=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N374,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N375=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N375,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N376=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N376,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N377=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N377,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N378=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N378,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N379=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N379,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N380=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N380,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N381=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N381,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N382=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N382,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N383=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N383,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N384=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N384,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N385=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N385,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N386=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N386,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N387=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N387,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N388=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N388,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N389=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N389,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N390=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N390,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N391=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N391,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N392=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N392,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N393=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N393,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N394=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N394,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N395=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N395,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N396=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N396,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N397=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N397,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N398=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N398,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N399=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N399,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N400=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N400,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N401=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N401,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N402=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N402,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N403=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N403,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N404=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N404,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N405=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N405,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N406=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N406,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N407=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N407,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N408=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N408,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N409=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N409,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N410=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N410,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N411=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N411,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N412=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N412,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N413=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N413,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N414=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N414,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N415=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N415,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N416=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N416,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N417=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N417,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N418=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N418,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N419=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N419,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N420=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N420,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N421=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N421,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N422=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N422,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N423=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N423,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N424=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N424,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N425=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N425,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N426=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N426,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N427=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N427,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N428=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N428,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N429=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N429,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N430=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N430,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N431=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N431,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N432=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N432,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N433=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N433,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N434=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N434,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N435=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N435,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N436=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N436,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N437=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N437,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N438=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N438,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N439=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N439,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N440=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N440,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N441=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N441,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N442=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N442,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N443=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N443,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N444=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N444,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N445=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N445,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N446=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N446,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N447=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N447,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N448=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N448,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N449=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N449,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N450=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N450,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N451=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N451,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N452=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N452,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N453=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N453,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N454=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N454,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N455=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N455,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N456=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N456,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N457=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N457,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N458=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N458,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N459=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N459,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N460=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N460,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N461=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N461,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N462=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N462,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N463=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N463,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N464=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N464,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N465=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N465,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N466=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N466,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N467=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N467,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N468=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N468,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N469=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N469,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N470=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N470,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N471=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N471,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N472=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N472,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N473=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N473,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N474=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N474,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N475=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N475,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N476=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N476,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N477=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N477,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N478=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N478,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N479=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N479,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N480=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N480,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N481=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N481,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N482=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N482,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N483=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N483,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N484=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N484,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N485=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N485,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N486=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N486,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N487=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N487,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N488=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N488,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N489=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N489,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N490=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N490,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N491=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N491,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N492=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N492,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N493=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N493,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N494=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N494,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N495=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N495,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N496=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N496,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N497=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N497,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N498=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N498,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N499=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N499,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,"要旨",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N500=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N500,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N501=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N501,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N502=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N502,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N503=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N503,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N504=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N504,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N505=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N505,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N506=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N506,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N507=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N507,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N508=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N508,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N509=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N509,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N510=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N510,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N511=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N511,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N512=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N512,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N513=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N513,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N514=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N514,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N515=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N515,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N516=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N516,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N517=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N517,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N518=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N518,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N519=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N519,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N520=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N520,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N521=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N521,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N522=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N522,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N523=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N523,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N524=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N524,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N525=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N525,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N526=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N526,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N527=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N527,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N528=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N528,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N529=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N529,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N530=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N530,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N531=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N531,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N532=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N532,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N533=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N533,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N534=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N534,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N535=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N535,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N536=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N536,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N537=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N537,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N538=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N538,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N539=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N539,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N540=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N540,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N541=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N541,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N542=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N542,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N543=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N543,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N544=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N544,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N545=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N545,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N546=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N546,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N547=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N547,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N548=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N548,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N549=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N549,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N550=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N550,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N551=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N551,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N552=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N552,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N553=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N553,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N554=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N554,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N555=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N555,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N556=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N556,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N557=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N557,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N558=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N558,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N559=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N559,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N560=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N560,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N561=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N561,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N562=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N562,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N563=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N563,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N564=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N564,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N565=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N565,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N566=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N566,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N567=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N567,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N568=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N568,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N569=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N569,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N570=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N570,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N571=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N571,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N572=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N572,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N573=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N573,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N574=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N574,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N575=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N575,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N576=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N576,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N577=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N577,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N578=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N578,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N579=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N579,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N580=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N580,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N581=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N581,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N582=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N582,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N583=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N583,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N584=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N584,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N585=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N585,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N586=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N586,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N587=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N587,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N588=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N588,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N589=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N589,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N590=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N590,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N591=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N591,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N592=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N592,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N593=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N593,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N594=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N594,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N595=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N595,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N596=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N596,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N597=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N597,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N598=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N598,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N599=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N599,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N600=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N600,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N601=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N601,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N602=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N602,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N603=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N603,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N604=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N604,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N605=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N605,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N606=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N606,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N607=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N607,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N608=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N608,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N609=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N609,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N610=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N610,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N611=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N611,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N612=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N612,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N613=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N613,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N614=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N614,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N615=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N615,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N616=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N616,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N617=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N617,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N618=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N618,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N619=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N619,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N620=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N620,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N621=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N621,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N622=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N622,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N623=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N623,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N624=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N624,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N625=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N625,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N626=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N626,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N627=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N627,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N628=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N628,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N629=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N629,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N630=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N630,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N631=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N631,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N632=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N632,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N633=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N633,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N634=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N634,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N635=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N635,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N636=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N636,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N637=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N637,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N638=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N638,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N639=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N639,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N640=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N640,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N641=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N641,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N642=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N642,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N643=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N643,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N644=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N644,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N645=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N645,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N646=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N646,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N647=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N647,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N648=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N648,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N649=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N649,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N650=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N650,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N651=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N651,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N652=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N652,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N653=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N653,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N654=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N654,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N655=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N655,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N656=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N656,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N657=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N657,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N658=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N658,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N659=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N659,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N660=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N660,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N661=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N661,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N662=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N662,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N663=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N663,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N664=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N664,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N665=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N665,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N666=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N666,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N667=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N667,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N668=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N668,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N669=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N669,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N670=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N670,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N671=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N671,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N672=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N672,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N673=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N673,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N674=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N674,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N675=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N675,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N676=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N676,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N677=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N677,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N678=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N678,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N679=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N679,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N680=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N680,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N681=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N681,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N682=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N682,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N683=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N683,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N684=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N684,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N685=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N685,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N686=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N686,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N687=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N687,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N688=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N688,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N689=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N689,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N690=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N690,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N691=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N691,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N692=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N692,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N693=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N693,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N694=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N694,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N695=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N695,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N696=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N696,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N697=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N697,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N698=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N698,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N699=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N699,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N700=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N700,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N701=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N701,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N702=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N702,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N703=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N703,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N704=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N704,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N705=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N705,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N706=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N706,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N707=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N707,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N708=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N708,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N709=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N709,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N710=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N710,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N711=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N711,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N712=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N712,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N713=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N713,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N714=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N714,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N715=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N715,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N716=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N716,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N717=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N717,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N718=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N718,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N719=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N719,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N720=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N720,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N721=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N721,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N722=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N722,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N723=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N723,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N724=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N724,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N725=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N725,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N726=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N726,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N727=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N727,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N728=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N728,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N729=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N729,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N730=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N730,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N731=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N731,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N732=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N732,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N733=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N733,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N734=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N734,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N735=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N735,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N736=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N736,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N737=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N737,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N738=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N738,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N739=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N739,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N740=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N740,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N741=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N741,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N742=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N742,'All Data'!$R:$R,0)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N743=\"\",\"\",INDEX('All Data'!$AP:$AP,MATCH(N743,'All Data'!$R:$R,0)))","v":""}]